{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["电线电缆检测中心"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"电线电缆检测中心","index":0,"n_rows":3016,"n_cols":9,"rows_kept":3016,"merged":[[0,0,0,7]]}
["武汉检验检测认证发展集团有限公司-电线电缆检测中心收费标准"]
["检验部门","一级项目序号","一级项目名称","二级项目名称","检验方法","收费标准","项目备注","类别名称"]
["电线电缆检测中心",5,"1%伸长时的应力",null,null,390,null,"全部参数"]
["电线电缆检测中心",3,"20℃时的电阻率",null,null,280,null,3]
["电线电缆检测中心",7,"20℃时的电阻率",null,null,280,null,"全部参数"]
["电线电缆检测中心",5,"20℃时的电阻率 ",null,null,280,null,"铜牌陕西军工"]
["电线电缆检测中心",3,"20℃时体积电阻率ρ20",null,null,300,null,"全部参数"]
["电线电缆检测中心",12,"4h交流电压试验（18kV,4h）",null,null,1500,null,"1×25"]
["电线电缆检测中心",12,"70℃绝缘电阻",null,null,600,null,"1×10"]
["电线电缆检测中心",11,"75℃绝缘电阻（80Ｖ～500Ｖ, 1min）",null,null,600,null,"1×25"]
["电线电缆检测中心",9,"90℃绝缘电阻",null,null,600,null,"1×10"]
["电线电缆检测中心",10,"90℃绝缘电阻（80Ｖ～500Ｖ, 1min）",null,null,600,null,"1×25"]
["电线电缆检测中心",5,"f值",null,null,110,null,"50黑"]
["电线电缆检测中心",9,"f值与规定平均外径上限的比值",null,null,110,null,"KVV"]
["电线电缆检测中心",22,"pH值和电导率试验","pH值和电导率",null,1000,null,"3×300+1×150"]
["电线电缆检测中心",24,"pH值和电导率试验","pH值和电导率",null,1000,null,"GB/T 33594-2017"]
["电线电缆检测中心",37,"pH值和电导率试验-护套","pH值",null,500,"护套为（U,YJ）时做","充电桩电缆"]
["电线电缆检测中心",37,"pH值和电导率试验-护套","电导率",null,500,"护套为（U,YJ）时做","充电桩电缆"]
["电线电缆检测中心",34,"pH值和电导率试验-绝缘","pH值",null,500,"绝缘为（EY）时做","充电桩电缆"]
["电线电缆检测中心",34,"pH值和电导率试验-绝缘","电导率",null,500,"绝缘为（EY）时做","充电桩电缆"]
["电线电缆检测中心",13,"半导电屏蔽电阻率(90℃)","老化前",null,250,null,"3×400"]
["电线电缆检测中心",13,"半导电屏蔽电阻率(90℃)","附加段老化后(100℃,7d)",null,250,null,"3×400"]
["电线电缆检测中心",14,"半导电屏蔽电阻率(90℃)","附加段老化后(100℃,7d)",null,250,null,"YJLHVS2"]
["电线电缆检测中心",17,"半导电屏蔽电阻率(90℃)","老化前",null,250,null,"YJLHV22"]
["电线电缆检测中心",17,"半导电屏蔽电阻率(90℃)","附加段老化后(100℃,7d)",null,250,null,"YJLHV22"]
["电线电缆检测中心",18,"半导电屏蔽电阻率(90℃)","老化前",null,250,null,"YJLHVS2"]
["电线电缆检测中心",18,"半导电屏蔽电阻率(90℃)","老化前",null,250,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",18,"半导电屏蔽电阻率(90℃)","附加段老化后(100℃,7d)",null,250,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",11,"包带间隙与金属带宽度之比",null,null,55,null,"3×400"]
["电线电缆检测中心",11,"包带间隙与金属带宽度之比",null,null,55,null,"YJV22-8.7/10"]
["电线电缆检测中心",11,"包带间隙与金属带宽度之比",null,null,55,null,"YJV22-26/35"]
["电线电缆检测中心",11,"包带间隙与金属带宽度之比",null,null,55,null,"YJLHV22"]
["电线电缆检测中心",12,"包带间隙与金属带宽度之比",null,null,55,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",7,"编织密度",null,null,110,null,"2×2×0.12"]
["电线电缆检测中心",7,"编织密度",null,null,110,null,"2×0.08"]
["电线电缆检测中心",7,"编织密度",null,null,110,null,"RVVP 300/300V"]
["电线电缆检测中心",7,"编织密度",null,null,110,null,"RVVP"]
["电线电缆检测中心",6,"标志","成品电缆表面标志",null,10,null,"1×2.5"]
["电线电缆检测中心",6,"标志","标志间距离",null,10,null,"1×2.5"]
["电线电缆检测中心",7,"标志","成品电缆表面标志",null,10,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",7,"标志","标志间距离",null,10,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",7,"标志","成品电缆表面标志",null,10,null,"1×16"]
["电线电缆检测中心",7,"标志","标志间距离",null,10,null,"1×16"]
["电线电缆检测中心",7,"标志","成品电缆表面标志",null,10,null,"1×0.5"]
["电线电缆检测中心",7,"标志","标志间距离",null,10,null,"1×0.5"]
["电线电缆检测中心",7,"标志","成品电缆表面标志",null,10,null,"1×25"]
["电线电缆检测中心",7,"标志","标志间距离",null,10,null,"1×25"]
["电线电缆检测中心",8,"标志","成品电缆表面标志",null,10,null,"6×1"]
["电线电缆检测中心",8,"标志","标志间距离",null,10,null,"6×1"]
["电线电缆检测中心",8,"标志","成品电缆表面标志",null,10,null,"1×0.75"]
["电线电缆检测中心",8,"标志","标志间距离",null,10,null,"1×0.75"]
["电线电缆检测中心",8,"标志","成品电缆表面标志",null,10,null,"2×1.0"]
["电线电缆检测中心",8,"标志","标志间距离",null,10,null,"2×1.0"]
["电线电缆检测中心",8,"标志","成品电缆表面标志",null,10,null,"1×0.08"]
["电线电缆检测中心",8,"标志","标志间距离",null,10,null,"1×0.08"]
["电线电缆检测中心",8,"标志","成品电缆表面标志",null,10,null,"2×0.12"]
["电线电缆检测中心",8,"标志","标志间距离",null,10,null,"2×0.12"]
["电线电缆检测中心",8,"标志","成品电缆表面标志",null,10,null,"1×1"]
["电线电缆检测中心",8,"标志","标志间距离",null,10,null,"1×1"]
["电线电缆检测中心",8,"标志","成品电缆表面标志",null,10,null,"2×0.3"]
["电线电缆检测中心",8,"标志","标志间距离",null,10,null,"2×0.3"]
["电线电缆检测中心",8,"标志","成品电缆表面标志",null,10,null,"2×4"]
["电线电缆检测中心",8,"标志","标志间距离",null,10,null,"2×4"]
["电线电缆检测中心",9,"标志","成品电缆表面标志",null,10,null,"1×95"]
["电线电缆检测中心",9,"标志","标志间距离",null,10,null,"1×95"]
["电线电缆检测中心",9,"标志","成品电缆表面标志",null,10,null,"2×0.5"]
["电线电缆检测中心",9,"标志","标志间距离",null,10,null,"2×0.5"]
["电线电缆检测中心",9,"标志","成品电缆表面标志",null,10,null,"3×300+1×150"]
["电线电缆检测中心",9,"标志","标志间距离",null,10,null,"3×300+1×150"]
["电线电缆检测中心",9,"标志","成品电缆表面标志",null,10,null,"3×16"]
["电线电缆检测中心",9,"标志","标志间距离",null,10,null,"3×16"]
["电线电缆检测中心",10,"标志","成品电缆表面标志",null,10,null,"2×1.5"]
["电线电缆检测中心",10,"标志","标志间距离",null,10,null,"2×1.5"]
["电线电缆检测中心",10,"标志","成品电缆表面标志",null,10,null,"2×0.08"]
["电线电缆检测中心",10,"标志","标志间距离",null,10,null,"2×0.08"]
["电线电缆检测中心",10,"标志","成品电缆表面标志",null,10,null,"2×35"]
["电线电缆检测中心",10,"标志","标志间距离",null,10,null,"2×35"]
["电线电缆检测中心",10,"标志","成品电缆表面标志",null,10,null,"3×0.3"]
["电线电缆检测中心",10,"标志","标志间距离",null,10,null,"3×0.3"]
["电线电缆检测中心",10,"标志","成品电缆表面标志",null,10,null,"YJY22"]
["电线电缆检测中心",10,"标志","标志间距离",null,10,null,"YJY22"]
["电线电缆检测中心",10,"标志","成品电缆表面标志",null,10,null,"VLHV22"]
["电线电缆检测中心",10,"标志","标志间距离",null,10,null,"VLHV22"]
["电线电缆检测中心",10,"标志","成品电缆表面标志",null,10,null,"YJLHV22"]
["电线电缆检测中心",10,"标志","标志间距离",null,10,null,"YJLHV22"]
["电线电缆检测中心",10,"标志","成品电缆表面标志",null,10,null,"YJLHVS2"]
["电线电缆检测中心",10,"标志","标志间距离",null,10,null,"YJLHVS2"]
["电线电缆检测中心",11,"标志","成品电缆表面标志",null,10,null,"2×0.75"]
["电线电缆检测中心",11,"标志","标志间距离",null,10,null,"2×0.75"]
["电线电缆检测中心",11,"标志","成品电缆表面标志",null,10,null,"1×1.5"]
["电线电缆检测中心",11,"标志","标志间距离",null,10,null,"1×1.5"]
["电线电缆检测中心",11,"标志","成品电缆表面标志",null,10,null,"3×400"]
["电线电缆检测中心",11,"标志","标志间距离 ",null,10,null,"3×400"]
["电线电缆检测中心",11,"标志","成品电缆表面标志",null,10,null,"GB/T 33594-2017"]
["电线电缆检测中心",11,"标志","标志间距离",null,10,null,"GB/T 33594-2017"]
["电线电缆检测中心",12,"标志","成品电缆表面标志",null,10,null,"2×2×0.12",{"$f":"IF(COUNTIF(#REF!,#REF!)>1,\"重复\",\"\")","v":{"$error":"#REF!"}}]
["电线电缆检测中心",12,"标志","标志间距离",null,10,null,"2×2×0.12"]
["电线电缆检测中心",12,"标志","成品电缆表面标志",null,10,null,"充电桩电缆"]
["电线电缆检测中心",12,"标志","标志间距离",null,10,null,"充电桩电缆"]
["电线电缆检测中心",13,"标志","成品电缆表面标志",null,10,null,"4×0.75"]
["电线电缆检测中心",13,"标志","标志间距离",null,10,null,"4×0.75"]
["电线电缆检测中心",14,"标志","成品电缆表面标志",null,10,null,"VLHVS2"]
["电线电缆检测中心",14,"标志","标志间距离",null,10,null,"VLHVS2"]
["电线电缆检测中心",15,"标志","成品电缆表面标志",null,10,null,"4×4"]
["电线电缆检测中心",15,"标志","标志间距离",null,10,null,"4×4"]
["电线电缆检测中心",15,"标志","成品电缆表面标志",null,10,null,"4×2.5"]
["电线电缆检测中心",15,"标志","标志间距离",null,10,null,"4×2.5"]
["电线电缆检测中心",16,"标志","成品电缆表面标志",null,10,null,"4×1.5"]
["电线电缆检测中心",16,"标志","标志间距离",null,10,null,"4×1.5"]
["电线电缆检测中心",16,"标志","成品电缆表面标志",null,10,null,"48×1"]
["电线电缆检测中心",16,"标志","标志间距离",null,10,null,"48×1"]
["电线电缆检测中心",16,"标志","成品电缆表面标志",null,10,null,"1×10"]
["电线电缆检测中心",16,"标志","标志间距离",null,10,null,"1×10"]
["电线电缆检测中心",16,"标志","成品电缆表面标志",null,10,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",16,"标志","标志间距离 ",null,10,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",16,"标志","成品电缆表面标志",null,10,null,"QC/T1037-2016"]
["电线电缆检测中心",16,"标志","标志间距离",null,10,null,"QC/T1037-2016"]
["电线电缆检测中心",19,"标志","成品电缆表面标志",null,10,null,"TICW计算机"]
["电线电缆检测中心",19,"标志","标志间距离",null,10,null,"TICW计算机"]
["电线电缆检测中心",7,"表面情况",null,null,270,null,"630/35-45/7"]
["电线电缆检测中心",7,"表面情况",null,null,270,null,"400/35-48/7"]
["电线电缆检测中心",7,"表面情况",null,null,270,null,"300/20-45/7"]
["电线电缆检测中心",7,"表面情况",null,null,270,null,"185/25-24/7"]
["电线电缆检测中心",5,"表面质量",null,null,270,null,"全部参数"]
["电线电缆检测中心",7,"表面质量",null,null,270,null,"铜牌陕西军工"]
["电线电缆检测中心",1,"材料烟密度",null,"GB/T 8323-2008",5000,null,"GB/T 8323-2008"]
["电线电缆检测中心",7,"缠绕屏蔽","缠绕层数",null,110,null,"2×0.08"]
["电线电缆检测中心",9,"成缆节距比电缆平均外径上限",null,null,110,null,"3×0.3"]
["电线电缆检测中心",11,"成缆节距比电缆平均外径上限",null,null,110,null,"2×2×0.12"]
["电线电缆检测中心",9,"成缆节距比每根编织绝缘线芯平均外径上线",null,null,110,null,"2×0.3"]
["电线电缆检测中心",6,"成品电缆标志",null,null,20,null,"50黑"]
["电线电缆检测中心",18,"成品电缆标志",null,null,20,null,"DIN 72551-5/1991"]
["电线电缆检测中心",10,"成品电缆机械强度","静态曲挠试验",null,350,null,"1×16"]
["电线电缆检测中心",11,"成品电缆机械强度","具有承力元件的中心垫芯抗张强度 ",null,350,null,"6×1"]
["电线电缆检测中心",11,"成品电缆机械强度","静态曲挠试验",null,350,null,"6×1"]
["电线电缆检测中心",11,"成品电缆机械强度","耐磨损试验",null,500,null,"6×1"]
["电线电缆检测中心",12,"成品电缆机械强度","弯曲试验（6000次双向弯曲，1500V电压）",null,470,null,"2×1.5"]
["电线电缆检测中心",12,"成品电缆机械强度","荷重断芯试验（0.5kg，0.1A）",null,300,null,"2×1.5"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"1×1"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"1×1"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×0.3"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×0.3"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×0.75"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×0.75"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×4"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×4"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"YC"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"YC"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"YZ"]
["电线电缆检测中心",12,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"YZ"]
["电线电缆检测中心",13,"成品电缆机械强度","静态曲挠试验",null,350,null,"1×95"]
["电线电缆检测中心",13,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×0.3"]
["电线电缆检测中心",13,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×0.3"]
["电线电缆检测中心",13,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×0.75"]
["电线电缆检测中心",13,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×0.75"]
["电线电缆检测中心",13,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×4"]
["电线电缆检测中心",13,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×4"]
["电线电缆检测中心",14,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×1.5"]
["电线电缆检测中心",14,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×1.5"]
["电线电缆检测中心",14,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"3×0.3"]
["电线电缆检测中心",14,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"3×0.3"]
["电线电缆检测中心",14,"成品电缆机械强度","耐磨损试验",null,500,null,"3×0.3"]
["电线电缆检测中心",15,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×0.75"]
["电线电缆检测中心",15,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×0.75"]
["电线电缆检测中心",16,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×0.75"]
["电线电缆检测中心",16,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×0.75"]
["电线电缆检测中心",16,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"1×1.5"]
["电线电缆检测中心",16,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"1×1.5"]
["电线电缆检测中心",16,"成品电缆机械强度","曲挠试验 ",null,400,null,"2×1.5"]
["电线电缆检测中心",16,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,350,null,"2×35"]
["电线电缆检测中心",16,"成品电缆机械强度","曲挠试验及试验后的浸水电压试验 ",null,400,null,"2×35"]
["电线电缆检测中心",16,"成品电缆机械强度","曲挠试验 ",null,400,null,"RVV"]
["电线电缆检测中心",17,"成品电缆机械强度","曲挠试验 ",null,400,null,"2×0.5"]
["电线电缆检测中心",17,"成品电缆机械强度","曲挠试验 ",null,400,null,"2×0.75"]
["电线电缆检测中心",13,"成品电缆机械强度试验","曲挠试验",null,350,null,"2×0.5"]
["电线电缆检测中心",13,"成品电缆机械强度试验","曲挠试验",null,400,null,"2×0.5"]
["电线电缆检测中心",13,"成品电缆机械强度试验","绝缘线芯撕离试验",null,490,null,"2×0.5"]
["电线电缆检测中心",13,"成品电缆机械强度试验","绝缘线芯撕离试验",null,490,null,"2×0.5"]
["电线电缆检测中心",28,"成品电缆机械强度试验","曲挠试验 ",null,400,null,"GB/T 33594-2017"]
["电线电缆检测中心",28,"成品电缆机械强度试验","曲挠试验 ",null,350,null,"GB/T 33594-2017"]
["电线电缆检测中心",40,"成品电缆机械强度试验","曲挠试验 ",null,350,null,"充电桩电缆"]
["电线电缆检测中心",40,"成品电缆机械强度试验","曲挠试验 ",null,400,null,"充电桩电缆"]
["电线电缆检测中心",3,"成品外径 ",null,null,80,null,"1.25 黑白"]
["电线电缆检测中心",21,"成束燃烧试验-A类","试样上炭化的长度距喷嘴底边向上的距离",null,4000,null,"3×300+1×150"]
["电线电缆检测中心",21,"成束燃烧试验-A类","试样上炭化的长度距喷嘴底边向上的距离",null,4000,null,"TICW计算机"]
["电线电缆检测中心",29,"成束燃烧试验-A类","试样上炭化的长度距喷嘴底边向上的距离",null,4000,null,"3×400"]
["电线电缆检测中心",29,"成束燃烧试验-A类","试样上炭化的长度距喷嘴底边向上的距离",null,4000,null,"3×400"]
["电线电缆检测中心",29,"成束燃烧试验-A类","试样上炭化的长度距喷嘴底边向上的距离",null,4000,null,"YJLHV22"]
["电线电缆检测中心",30,"成束燃烧试验-A类","试样上炭化的长度距喷嘴底边向上的距离",null,4000,null,"YJLHVS2"]
["电线电缆检测中心",30,"成束燃烧试验-A类","试样上炭化的长度距喷嘴底边向上的距离",null,4000,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",1,"尺寸","直径偏差",null,75,null,3]
["电线电缆检测中心",1,"尺寸","f值",null,110,null,3]
["电线电缆检测中心",1,"尺寸","直径",null,75,null,"全部参数"]
["电线电缆检测中心",1,"尺寸","不圆度",null,110,null,"全部参数"]
["电线电缆检测中心",1,"尺寸","直径偏差",null,75,null,6]
["电线电缆检测中心",1,"尺寸","不圆度",null,110,null,6]
["电线电缆检测中心",1,"尺寸","厚度a",null,110,null,"全部参数"]
["电线电缆检测中心",1,"尺寸","宽度b",null,110,null,"全部参数"]
["电线电缆检测中心",1,"尺寸","厚度a",null,110,null,"铜牌陕西军工"]
["电线电缆检测中心",1,"尺寸","宽度b",null,110,null,"铜牌陕西军工"]
["电线电缆检测中心",2,"尺寸","导体直径 ",null,75,null,"全部参数"]
["电线电缆检测中心",2,"尺寸","导体不圆度",null,30,null,"全部参数"]
["电线电缆检测中心",2,"尺寸","漆膜厚度 ",null,75,null,"全部参数"]
["电线电缆检测中心",2,"尺寸","漆包线外径",null,30,null,"全部参数"]
["电线电缆检测中心",2,"尺寸","f值",null,110,null,"全部参数"]
["电线电缆检测中心",1,"尺寸及其允许偏差","直径偏差",null,75,null,"全部参数"]
["电线电缆检测中心",14,"冲击电压试验及交流电压试验","弯曲试验后冲击电压试验(95kV,正负极各10次)",null,1500,null,"1×25"]
["电线电缆检测中心",14,"冲击电压试验及交流电压试验","冲击试验后交流电压试验(18kV,15min)",null,1500,null,"1×25"]
["电线电缆检测中心",2,"单根阻燃性能","上支架下缘与炭化部分起点间距离",18380.12,300,null,"单根（含滴落物）-12706-2020和9330-2020"]
["电线电缆检测中心",18,"单根阻燃性能","上支架下缘与炭化部分起点间距离",18380.12,300,null,"各种单项试验"]
["电线电缆检测中心",18,"单根阻燃性能","燃烧向下延伸至上支架下缘距离",18380.12,300,null,"各种单项试验"]
["电线电缆检测中心",10,"单位长度质量",null,null,270,null,"630/35-45/7"]
["电线电缆检测中心",10,"单位长度质量",null,null,270,null,"400/35-48/7"]
["电线电缆检测中心",10,"单位长度质量","导线单位长度质量（无油脂）",null,270,null,"300/20-45/7"]
["电线电缆检测中心",10,"单位长度质量",null,null,270,null,"185/25-24/7"]
["电线电缆检测中心",5,"导体单丝直径",null,null,110,null,"1.25 黑白"]
["电线电缆检测中心",5,"导体单丝直径",null,null,110,null,1]
["电线电缆检测中心",6,"导体单丝直径",null,null,110,null,"0.75 白"]
["电线电缆检测中心",6,"导体单丝直径",null,null,110,null,1]
["电线电缆检测中心",6,"导体单丝直径",null,null,110,null,"DIN 72551-5/1991"]
["电线电缆检测中心",1,"导体单线根数",null,null,110,null,"1×10"]
["电线电缆检测中心",1,"导体单线根数",null,null,110,null,"JKLYJ-1"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"60227 IEC 01（BV） 450/750V"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"2×0.75"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"1×0.75"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"1×2.5"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"BVR 450/750V"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"BVVB 300/500V"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"KVV"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"KVV22"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"KVVP"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"KVVP2-22"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"KYJV"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"KYJVP"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"KYJVP2-22"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"1×10"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"1×25"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"JKLYJ-10"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"3×16"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJY22"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"VV"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"VV22"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"WDZAN-YJY23"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJV"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJV22"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJV32"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"3×400"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"JKLV"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"JKLYJ-1"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJV22-8.7/10"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJV-8.7/10"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJV22-26/35"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJV-26/35"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"全项WDZAN-BYJ-105 450/750 1×2.5"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"常规WDZA-BYJ 450/750V  1×2.5"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"VLHV22"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"VLHVS2"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJLHVS2常规"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"YJLHS2常规"]
["电线电缆检测中心",2,"导体单线根数",null,null,110,null,"充电桩电缆"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"1×1.5"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"1×0.5"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"2×1.5"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"4×4"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"4×1.5"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"4×0.75"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"2×0.75"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"4×2.5"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"48×1"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"KYJV22"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"VLHV22常规"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"VLHVS2常规"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"TICW计算机"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"GB/T 33594-2017"]
["电线电缆检测中心",3,"导体单线根数",null,null,110,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",4,"导体单线根数",null,null,110,null,"4×1.5"]
["电线电缆检测中心",4,"导体单线根数",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"2×1.0"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"RVS 300/300V"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"RVV 300/500V"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"2×0.08"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"2×2×0.12"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"RVVP 300/300V"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"2×35"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"1×1"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"2×0.3"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"2×0.75"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"2×4"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"YC 450/750V"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"YCW"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"3×0.3"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"KVVR"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"KVVRP"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"YC"]
["电线电缆检测中心",2,"导体单线直径",null,null,110,null,"YZ"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"2×0.75"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"2×1.5"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"1×1.5"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"6×1"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"1×16"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"1×95"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"1×0.5"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"2×0.5"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"1×0.08"]
["电线电缆检测中心",3,"导体单线直径",null,null,110,null,"2×0.12"]
["电线电缆检测中心",4,"导体单线直径",null,null,110,null,"2×0.08"]
["电线电缆检测中心",2,"导体导通试验",null,null,220,null,"2×0.08"]
["电线电缆检测中心",4,"导体导通试验",null,null,220,null,"1×0.08"]
["电线电缆检测中心",4,"导体导通试验",null,null,220,null,"2×0.12"]
["电线电缆检测中心",3,"导体根数",null,null,110,null,"1×0.08"]
["电线电缆检测中心",4,"导体根数",null,null,110,null,"1.25 黑白"]
["电线电缆检测中心",4,"导体根数",null,null,110,null,1]
["电线电缆检测中心",5,"导体根数",null,null,110,null,"0.75 白"]
["电线电缆检测中心",5,"导体根数",null,null,110,null,1]
["电线电缆检测中心",5,"导体根数",null,null,110,null,"DIN 72551-5/1991"]
["电线电缆检测中心",4,"导体根数(根)",null,null,110,null,"50黑"]
["电线电缆检测中心",8,"导体绞合节距",null,null,110,null,"DIN 72551-5/1991"]
["电线电缆检测中心",8,"导体拉断力",null,null,4800,"拉3根","1×25"]
["电线电缆检测中心",9,"导体拉断力",null,null,4800,"拉3根","1×25"]
["电线电缆检测中心",11,"导体拉断力",null,null,4800,"拉3根","1×25"]
["电线电缆检测中心",6,"导体屏蔽层厚度",null,null,110,null,"1×25"]
["电线电缆检测中心",9,"导体屏蔽层厚度",null,null,110,null,"1×25"]
["电线电缆检测中心",4,"导体外形尺寸",null,null,80,null,"0.75 白"]
["电线电缆检测中心",6,"导体直流电阻(20℃)",null,null,220,null,"JKLYJ-1"]
["电线电缆检测中心",6,"导体直流电阻(20℃)",null,null,220,null,"JKLYJ-10"]
["电线电缆检测中心",7,"导体直流电阻(20℃)",null,null,220,null,"1×10"]
["电线电缆检测中心",9,"导体直流电阻(20℃)",null,null,220,null,"1×25"]
["电线电缆检测中心",9,"导体直流电阻(20℃)",null,null,220,null,"JKLYJ-10"]
["电线电缆检测中心",10,"导体直流电阻(20℃)",null,null,220,null,"1×10"]
["电线电缆检测中心",10,"导体直流电阻(20℃)",null,null,220,null,"1×25"]
["电线电缆检测中心",10,"导体直流电阻(20℃)",null,null,220,null,"JKLV"]
["电线电缆检测中心",10,"导体直流电阻(20℃)",null,null,220,null,"JKLYJ-1"]
["电线电缆检测中心",12,"导体直流电阻(20℃)",null,null,220,null,"1×25"]
["电线电缆检测中心",9,"导体中心间距",null,null,110,null,"2×1.5"]
["电线电缆检测中心",9,"导体中心间距",null,null,110,null,"2×1.5"]
["电线电缆检测中心",2,"导体种类",null,null,110,null,"2×0.75"]
["电线电缆检测中心",2,"导体种类",null,null,110,null,"2×1.5"]
["电线电缆检测中心",2,"导体种类",null,null,110,null,"1×1.5"]
["电线电缆检测中心",2,"导体种类",null,null,110,null,"4×0.75"]
["电线电缆检测中心",5,"导线外径",null,null,110,null,"630/35-45/7"]
["电线电缆检测中心",5,"导线外径",null,null,110,null,"400/35-48/7"]
["电线电缆检测中心",5,"导线外径",null,null,110,null,"300/20-45/7"]
["电线电缆检测中心",5,"导线外径",null,null,110,null,"185/25-24/7"]
["电线电缆检测中心",14,"导线整体拉断力",null,null,1600,"拉1根","630/35-45/7"]
["电线电缆检测中心",14,"导线整体拉断力",null,null,1600,"拉1根","400/35-48/7"]
["电线电缆检测中心",14,"导线整体拉断力",null,null,1600,"拉1根","300/20-45/7"]
["电线电缆检测中心",14,"导线整体拉断力(L=10m)",null,null,1600,"拉1根","185/25-24/7"]
["电线电缆检测中心",15,"低温冲击试验",null,null,800,"包含电压","QC/T1037-2016"]
["电线电缆检测中心",16,"低温冲击试验(-15℃)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",16,"低温冲击试验(-15℃)",null,null,400,null,"3×16"]
["电线电缆检测中心",17,"低温冲击试验(-15℃)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",17,"低温冲击试验(-15℃)",null,null,400,null,"VLHV22"]
["电线电缆检测中心",18,"低温冲击试验(-15℃)",null,null,400,null,"VLHVS2"]
["电线电缆检测中心",19,"低温冲击试验(-15℃)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",20,"低温冲击试验(-15℃)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",21,"低温冲击试验(-15℃)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",21,"低温冲击试验(-15℃)",null,null,400,null,"YJY22"]
["电线电缆检测中心",21,"低温冲击试验(-15℃)",null,null,400,null,"YJLHV22"]
["电线电缆检测中心",21,"低温冲击试验(-15℃)",null,null,400,null,"YJLHVS2"]
["电线电缆检测中心",23,"低温冲击试验(-15℃)",null,null,400,null,"3×400"]
["电线电缆检测中心",24,"低温冲击试验(-15℃)",null,null,400,null,"YJLHVS2"]
["电线电缆检测中心",27,"低温冲击试验(-15℃)",null,null,400,null,"3×400"]
["电线电缆检测中心",27,"低温冲击试验(-15℃)",null,null,400,null,"YJLHV22"]
["电线电缆检测中心",28,"低温冲击试验(-15℃)",null,null,400,null,"YJLHVS2"]
["电线电缆检测中心",28,"低温冲击试验(-15℃)",null,null,400,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",29,"低温冲击试验(-15℃)",null,null,400,null,"3×400"]
["电线电缆检测中心",22,"低温冲击试验（-25℃/-40℃）",null,null,400,null,"GB/T 33594-2017"]
["电线电缆检测中心",13,"低温弹性","绝缘低温弯曲试验（-15℃）",null,400,null,"1×0.5"]
["电线电缆检测中心",10,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"1×2.5"]
["电线电缆检测中心",10,"低温弹性和冲击强度","绝缘低温拉伸试验（-15℃）",null,400,null,"1×2.5"]
["电线电缆检测中心",10,"低温弹性和冲击强度","成品电缆低温冲击试验（-15℃）",null,400,null,"1×2.5"]
["电线电缆检测中心",10,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"1×0.75"]
["电线电缆检测中心",11,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"1×1.5"]
["电线电缆检测中心",11,"低温弹性和冲击强度","绝缘低温拉伸试验(-15℃)",null,400,null,"1×1.5"]
["电线电缆检测中心",11,"低温弹性和冲击强度","绝缘低温冲击试验（-15℃）",null,400,null,"1×1.5"]
["电线电缆检测中心",11,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",11,"低温弹性和冲击强度","成品电缆低温冲击（-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",12,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×1.0"]
["电线电缆检测中心",12,"低温弹性和冲击强度","成品电缆低温冲击（-15℃）",null,400,null,"2×1.0"]
["电线电缆检测中心",13,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",13,"低温弹性和冲击强度","护套低温弯曲试验(-15℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",13,"低温弹性和冲击强度","成品电缆低温冲击试验（-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",13,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"1×0.75"]
["电线电缆检测中心",13,"低温弹性和冲击强度","绝缘低温拉伸试验（-15℃）",null,400,null,"1×0.75"]
["电线电缆检测中心",13,"低温弹性和冲击强度","护套低温弯曲试验(-15℃)",null,400,null,"1×0.75"]
["电线电缆检测中心",13,"低温弹性和冲击强度","护套低温拉伸试验（-15℃）",null,400,null,"1×0.75"]
["电线电缆检测中心",13,"低温弹性和冲击强度","成品电缆低温冲击试验（-15℃）",null,400,null,"1×0.75"]
["电线电缆检测中心",13,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"1×0.08"]
["电线电缆检测中心",13,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×0.12"]
["电线电缆检测中心",14,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",14,"低温弹性和冲击强度","护套低温弯曲试验(-15℃)",null,400,null,"2×0.5"]
["电线电缆检测中心",14,"低温弹性和冲击强度","成品电缆低温冲击试验（-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",14,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"低温弹性和冲击强度","护套低温弯曲试验(-15℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"低温弹性和冲击强度","护套低温拉伸(-15℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"低温弹性和冲击强度","成品电缆低温冲击试验（-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×1.5"]
["电线电缆检测中心",14,"低温弹性和冲击强度","护套低温弯曲试验(-15℃)",null,400,null,"2×1.5"]
["电线电缆检测中心",14,"低温弹性和冲击强度","护套低温拉伸试验(-15℃)",null,400,null,"2×1.5"]
["电线电缆检测中心",14,"低温弹性和冲击强度","成品电缆低温冲击试验（-15℃）",null,400,null,"2×1.5"]
["电线电缆检测中心",14,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"1×0.08"]
["电线电缆检测中心",14,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×0.08"]
["电线电缆检测中心",15,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×1.5"]
["电线电缆检测中心",15,"低温弹性和冲击强度","护套低温弯曲试验(-15℃)",null,400,null,"2×1.5"]
["电线电缆检测中心",15,"低温弹性和冲击强度","护套低温拉伸试验（-15℃）",null,400,null,"2×1.5"]
["电线电缆检测中心",15,"低温弹性和冲击强度","成品电缆低温冲击试验（-15℃）",null,400,null,"2×1.5"]
["电线电缆检测中心",15,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"低温弹性和冲击强度","护套低温弯曲试验(-15℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"低温弹性和冲击强度","成品电缆低温冲击试验（-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×0.12"]
["电线电缆检测中心",16,"低温弹性和冲击强度","护套低温弯曲试验(-15℃)",null,400,null,"2×0.08"]
["电线电缆检测中心",16,"低温弹性和冲击强度","护套低温拉伸试验(-15℃)",null,400,null,"2×0.08"]
["电线电缆检测中心",16,"低温弹性和冲击强度","成品电缆低温冲击试验（-15℃）",null,400,null,"2×0.08"]
["电线电缆检测中心",16,"低温弹性和冲击强度","成品电线低温冲击试验（-15℃）",null,400,null,"2×0.08"]
["电线电缆检测中心",16,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×0.08"]
["电线电缆检测中心",17,"低温弹性和冲击强度","绝缘低温弯曲试验（-15℃）",null,400,null,"2×2×0.12"]
["电线电缆检测中心",17,"低温弹性和冲击强度","护套低温弯曲试验(-15℃)",null,400,null,"2×2×0.12"]
["电线电缆检测中心",17,"低温弹性和冲击强度","护套低温拉伸试验(-15℃)",null,400,null,"2×2×0.12"]
["电线电缆检测中心",17,"低温弹性和冲击强度","成品电线低温冲击试验（-15℃）",null,400,null,"2×2×0.12"]
["电线电缆检测中心",10,"低温弹性试验","绝缘低温弯曲试验（-15℃）",null,400,null,"2×1.5"]
["电线电缆检测中心",11,"低温弹性试验","绝缘低温弯曲试验（-15℃）",null,400,null,"1×1.5"]
["电线电缆检测中心",11,"低温弹性试验","绝缘低温拉伸试验 (-15℃)",null,400,null,"1×1.5"]
["电线电缆检测中心",11,"低温弹性试验","绝缘低温弯曲试验（-15℃）",null,400,null,"1×0.5"]
["电线电缆检测中心",15,"低温拉伸试验",null,null,400,null,"QC/T1037-2016"]
["电线电缆检测中心",14,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"3×300+1×150"]
["电线电缆检测中心",14,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"3×16"]
["电线电缆检测中心",15,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"3×300+1×150"]
["电线电缆检测中心",15,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"VLHV22"]
["电线电缆检测中心",17,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"VLHVS2"]
["电线电缆检测中心",19,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"3×300+1×150"]
["电线电缆检测中心",22,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"3×400"]
["电线电缆检测中心",23,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"YJLHVS2"]
["电线电缆检测中心",26,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"3×400"]
["电线电缆检测中心",26,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"YJLHV22"]
["电线电缆检测中心",27,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"YJLHVS2"]
["电线电缆检测中心",27,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",28,"低温拉伸试验(-15℃)","断裂伸长率",null,400,null,"3×400"]
["电线电缆检测中心",20,"低温拉伸试验（-25℃/-40℃）","断裂伸长率",null,400,null,"GB/T 33594-2017"]
["电线电缆检测中心",17,"低温拉伸试验-断裂伸长率 (-15℃)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",19,"低温拉伸试验-断裂伸长率 (-15℃)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",19,"低温拉伸试验-断裂伸长率 (-15℃)",null,null,400,null,"YJY22"]
["电线电缆检测中心",19,"低温拉伸试验-断裂伸长率 (-15℃)",null,null,400,null,"YJLHV22"]
["电线电缆检测中心",19,"低温拉伸试验-断裂伸长率 (-15℃)",null,null,400,null,"YJLHVS2"]
["电线电缆检测中心",12,"低温试验","护套弯曲试验 (-35℃)",null,400,null,"2×0.3"]
["电线电缆检测中心",12,"低温试验","护套弯曲试验 (-35℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",12,"低温试验","护套伸长率试验 (-35℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",12,"低温试验","护套弯曲试验 (-35℃)",null,400,null,"2×4"]
["电线电缆检测中心",12,"低温试验","护套伸长率试验 (-35℃)",null,400,null,"2×4"]
["电线电缆检测中心",15,"低温试验","护套弯曲试验 (-35℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"低温试验","护套弯曲试验 (-35℃)",null,400,null,"1×1.5"]
["电线电缆检测中心",15,"低温试验","护套伸长率试验(-35℃)",null,400,null,"1×1.5"]
["电线电缆检测中心",15,"低温试验","护套弯曲试验 (-35℃)",null,400,null,"2×35"]
["电线电缆检测中心",15,"低温试验","护套伸长率试验 (-35℃)",null,400,null,"2×35"]
["电线电缆检测中心",15,"低温弯曲试验",null,null,800,null,"QC/T1037-2016"]
["电线电缆检测中心",8,"低温性能试验","低温卷绕 （温度: -40 ℃  冷冻时间: 4 h        芯轴直径: 10 mm ）",null,400,null,"1.25 黑白"]
["电线电缆检测中心",8,"低温性能试验","低温冲击 （温度: -15 ℃ ，冷冻时间: 16 h ，    落锤质量: 100 g ） 冲击后",null,400,null,"1.25 黑白"]
["电线电缆检测中心",9,"低温性能试验","低温卷绕 （温度: -40 ℃  时间: 4 h  芯轴   直径: 6 mm  重物: 0.5 kg  卷绕   速度: 1 s-1  卷绕圈数: 3圈）",null,400,null,"0.75 白"]
["电线电缆检测中心",9,"低温性能试验","低温冲击 （温度: -15 ℃  时间: 16 h  落锤   质量: 100 g ）",null,400,null,"0.75 白"]
["电线电缆检测中心",9,"低温性能试验","低温卷绕 （温度: -40 ℃ 时间: 4 h  芯轴   直径: 10 mm  砝码: 2.5 kg  卷绕速度:1 s-1  卷绕匝数: 3）",null,400,null,1]
["电线电缆检测中心",9,"低温性能试验","低温冲击 （温度: -15 ℃ 时间: 16 h   落锤质量: 100 g ）",null,400,null,1]
["电线电缆检测中心",11,"低温性能试验","低温冲击 (温度: - 15℃  时间: 16 h  落锤   质量: 400 g ） 冲击后",null,800,null,"50黑"]
["电线电缆检测中心",11,"低温性能试验","低温卷绕 （温度: -40 ℃ 时间: 4 h  芯轴   直径: 10 mm  砝码: 2.5 kg  卷绕速度:1 s-1  卷绕匝数: 3）",null,800,null,"DIN 72551-5/1991"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"1×2.5"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"1×2.5"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"1×0.75"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"1×0.75"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"02RV"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"02RV"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"06RV"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"06RV"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"BLV"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"BLV"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"BV"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"BV"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"BVR"]
["电线电缆检测中心",12,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"BVR"]
["电线电缆检测中心",13,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"1×1.5"]
["电线电缆检测中心",13,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"1×1.5"]
["电线电缆检测中心",13,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"1×0.5"]
["电线电缆检测中心",13,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"1×0.5"]
["电线电缆检测中心",13,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×1.5"]
["电线电缆检测中心",13,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×1.5"]
["电线电缆检测中心",14,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.5"]
["电线电缆检测中心",14,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.5"]
["电线电缆检测中心",14,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×1.0"]
["电线电缆检测中心",14,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×1.0"]
["电线电缆检测中心",14,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"RVS"]
["电线电缆检测中心",14,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"RVS"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"1×0.5"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"1×0.5"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.75"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.75"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"1×0.75"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"1×0.75"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"1×0.08"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"1×0.08"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"BVVB,BLVVB"]
["电线电缆检测中心",15,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"BVVB,BLVVB"]
["电线电缆检测中心",16,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.12"]
["电线电缆检测中心",16,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.12"]
["电线电缆检测中心",16,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"1×0.08"]
["电线电缆检测中心",16,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"1×0.08"]
["电线电缆检测中心",16,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.08"]
["电线电缆检测中心",16,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.08"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×1.5"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×1.5"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.5"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.5"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.12"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.12"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"1×0.08"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"1×0.08"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.08"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.08"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"3×300+1×150"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"3×300+1×150"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"3×16"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"3×16"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"AVVR"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"AVVR"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"RVV"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"RVV"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"RVVP"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"RVVP"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"VV,VLV"]
["电线电缆检测中心",17,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"VV,VLV"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.5"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.5"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.75"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.75"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×0.08"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×0.08"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"3×300+1×150"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"3×300+1×150"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"VLHV22"]
["电线电缆检测中心",18,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"VLHV22"]
["电线电缆检测中心",19,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"2×2×0.12"]
["电线电缆检测中心",19,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"2×2×0.12"]
["电线电缆检测中心",19,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"VLHVS2"]
["电线电缆检测中心",19,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"VLHVS2"]
["电线电缆检测中心",20,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"3×300+1×150"]
["电线电缆检测中心",20,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"3×300+1×150"]
["电线电缆检测中心",20,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"YJV,YJLV"]
["电线电缆检测中心",20,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"YJV,YJLV"]
["电线电缆检测中心",22,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"3×300+1×150"]
["电线电缆检测中心",22,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"3×300+1×150"]
["电线电缆检测中心",22,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"YJY22"]
["电线电缆检测中心",22,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"YJY22"]
["电线电缆检测中心",22,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"YJLHV22"]
["电线电缆检测中心",22,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"YJLHV22"]
["电线电缆检测中心",22,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"YJLHVS2"]
["电线电缆检测中心",22,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"YJLHVS2"]
["电线电缆检测中心",25,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"3×400"]
["电线电缆检测中心",25,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"3×400"]
["电线电缆检测中心",29,"电缆单根垂直燃烧试验","上支架下缘与炭化部分起点间距离",null,300,null,"3×400"]
["电线电缆检测中心",29,"电缆单根垂直燃烧试验","燃烧向下延伸至上支架下缘距离",null,300,null,"3×400"]
["电线电缆检测中心",16,"电缆的燃烧试验","电缆单根垂直燃烧试验",null,300,null,"2×0.75"]
["电线电缆检测中心",17,"电缆的燃烧试验","电缆单根垂直燃烧试验",null,300,null,"4×0.75"]
["电线电缆检测中心",18,"电缆的燃烧试验","电缆单根垂直燃烧试验",null,300,null,"2×0.75"]
["电线电缆检测中心",19,"电缆的燃烧试验","电缆单根垂直燃烧试验",null,300,null,"4×2.5"]
["电线电缆检测中心",19,"电缆的燃烧试验","电缆单根垂直燃烧试验",null,300,null,"4×4"]
["电线电缆检测中心",20,"电缆的燃烧试验","电缆单根垂直燃烧试验",null,300,null,"4×2.5"]
["电线电缆检测中心",20,"电缆的燃烧试验","电缆单根垂直燃烧试验",null,300,null,"48×1"]
["电线电缆检测中心",20,"电缆的燃烧试验","成束燃烧试验-A类",null,4000,null,"48×1"]
["电线电缆检测中心",20,"电缆的燃烧试验","pH值和电导率试验",null,1000,"每层","48×1"]
["电线电缆检测中心",20,"电缆的燃烧试验","烟密度试验-最小透光率",null,3000,null,"48×1"]
["电线电缆检测中心",24,"电缆的燃烧试验","电缆单根垂直燃烧试验",null,300,null,"充电桩电缆"]
["电线电缆检测中心",8,"电缆的燃烧性能","电缆单根垂直燃烧试验",null,300,null,"WDZAN"]
["电线电缆检测中心",16,"电缆的燃烧性能","电缆单根垂直燃烧试验",null,300,null,"2×0.5"]
["电线电缆检测中心",16,"电缆的燃烧性能","电缆单根垂直燃烧试验",null,300,null,"2×0.75"]
["电线电缆检测中心",16,"电缆的燃烧性能","电缆单根垂直燃烧试验",null,300,null,"KVV"]
["电线电缆检测中心",17,"电缆的燃烧性能","电缆单根垂直燃烧试验",null,300,null,"4×0.75"]
["电线电缆检测中心",18,"电缆的燃烧性能","电缆单根垂直燃烧试验",null,300,null,"2×0.75"]
["电线电缆检测中心",18,"电缆的燃烧性能","电缆单根垂直燃烧试验",null,300,null,"2×0.5"]
["电线电缆检测中心",20,"电缆的燃烧性能","电缆单根垂直燃烧试验",null,300,null,"4×1.5"]
["电线电缆检测中心",20,"电缆的燃烧性能","电缆单根垂直燃烧试验",null,300,null,"TICW计算机"]
["电线电缆检测中心",6,"电缆拉断力",null,null,4800,"拉3根","1×10"]
["电线电缆检测中心",9,"电缆拉断力",null,null,4800,"拉3根","1×10"]
["电线电缆检测中心",5,"电缆外径",null,null,75,null,"JKLYJ-1"]
["电线电缆检测中心",6,"电缆外径",null,null,75,null,"1×10"]
["电线电缆检测中心",7,"电缆外径",null,null,75,null,"1×25"]
["电线电缆检测中心",7,"电缆外径",null,null,75,null,"3×300+1×150"]
["电线电缆检测中心",7,"电缆外径",null,null,75,null,"YJV"]
["电线电缆检测中心",7,"电缆外径",null,null,75,null,"JKLV"]
["电线电缆检测中心",7,"电缆外径",null,null,75,null,"JKLYJ-1"]
["电线电缆检测中心",7,"电缆外径",null,null,75,null,"YJLHVS2常规"]
["电线电缆检测中心",8,"电缆外径",null,null,75,null,"3×300+1×150"]
["电线电缆检测中心",8,"电缆外径",null,null,75,null,"3×16"]
["电线电缆检测中心",8,"电缆外径",null,null,75,null,"VV"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"1×25"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"3×300+1×150"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"VV22"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"WDZAN-YJY23"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"YJV22"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"YJV32"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"YJY22"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"VLHV22"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"YJLHV22"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"VLHVS2"]
["电线电缆检测中心",9,"电缆外径",null,null,75,null,"YJLHVS2"]
["电线电缆检测中心",10,"电缆外径",null,null,75,null,"GB/T 33594-2017"]
["电线电缆检测中心",11,"电缆外径",null,null,75,null,"VLHV22常规"]
["电线电缆检测中心",11,"电缆外径",null,null,75,null,"VLHVS2常规"]
["电线电缆检测中心",12,"电缆外径",null,null,75,null,"YJLHV22常规"]
["电线电缆检测中心",10,"电缆外径 ",null,null,75,null,"3×400"]
["电线电缆检测中心",10,"电缆外径 ",null,null,75,null,"YJV-8.7/10"]
["电线电缆检测中心",10,"电缆外径 ",null,null,75,null,"YJV-26/35"]
["电线电缆检测中心",11,"电缆外径 ",null,null,75,null,"YJLHVS2"]
["电线电缆检测中心",13,"电缆外径 ",null,null,75,null,"YJLHV22常规"]
["电线电缆检测中心",13,"电缆外径 ",null,null,75,null,"YJLHS2常规"]
["电线电缆检测中心",13,"电缆外径 ",null,null,75,null,"YJLHVS2常规"]
["电线电缆检测中心",14,"电缆外径 ",null,null,75,null,"YJV22-8.7/10"]
["电线电缆检测中心",14,"电缆外径 ",null,null,75,null,"3×400"]
["电线电缆检测中心",14,"电缆外径 ",null,null,75,null,"YJV22-26/35"]
["电线电缆检测中心",14,"电缆外径 ",null,null,75,null,"YJLHV22"]
["电线电缆检测中心",15,"电缆外径 ",null,null,75,null,"3×400"]
["电线电缆检测中心",15,"电缆外径 ",null,null,75,null,"YJLHVS2"]
["电线电缆检测中心",15,"电缆外径 ",null,null,75,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",6,"电气性能试验","导体直流电阻",null,220,null,"1.25 黑白"]
["电线电缆检测中心",6,"电气性能试验","耐电压 ( 1 kV 30 min 然后以500V/s 的速率升压至5 kV）",null,600,null,"1.25 黑白"]
["电线电缆检测中心",6,"电气性能试验","绝缘体积电阻率",null,500,null,"1.25 黑白"]
["电线电缆检测中心",6,"电气性能试验","线性电阻",null,600,null,1]
["电线电缆检测中心",6,"电气性能试验","介电硬度和耐击穿电压试验 ( 1 kV ，30 min 然后以500 V/s 的   速度升压至5 kV）",null,600,null,1]
["电线电缆检测中心",7,"电气性能试验","导体直流电阻",null,220,"220/芯","50黑"]
["电线电缆检测中心",7,"电气性能试验","工频交流电压和击穿电压试验 ( 1 kV 30 min 然后以500V/s 的速度升压至5 kV）",null,600,null,"50黑"]
["电线电缆检测中心",7,"电气性能试验","绝缘体积电阻系数",null,600,null,"50黑"]
["电线电缆检测中心",7,"电气性能试验","20 ℃ 导体直流电阻",null,220,null,"0.75 白"]
["电线电缆检测中心",7,"电气性能试验","耐电压 ( 1 kV 30 min 然后以500V/s 的速率升压至5 kV）",null,600,null,"0.75 白"]
["电线电缆检测中心",7,"电气性能试验","绝缘体积电阻率",null,500,null,"0.75 白"]
["电线电缆检测中心",7,"电气性能试验","20 ℃ 导体直流电阻",null,220,null,1]
["电线电缆检测中心",7,"电气性能试验","耐电压 (1 kV 30 min 然后以500V/s 的速率升压至5 kV）",null,600,null,1]
["电线电缆检测中心",7,"电气性能试验","绝缘体积电阻率",null,500,null,1]
["电线电缆检测中心",9,"电气性能试验","20 ℃ 导体直流电阻",null,220,"220/芯","DIN 72551-5/1991"]
["电线电缆检测中心",9,"电气性能试验","耐电压 (1 kV 30 min 然后以500V/s 的速率升压至5 kV）",null,600,null,"DIN 72551-5/1991"]
["电线电缆检测中心",9,"电气性能试验","绝缘体积电阻率",null,500,null,"DIN 72551-5/1991"]
["电线电缆检测中心",3,"电线平均外径上限 ",null,null,75,null,"50黑"]
["电线电缆检测中心",3,"电线外形尺寸",null,null,75,null,1]
["电线电缆检测中心",3,"电线外形尺寸",null,null,75,null,"0.75 白"]
["电线电缆检测中心",3,"电线外形尺寸",null,null,75,null,"DIN 72551-5/1991"]
["电线电缆检测中心",5,"电性能","20℃时的直流电阻",null,220,null,"全部参数"]
["电线电缆检测中心",5,"电性能","击穿电压",null,600,null,"全部参数"]
["电线电缆检测中心",5,"电性能","击穿电压",null,800,null,"全部参数"]
["电线电缆检测中心",5,"电性能","漆膜连续性（个）（缺陷） （试验电压:1500V）",null,110,null,"全部参数"]
["电线电缆检测中心",5,"电性能","介质损耗系数tanδ",null,800,null,"全部参数"]
["电线电缆检测中心",6,"电性能","导体直流电阻(20℃)",null,220,null,"60227 IEC 01（BV） 450/750V"]
["电线电缆检测中心",6,"电性能","导体直流电阻(20℃)",null,220,null,"BVR 450/750V"]
["电线电缆检测中心",6,"电性能","导体直流电阻(20℃)",null,220,null,"BYJ"]
["电线电缆检测中心",6,"电性能","导体直流电阻(20℃)",null,220,null,"全项WDZAN-BYJ-105 450/750 1×2.5"]
["电线电缆检测中心",6,"电性能","导体直流电阻(20℃)",null,220,null,"常规WDZA-BYJ 450/750V  1×2.5"]
["电线电缆检测中心",7,"电性能","导体直流电阻(20℃)",null,660,null,"2×1.5"]
["电线电缆检测中心",7,"电性能","绝缘线芯交流电压试验(2000V/5min)",null,400,null,"2×1.5"]
["电线电缆检测中心",7,"电性能","导体直流电阻(20℃)",null,220,null,"1×2.5"]
["电线电缆检测中心",7,"电性能","70℃绝缘电阻",null,600,null,"1×2.5"]
["电线电缆检测中心",7,"电性能","成品电缆交流电压试验(2500V/5min)",null,400,null,"1×2.5"]
["电线电缆检测中心",7,"电性能","导体直流电阻(20℃)",null,220,null,"1×0.75"]
["电线电缆检测中心",7,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"1×0.75"]
["电线电缆检测中心",7,"电性能","导体直流电阻(20℃)",null,220,null,"02RV"]
["电线电缆检测中心",7,"电性能","70℃绝缘电阻",null,600,null,"02RV"]
["电线电缆检测中心",7,"电性能","绝缘线芯交流电压试验(2500V/5min)",null,400,null,"02RV"]
["电线电缆检测中心",7,"电性能","导体直流电阻(20℃)",null,220,null,"06RV"]
["电线电缆检测中心",7,"电性能","70℃绝缘电阻",null,600,null,"06RV"]
["电线电缆检测中心",7,"电性能","绝缘线芯交流电压试验(2000V/5min)",null,400,null,"06RV"]
["电线电缆检测中心",7,"电性能","导体直流电阻(20℃)",null,220,null,"BLV"]
["电线电缆检测中心",7,"电性能","70℃绝缘电阻",null,600,null,"BLV"]
["电线电缆检测中心",7,"电性能","成品电缆交流电压试验(2500V/5min)",null,400,null,"BLV"]
["电线电缆检测中心",7,"电性能","导体直流电阻(20℃)",null,220,null,"BV"]
["电线电缆检测中心",7,"电性能","70℃绝缘电阻",null,600,null,"BV"]
["电线电缆检测中心",7,"电性能","绝缘线芯交流电压试验(2500V/5min)",null,400,null,"BV"]
["电线电缆检测中心",7,"电性能","导体直流电阻(20℃)",null,220,null,"BVR"]
["电线电缆检测中心",7,"电性能","70℃绝缘电阻",null,600,null,"BVR"]
["电线电缆检测中心",7,"电性能","成品电缆交流电压试验(2500V/5min)",null,400,null,"BVR"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,220,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",8,"电性能","成品电缆电压试验(2000V/5min)",null,400,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,220,null,"1×16"]
["电线电缆检测中心",8,"电性能","成品电缆交流电压试验(1000V/5min)",null,400,null,"1×16"]
["电线电缆检测中心",8,"电性能","70℃绝缘电阻",null,600,null,"1×1.5"]
["电线电缆检测中心",8,"电性能","绝缘线芯交流电压试验(2500V/5min)",null,400,null,"1×1.5"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,220,null,"1×1.5"]
["电线电缆检测中心",8,"电性能","70℃绝缘电阻",null,600,null,"1×0.5"]
["电线电缆检测中心",8,"电性能","90℃绝缘电阻",null,600,null,"1×0.5"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,220,null,"1×0.5"]
["电线电缆检测中心",8,"电性能","绝缘线芯交流电压试验(2000V/5min)",null,400,null,"1×0.5"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,440,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,440,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,440,null,"BVVB 300/500V"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,400,null,"2×0.5"]
["电线电缆检测中心",8,"电性能","绝缘线芯电压试验（2000V/5min）",null,400,null,"2×0.5"]
["电线电缆检测中心",8,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×0.5"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,440,null,"RVS 300/300V"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,440,null,"RVV 300/500V"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,220,null,"YC 450/750V"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,660,null,"YJV"]
["电线电缆检测中心",8,"电性能","导体直流电阻(20℃)",null,660,null,"YJLHVS2常规"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,660,null,"6×1"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"6×1"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"6×1"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(2000V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,220,null,"1×0.75"]
["电线电缆检测中心",9,"电性能","70℃绝缘电阻",null,600,null,"1×0.75"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(2000V/5min)",null,400,null,"1×0.75"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"1×0.75"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"2×1.0"]
["电线电缆检测中心",9,"电性能","70℃绝缘电阻",null,600,null,"2×1.0"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×1.0"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,220,null,"1×0.08"]
["电线电缆检测中心",9,"电性能","90℃绝缘电阻",null,600,null,"1×0.08"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(1500V/5min)",null,400,null,"1×0.08"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.12"]
["电线电缆检测中心",9,"电性能","70℃绝缘电阻",null,600,null,"2×0.12"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(1500V/5min)",null,400,null,"2×0.12"]
["电线电缆检测中心",9,"电性能","70℃绝缘电阻",null,600,null,"1×0.08"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,220,null,"1×1"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(1500V/5min)",null,400,null,"1×1"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"1×1"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.3"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(1500V/5min)",null,400,null,"2×0.3"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×0.3"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.75"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"2×4"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×4"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"2×4"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"YCW"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,660,null,"3×300+1×150"]
["电线电缆检测中心",9,"电性能","90℃绝缘电阻常数Ki",null,600,null,"3×300+1×150"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"3×300+1×150"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,660,null,"VV"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"BVVB,BLVVB"]
["电线电缆检测中心",9,"电性能","70℃绝缘电阻",null,600,null,"BVVB,BLVVB"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(2000V/5min)",null,400,null,"BVVB,BLVVB"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"BVVB,BLVVB"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"RVS"]
["电线电缆检测中心",9,"电性能","70℃绝缘电阻",null,600,null,"RVS"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"RVS"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"RVV"]
["电线电缆检测中心",9,"电性能","70℃绝缘电阻",null,600,null,"RVV"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"RVV"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"RVV"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,220,null,"YC"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(1500V/5min)",null,400,null,"YC"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"YC"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,660,null,"YJV,YJLV"]
["电线电缆检测中心",9,"电性能","90℃绝缘电阻常数Ki",null,600,null,"YJV,YJLV"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"YJV,YJLV"]
["电线电缆检测中心",9,"电性能","导体直流电阻(20℃)",null,440,null,"YZ"]
["电线电缆检测中心",9,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"YZ"]
["电线电缆检测中心",9,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"YZ"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,220,null,"1×95"]
["电线电缆检测中心",10,"电性能","成品电缆交流电压试验(1000V/5min)",null,400,null,"1×95"]
["电线电缆检测中心",10,"电性能","70℃绝缘电阻",null,600,null,"2×1.5"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(2000V/5min)",null,400,null,"2×1.5"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,220,null,"1×0.5"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(2000V/5min)",null,400,null,"1×0.5"]
["电线电缆检测中心",10,"电性能","70℃绝缘电阻",null,600,null,"2×0.5"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(1500V/5min)",null,400,null,"2×0.5"]
["电线电缆检测中心",10,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×0.5"]
["电线电缆检测中心",10,"电性能","70℃绝缘电阻",null,600,null,"2×0.75"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.5"]
["电线电缆检测中心",10,"电性能","90℃绝缘电阻",null,600,null,"2×0.5"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.75"]
["电线电缆检测中心",10,"电性能","90℃绝缘电阻",null,600,null,"2×0.75"]
["电线电缆检测中心",10,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,440,null,"2×1.5"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"2×1.5"]
["电线电缆检测中心",10,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×1.5"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,220,null,"1×0.08"]
["电线电缆检测中心",10,"电性能","成品电缆交流电压试验(1500V/5min)",null,400,null,"1×0.08"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.08"]
["电线电缆检测中心",10,"电性能","90℃绝缘电阻",null,600,null,"2×0.08"]
["电线电缆检测中心",10,"电性能","成品电缆交流电压试验(绝缘厚度0.6mm及以下：1500V/5min；绝缘厚度0.6mm以上：2000V/5min)",null,400,null,"2×0.08"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,440,null,"RVVP 300/300V"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,660,null,"3×300+1×150"]
["电线电缆检测中心",10,"电性能","20℃绝缘电阻常数Ki",null,600,null,"3×300+1×150"]
["电线电缆检测中心",10,"电性能","70℃绝缘电阻常数Ki",null,600,null,"3×300+1×150"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"3×300+1×150"]
["电线电缆检测中心",10,"电性能","绝缘吸水试验(电压法)",null,1200,null,"3×300+1×150"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,660,null,"3×16"]
["电线电缆检测中心",10,"电性能","20℃绝缘电阻常数Ki",null,600,null,"3×16"]
["电线电缆检测中心",10,"电性能","70℃绝缘电阻常数Ki",null,600,null,"3×16"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"3×16"]
["电线电缆检测中心",10,"电性能","绝缘吸水试验(电压法)",null,1200,null,"3×16"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,660,null,"VV22"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,660,null,"WDZAN-YJY23"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,660,null,"YJV22"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,660,null,"YJV32"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,660,null,"YJY22"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,440,null,"AVVR"]
["电线电缆检测中心",10,"电性能","70℃绝缘电阻",null,600,null,"AVVR"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(1500V/5min)",null,400,null,"AVVR"]
["电线电缆检测中心",10,"电性能","成品电缆交流电压试验(1500V/5min)",null,400,null,"AVVR"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,660,null,"VV,VLV"]
["电线电缆检测中心",10,"电性能","20℃绝缘电阻常数Ki",null,600,null,"VV,VLV"]
["电线电缆检测中心",10,"电性能","70℃绝缘电阻常数Ki",null,600,null,"VV,VLV"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"VV,VLV"]
["电线电缆检测中心",10,"电性能","导体直流电阻(20℃)",null,660,null,"VLHVS2"]
["电线电缆检测中心",10,"电性能","70℃绝缘电阻常数Ki",null,600,null,"VLHVS2"]
["电线电缆检测中心",10,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"VLHVS2"]
["电线电缆检测中心",10,"电性能","绝缘吸水试验(电压法)",null,1200,null,"VLHVS2"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,440,null,"2×1.5"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(2000V/5min)",null,400,null,"2×1.5"]
["电线电缆检测中心",11,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×1.5"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,660,null,"6×1"]
["电线电缆检测中心",11,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"6×1"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"6×1"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.12"]
["电线电缆检测中心",11,"电性能","成品电缆交流电压试验(1500V/5min)",null,400,null,"2×0.12"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.08"]
["电线电缆检测中心",11,"电性能","70℃绝缘电阻",null,600,null,"2×0.08"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(1500V/5min)",null,400,null,"2×0.08"]
["电线电缆检测中心",11,"电性能","成品电缆交流电压试验(1500V/5min)",null,400,null,"2×0.08"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,440,null,"2×35"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"2×35"]
["电线电缆检测中心",11,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×35"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.3"]
["电线电缆检测中心",11,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×0.3"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,440,null,"3×0.3"]
["电线电缆检测中心",11,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"3×0.3"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,440,null,"KVV"]
["电线电缆检测中心",11,"电性能","70℃绝缘电阻",null,300,null,"KVVR"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,440,null,"KYJV"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,660,null,"3×300+1×150"]
["电线电缆检测中心",11,"电性能","70℃绝缘电阻常数Ki",null,600,null,"3×300+1×150"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"3×300+1×150"]
["电线电缆检测中心",11,"电性能","绝缘吸水试验(电压法)",null,1200,null,"3×300+1×150"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,660,null,"YJY22"]
["电线电缆检测中心",11,"电性能","90℃绝缘电阻常数Ki",null,300,null,"YJY22"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"YJY22"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,440,null,"RVVP"]
["电线电缆检测中心",11,"电性能","70℃绝缘电阻",null,600,null,"RVVP"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"RVVP"]
["电线电缆检测中心",11,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"RVVP"]
["电线电缆检测中心",11,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","YJV-8.7/10"]
["电线电缆检测中心",11,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","YJV-26/35"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,660,null,"VLHV22"]
["电线电缆检测中心",11,"电性能","20℃绝缘电阻常数Ki",null,600,null,"VLHV22"]
["电线电缆检测中心",11,"电性能","70℃绝缘电阻常数Ki",null,600,null,"VLHV22"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"VLHV22"]
["电线电缆检测中心",11,"电性能","绝缘吸水试验(电压法)",null,1200,null,"VLHV22"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,660,null,"YJLHV22"]
["电线电缆检测中心",11,"电性能","90℃绝缘电阻常数Ki",null,300,null,"YJLHV22"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"YJLHV22"]
["电线电缆检测中心",11,"电性能","导体直流电阻(20℃)",null,660,null,"YJLHVS2"]
["电线电缆检测中心",11,"电性能","90℃绝缘电阻常数Ki",null,300,null,"YJLHVS2"]
["电线电缆检测中心",11,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"YJLHVS2"]
["电线电缆检测中心",12,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.75"]
["电线电缆检测中心",12,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",12,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",12,"电性能","导体直流电阻(20℃)",null,220,null,"1×1.5"]
["电线电缆检测中心",12,"电性能","绝缘线芯交流电压试验(2500V/5min)",null,400,null,"1×1.5"]
["电线电缆检测中心",12,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"1×1.5"]
["电线电缆检测中心",12,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.08"]
["电线电缆检测中心",12,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"2×0.08"]
["电线电缆检测中心",12,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×0.08"]
["电线电缆检测中心",12,"电性能","导体直流电阻(20℃)",null,660,null,"KVV22"]
["电线电缆检测中心",12,"电性能","导体直流电阻(20℃)",null,660,null,"KYJV22"]
["电线电缆检测中心",12,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","3×400"]
["电线电缆检测中心",12,"电性能","tanδ(95℃～100℃,2kV)",null,2800,null,"3×400"]
["电线电缆检测中心",12,"电性能","加热循环试验",null,2000,null,"3×400"]
["电线电缆检测中心",12,"电性能","随后的局部放电试验（1.73 U0）",null,1200,null,"3×400"]
["电线电缆检测中心",12,"电性能","冲击电压试验(95℃～100℃,75kV正负极性各10次)",null,1500,null,"3×400"]
["电线电缆检测中心",12,"电性能","4h工频电压试验(4U0)",null,1500,null,"3×400"]
["电线电缆检测中心",12,"电性能","冲击电压试验(95℃～100℃,95kV正负极性各10次)",null,1500,null,"3×400"]
["电线电缆检测中心",12,"电性能","随后的交流电压试验(室温,30.5kV,15min)",null,1500,null,"3×400"]
["电线电缆检测中心",12,"电性能","弯曲试验",null,470,null,"3×400"]
["电线电缆检测中心",12,"电性能","弯曲随后的局部放电试验（1.73 U0）",null,1200,null,"3×400"]
["电线电缆检测中心",12,"电性能","tanδ(95℃～100℃,26kV)",null,2800,null,"3×400"]
["电线电缆检测中心",12,"电性能","冲击电压试验(95℃～100℃,200kV正负极性各10次)",null,1500,null,"3×400"]
["电线电缆检测中心",12,"电性能","随后的交流电压试验(室温,91kV,15min)",null,1500,null,"3×400"]
["电线电缆检测中心",12,"电性能","导体直流电阻(20℃)",null,660,null,"VLHV22常规"]
["电线电缆检测中心",12,"电性能","导体直流电阻(20℃)",null,660,null,"VLHVS2常规"]
["电线电缆检测中心",12,"电性能","导体直流电阻(20℃)",null,660,null,"GB/T 33594-2017"]
["电线电缆检测中心",12,"电性能","绝缘电阻常数",null,600,null,"GB/T 33594-2017"]
["电线电缆检测中心",12,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"GB/T 33594-2017"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,660,null,"2×2×0.12"]
["电线电缆检测中心",13,"电性能","70℃绝缘电阻",null,600,null,"2×2×0.12"]
["电线电缆检测中心",13,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：1500V/5min； 绝缘厚度大于0.6mm：2000V/5min)",null,400,null,"2×2×0.12"]
["电线电缆检测中心",13,"电性能","成品电缆交流电压试验(2000V/5min)",null,400,null,"2×2×0.12"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.5"]
["电线电缆检测中心",13,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"2×0.5"]
["电线电缆检测中心",13,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"2×0.5"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.75"]
["电线电缆检测中心",13,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",13,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,440,null,"KVVP"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,660,null,"KVVP2-22"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,440,null,"KVVRP"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,440,null,"KYJVP"]
["电线电缆检测中心",13,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"KYJVP"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,660,null,"KYJVP2-22"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,660,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,440,null,"KVV"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,660,null,"YJY"]
["电线电缆检测中心",13,"电性能","90℃绝缘电阻常数Ki",null,600,null,"YJY"]
["电线电缆检测中心",13,"电性能","绝缘线芯交流电压试验(4U_(0)/4h)",null,1000,null,"YJY"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,660,null,"YJLHV22常规"]
["电线电缆检测中心",13,"电性能","导体直流电阻（20℃）",null,960,"320/芯","YJLHVS2"]
["电线电缆检测中心",13,"电性能","弯曲试验",null,470,null,"YJLHVS2"]
["电线电缆检测中心",13,"电性能","弯曲随后的局部放电试验（1.73 U0）",null,1200,null,"YJLHVS2"]
["电线电缆检测中心",13,"电性能","加热循环试验",null,2000,null,"YJLHVS2"]
["电线电缆检测中心",13,"电性能","随后的局部放电试验（1.73 U0）",null,1200,null,"YJLHVS2"]
["电线电缆检测中心",13,"电性能","冲击电压试验(95℃～100℃,75kV正负极性各10次)",null,1500,null,"YJLHVS2"]
["电线电缆检测中心",13,"电性能","随后的交流电压试验(室温,30.5kV,15min)",null,1500,null,"YJLHVS2"]
["电线电缆检测中心",13,"电性能","导体直流电阻(20℃)",null,440,null,"QC/T1037-2016"]
["电线电缆检测中心",13,"电性能","绝缘层绝缘体积电阻率",null,600,null,"QC/T1037-2016"]
["电线电缆检测中心",13,"电性能","护套层耐压",null,400,null,"QC/T1037-2016"]
["电线电缆检测中心",14,"电性能","70℃绝缘电阻",null,600,null,"4×0.75"]
["电线电缆检测中心",14,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"4×0.75"]
["电线电缆检测中心",14,"电性能","90℃绝缘电阻",null,600,null,"4×0.75"]
["电线电缆检测中心",14,"电性能","导体直流电阻(20℃)",null,660,null,"4×0.75"]
["电线电缆检测中心",14,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"4×0.75"]
["电线电缆检测中心",14,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","YJLHV22常规"]
["电线电缆检测中心",14,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","YJLHS2常规"]
["电线电缆检测中心",14,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","YJLHVS2常规"]
["电线电缆检测中心",14,"电性能","导体直流电阻(20℃)",null,440,null,"充电桩电缆"]
["电线电缆检测中心",14,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"充电桩电缆"]
["电线电缆检测中心",14,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"充电桩电缆"]
["电线电缆检测中心",14,"电性能","护套表面电阻",null,660,null,"充电桩电缆"]
["电线电缆检测中心",15,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.75"]
["电线电缆检测中心",15,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"电性能","导体直流电阻(20℃)",null,440,null,"2×0.5"]
["电线电缆检测中心",15,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"2×0.5"]
["电线电缆检测中心",15,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"2×0.5"]
["电线电缆检测中心",15,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","YJV22-8.7/10"]
["电线电缆检测中心",15,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","YJV22-26/35"]
["电线电缆检测中心",16,"电性能","导体直流电阻(20℃)",null,660,null,"4×4"]
["电线电缆检测中心",16,"电性能","70℃绝缘电阻",null,600,null,"4×4"]
["电线电缆检测中心",16,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"4×4"]
["电线电缆检测中心",16,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"4×4"]
["电线电缆检测中心",16,"电性能","导体直流电阻(20℃)",null,660,null,"4×2.5"]
["电线电缆检测中心",16,"电性能","90℃绝缘电阻",null,600,null,"4×2.5"]
["电线电缆检测中心",16,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"4×2.5"]
["电线电缆检测中心",16,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"4×2.5"]
["电线电缆检测中心",16,"电性能","90℃绝缘电阻",null,600,null,"4×4"]
["电线电缆检测中心",16,"电性能","弯曲随后的局部放电试验（1.73 U0）",null,1500,null,"3×400"]
["电线电缆检测中心",16,"电性能","随后的局部放电试验（1.73 U0）",null,1200,null,"3×400"]
["电线电缆检测中心",16,"电性能","冲击电压试验(95℃～100℃,75kV正负极性各10次)",null,1500,null,"3×400"]
["电线电缆检测中心",16,"电性能","随后的交流电压试验(室温,30.5kV,15min)",null,1500,null,"3×400"]
["电线电缆检测中心",16,"电性能","弯曲随后的局部放电试验（1.73 U0）",null,1200,null,"3×400"]
["电线电缆检测中心",16,"电性能","随后的局部放电试验（1.73 U0）",null,1500,null,"3×400"]
["电线电缆检测中心",16,"电性能","冲击电压试验(95℃～100℃,95kV正负极性各10次)",null,1500,null,"3×400"]
["电线电缆检测中心",16,"电性能","冲击电压试验(95℃～100℃,200kV正负极性各10次)",null,1500,null,"3×400"]
["电线电缆检测中心",16,"电性能","随后的交流电压试验(室温,91kV,15min)",null,1500,null,"3×400"]
["电线电缆检测中心",16,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","3×400"]
["电线电缆检测中心",16,"电性能","弯曲试验",null,470,null,"3×400"]
["电线电缆检测中心",16,"电性能","加热循环试验",null,2000,null,"3×400"]
["电线电缆检测中心",16,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","YJLHV22"]
["电线电缆检测中心",16,"电性能","弯曲试验",null,470,null,"YJLHV22"]
["电线电缆检测中心",16,"电性能","弯曲随后的局部放电试验（1.73 U0）",null,1200,null,"YJLHV22"]
["电线电缆检测中心",16,"电性能","tanδ(95℃～100℃,2kV)",null,2800,null,"YJLHV22"]
["电线电缆检测中心",16,"电性能","加热循环试验",null,2000,null,"YJLHV22"]
["电线电缆检测中心",16,"电性能","随后的局部放电试验（1.73 U0）",null,1200,null,"YJLHV22"]
["电线电缆检测中心",16,"电性能","冲击电压试验(95℃～100℃,75kV正负极性各10次)",null,1500,null,"YJLHV22"]
["电线电缆检测中心",16,"电性能","随后的交流电压试验(室温,30.5kV,15min)",null,1500,null,"YJLHV22"]
["电线电缆检测中心",16,"电性能","4h工频电压试验(4U0)",null,1500,null,"YJLHV22"]
["电线电缆检测中心",16,"电性能","导体直流电阻(20℃)",null,440,null,"TICW计算机"]
["电线电缆检测中心",16,"电性能","70℃绝缘电阻",null,600,null,"TICW计算机"]
["电线电缆检测中心",16,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"TICW计算机"]
["电线电缆检测中心",17,"电性能","导体直流电阻(20℃)",null,660,null,"4×1.5"]
["电线电缆检测中心",17,"电性能","70℃绝缘电阻",null,600,null,"4×1.5"]
["电线电缆检测中心",17,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"4×1.5"]
["电线电缆检测中心",17,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"4×1.5"]
["电线电缆检测中心",17,"电性能","导体直流电阻(20℃)",null,660,null,"4×2.5"]
["电线电缆检测中心",17,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"4×2.5"]
["电线电缆检测中心",17,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"4×2.5"]
["电线电缆检测中心",17,"电性能","导体直流电阻(20℃)",null,660,null,"48×1"]
["电线电缆检测中心",17,"电性能","90℃绝缘电阻",null,600,null,"48×1"]
["电线电缆检测中心",17,"电性能","绝缘线芯交流电压试验(绝缘厚度0.6mm及以下：2000V/5min； 绝缘厚度大于0.6mm：2500V/5min)",null,400,null,"48×1"]
["电线电缆检测中心",17,"电性能","成品电缆交流电压试验(3000V/5min)",null,400,null,"48×1"]
["电线电缆检测中心",17,"电性能","导体直流电阻（20℃）",null,960,null,"YJLHVS2"]
["电线电缆检测中心",17,"电性能","弯曲试验",null,470,null,"YJLHVS2"]
["电线电缆检测中心",17,"电性能","弯曲随后的局部放电试验（1.73 U0）",null,1200,null,"YJLHVS2"]
["电线电缆检测中心",17,"电性能","tanδ(95℃～100℃,2kV)",null,2800,null,"YJLHVS2"]
["电线电缆检测中心",17,"电性能","加热循环试验",null,2000,null,"YJLHVS2"]
["电线电缆检测中心",17,"电性能","随后的局部放电试验（1.73 U0）",null,1200,null,"YJLHVS2"]
["电线电缆检测中心",17,"电性能","冲击电压试验(95℃～100℃,75kV正负极性各10次)",null,1500,null,"YJLHVS2"]
["电线电缆检测中心",17,"电性能","随后的交流电压试验(室温,30.5kV,15min)",null,1500,null,"YJLHVS2"]
["电线电缆检测中心",17,"电性能","4h工频电压试验(4U0)",null,1500,null,"YJLHVS2"]
["电线电缆检测中心",17,"电性能","导体直流电阻（20℃）",null,960,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",17,"电性能","弯曲试验",null,470,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",17,"电性能","弯曲随后的局部放电试验（1.73 U0）",null,1200,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",17,"电性能","tanδ(95℃～100℃,26kV)",null,2800,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",17,"电性能","加热循环试验",null,2000,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",17,"电性能","随后的局部放电试验（1.73 U0）",null,1200,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",17,"电性能","冲击电压试验(95℃～100℃,200kV正负极性各10次)",null,1500,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",17,"电性能","随后的交流电压试验(室温,91kV,15min)",null,1500,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",17,"电性能","4h工频电压试验(4U0)",null,1500,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",18,"电性能","导体直流电阻（20℃）",null,960,"320/芯（其中制备样品100/芯）","3×400"]
["电线电缆检测中心",18,"电性能","弯曲试验",null,470,null,"3×400"]
["电线电缆检测中心",18,"电性能","弯曲随后的局部放电试验（1.73 U0）",null,1200,null,"3×400"]
["电线电缆检测中心",18,"电性能","加热循环试验",null,2000,null,"3×400"]
["电线电缆检测中心",18,"电性能","随后的局部放电试验（1.73 U0）",null,1200,null,"3×400"]
["电线电缆检测中心",18,"电性能","冲击电压试验(95℃～100℃,75kV正负极性各10次)",null,1500,null,"3×400"]
["电线电缆检测中心",18,"电性能","随后的交流电压试验(室温,30.5kV,15min)",null,1500,null,"3×400"]
["电线电缆检测中心",8,"电压试验（3.5kV,1min）",null,null,1000,null,"1×10"]
["电线电缆检测中心",9,"电压试验（3.5kV,1min）",null,null,1000,null,"1×10"]
["电线电缆检测中心",11,"电压试验（3.5kV,1min）",null,null,1000,null,"1×10"]
["电线电缆检测中心",12,"电压试验（3.5kV,1min）",null,null,1000,null,"1×10"]
["电线电缆检测中心",1,"毒性指数",null,"GB/T 32129-2015",5000,null,"GB/T32129-2015"]
["电线电缆检测中心",9,"镀层质量","热镀锌钢丝表面",null,270,null,"全部参数"]
["电线电缆检测中心",9,"镀层质量","钢丝锌层重量(g/m2)",null,270,null,"全部参数"]
["电线电缆检测中心",9,"镀层质量","钢丝锌层牢固性（芯棒直径10d ，缠绕6圈）",null,280,null,"全部参数"]
["电线电缆检测中心",12,"镀锌钢线单线性能","抗拉强度（绞后）",null,250,null,"630/35-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","1%伸长时的应力",null,390,null,"630/35-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","断裂伸长率",null,280,null,"630/35-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","扭转(100d)",null,770,null,"630/35-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","锌层重量",null,280,null,"630/35-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","镀锌层附着性(4d,8圈)",null,280,null,"630/35-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","卷绕(1d,8圈)",null,580,null,"630/35-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","镀锌层连续性",null,280,null,"630/35-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","抗拉强度（绞后）",null,250,null,"300/20-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","1%伸长时的应力",null,390,null,"300/20-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","断裂伸长率(%)",null,280,null,"300/20-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","扭转(100d)",null,770,null,"300/20-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","锌层重量",null,280,null,"300/20-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","镀锌层附着性(4d,8圈)",null,280,null,"300/20-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","卷绕(3d,8圈)",null,580,null,"300/20-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","镀锌层连续性",null,280,null,"300/20-45/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","抗拉强度（绞后）",null,250,null,"185/25-24/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","1%伸长时的应力",null,390,null,"185/25-24/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","断裂伸长率",null,280,null,"185/25-24/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","扭转(100d)",null,770,null,"185/25-24/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","锌层重量",null,280,null,"185/25-24/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","镀锌层附着性(4d,8圈)",null,280,null,"185/25-24/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","镀锌层连续性",null,280,null,"185/25-24/7"]
["电线电缆检测中心",12,"镀锌钢线单线性能","卷绕(1d,8圈)",null,580,null,"185/25-24/7"]
["电线电缆检测中心",2,"镀锌钢线根数",null,null,110,null,"630/35-45/7"]
["电线电缆检测中心",2,"镀锌钢线根数",null,null,110,null,"300/20-45/7"]
["电线电缆检测中心",2,"镀锌钢线根数",null,null,110,null,"185/25-24/7"]
["电线电缆检测中心",4,"镀锌钢线直径",null,null,110,null,"630/35-45/7"]
["电线电缆检测中心",4,"镀锌钢线直径",null,null,110,null,"300/20-45/7"]
["电线电缆检测中心",4,"镀锌钢线直径",null,null,110,null,"185/25-24/7"]
["电线电缆检测中心",6,"断裂后伸长率(L0=250mm)",null,null,250,null,"全部参数"]
["电线电缆检测中心",10,"对绞合节距比每根绝缘线芯平均外径上线",null,null,110,null,"2×2×0.12"]
["电线电缆检测中心",13,"纺纤编织层的耐热性(铝块处理条件：260℃,4h)",null,null,600,null,"3×0.3"]
["电线电缆检测中心",13,"纺纤编织层的耐热性(铝块处理条件：260℃,4h)",null,null,600,null,"2×0.3"]
["电线电缆检测中心",11,"非污染试验","绝缘非污染试验(80℃,7d)",null,450,null,"2×1.5"]
["电线电缆检测中心",11,"非污染试验","护套非污染试验(80℃,7d)",null,450,null,"2×1.5"]
["电线电缆检测中心",13,"非污染试验","绝缘非污染试验(80℃,7d)",null,450,null,"2×1.5"]
["电线电缆检测中心",13,"非污染试验","护套非污染试验(80℃,7d)",null,450,null,"2×1.5"]
["电线电缆检测中心",13,"非污染试验","绝缘非污染试验(80℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",13,"非污染试验","护套非污染试验(80℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",25,"氟含量",null,null,1000,"1000/层","3×300+1×150"]
["电线电缆检测中心",27,"氟含量",null,null,1000,"1000/层","GB/T 33594-2017"]
["电线电缆检测中心",39,"氟含量-护套",null,null,1000,"护套为（U,YJ）时做","充电桩电缆"]
["电线电缆检测中心",36,"氟含量-绝缘",null,null,1000,"绝缘为（EY）时做","充电桩电缆"]
["电线电缆检测中心",6,"复合覆盖层中的护套平均厚度",null,null,110,null,"1×95"]
["电线电缆检测中心",7,"复合覆盖层中的护套最薄厚度",null,null,110,null,"1×95"]
["电线电缆检测中心",12,"覆盖层或复合覆盖层中的护套机械性能","老化前拉力试验",null,250,null,"1×95"]
["电线电缆检测中心",12,"覆盖层或复合覆盖层中的护套机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"1×95"]
["电线电缆检测中心",12,"覆盖层或复合覆盖层中的护套机械性能","浸矿物油后拉力试验（100℃,24h）",null,900,null,"1×95"]
["电线电缆检测中心",12,"覆盖层或复合覆盖层中的护套机械性能","浸矿物油后拉力试验（100℃,25h）",null,900,null,"1×95"]
["电线电缆检测中心",12,"覆盖层或复合覆盖层中的护套机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"1×95"]
["电线电缆检测中心",9,"覆盖层机械性能","老化前拉力试验",null,250,null,"1×16"]
["电线电缆检测中心",9,"覆盖层机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"1×16"]
["电线电缆检测中心",9,"覆盖层机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"1×16"]
["电线电缆检测中心",4,"覆盖层平均厚度",null,null,110,null,"1×16"]
["电线电缆检测中心",4,"覆盖层平均厚度",null,null,110,null,"1×95"]
["电线电缆检测中心",5,"覆盖层最薄处厚度",null,null,110,null,"1×16"]
["电线电缆检测中心",5,"覆盖层最薄处厚度",null,null,110,null,"1×95"]
["电线电缆检测中心",10,"钢带厚度",null,null,55,null,"3×400"]
["电线电缆检测中心",10,"钢带厚度",null,null,55,null,"YJV22-8.7/10"]
["电线电缆检测中心",10,"钢带厚度",null,null,55,null,"YJV22-26/35"]
["电线电缆检测中心",10,"钢带厚度",null,null,55,null,"YJLHV22"]
["电线电缆检测中心",11,"钢带厚度",null,null,55,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",7,"钢绞线的最小破断拉力",null,null,490,null,"全部参数"]
["电线电缆检测中心",10,"钢丝铠装 -直径",null,null,110,null,"4×4"]
["电线电缆检测中心",8,"钢丝力学性能","抗拉强度",null,195,null,"全部参数"]
["电线电缆检测中心",8,"钢丝力学性能","伸长率(L0=200mm)",null,195,null,"全部参数"]
["电线电缆检测中心",8,"钢丝力学性能","扭转 （L=100d)",null,770,null,"全部参数"]
["电线电缆检测中心",3,"钢丝内层节径比",null,null,85,null,"全部参数"]
["电线电缆检测中心",4,"钢丝外层节径比",null,null,85,null,"全部参数"]
["电线电缆检测中心",2,"钢丝直径",null,null,75,null,"全部参数"]
["电线电缆检测中心",18,"高密度聚乙烯绝缘熔体指数试验",null,null,450,null,"1×25"]
["电线电缆检测中心",20,"高密度聚乙烯绝缘熔体指数试验",null,null,450,null,"1×25"]
["电线电缆检测中心",15,"高温压力",null,null,600,null,"QC/T1037-2016"]
["电线电缆检测中心",9,"高温压力试验","绝缘高温压力试验（80℃；4h）",null,600,null,"1×2.5"]
["电线电缆检测中心",9,"高温压力试验","绝缘高温压力试验（80℃；4h）",null,600,null,"1×0.75"]
["电线电缆检测中心",10,"高温压力试验","绝缘高温压力试验（70℃；4h）",null,600,null,"2×0.5"]
["电线电缆检测中心",11,"高温压力试验","绝缘高温压力试验（70℃；4h）",null,600,null,"2×1.0"]
["电线电缆检测中心",12,"高温压力试验","绝缘高温压力(80℃,4h)",null,600,null,"2×0.75"]
["电线电缆检测中心",12,"高温压力试验","护套高温压力(80℃,4h)",null,600,null,"2×0.75"]
["电线电缆检测中心",12,"高温压力试验","绝缘高温压力(80℃,4h)",null,600,null,"1×0.75"]
["电线电缆检测中心",12,"高温压力试验","护套高温压力(80℃,4h)",null,600,null,"1×0.75"]
["电线电缆检测中心",12,"高温压力试验","绝缘高温压力试验（90℃；4h）",null,600,null,"1×0.08"]
["电线电缆检测中心",12,"高温压力试验","绝缘高温压力试验（80℃；4h）",null,600,null,"2×0.12"]
["电线电缆检测中心",12,"高温压力试验","绝缘高温压力试验（80℃；4h）",null,600,null,"1×0.08"]
["电线电缆检测中心",13,"高温压力试验","绝缘高温压力(70℃,4h)",null,600,null,"2×0.5"]
["电线电缆检测中心",13,"高温压力试验","护套高温压力（70℃，4h）",null,600,null,"2×0.5"]
["电线电缆检测中心",13,"高温压力试验","绝缘高温压力(90℃,4h)",null,600,null,"2×0.5"]
["电线电缆检测中心",13,"高温压力试验","护套高温压力（90℃，4h）",null,600,null,"2×0.5"]
["电线电缆检测中心",13,"高温压力试验","绝缘高温压力 (90℃,4h)",null,600,null,"2×0.75"]
["电线电缆检测中心",13,"高温压力试验","护套高温压力（90℃，4h）",null,600,null,"2×0.75"]
["电线电缆检测中心",13,"高温压力试验","护套高温压力（温度：70℃； 时间： D≤15,4h D>15,6h）",null,600,null,"2×1.5"]
["电线电缆检测中心",13,"高温压力试验","绝缘高温压力(70℃,4h)",null,600,null,"2×1.5"]
["电线电缆检测中心",13,"高温压力试验","绝缘高温压力试验（90℃；4h）",null,600,null,"1×0.08"]
["电线电缆检测中心",13,"高温压力试验","绝缘高温压力试验（80℃；4h）",null,600,null,"1×0.08"]
["电线电缆检测中心",13,"高温压力试验","绝缘高温压力试验（90℃；4h）",null,600,null,"2×0.08"]
["电线电缆检测中心",13,"高温压力试验","绝缘高温压力试验（70℃；4h）",null,600,null,"2×0.08"]
["电线电缆检测中心",14,"高温压力试验","绝缘高温压力(80℃,4h)",null,600,null,"2×1.5"]
["电线电缆检测中心",14,"高温压力试验","护套高温压力（温度：80℃； 时间： D≤15,4h D>15,6h）",null,600,null,"2×1.5"]
["电线电缆检测中心",14,"高温压力试验","绝缘高温压力(70℃,4h)",null,600,null,"2×0.75"]
["电线电缆检测中心",14,"高温压力试验","护套高温压力（70℃，4h）",null,600,null,"2×0.75"]
["电线电缆检测中心",14,"高温压力试验","绝缘高温压力试验（80℃；4h）",null,600,null,"2×0.12"]
["电线电缆检测中心",15,"高温压力试验","绝缘高温压力 (80℃,4h)",null,600,null,"2×0.08"]
["电线电缆检测中心",15,"高温压力试验","护套高温压力(80℃,4h)",null,600,null,"2×0.08"]
["电线电缆检测中心",15,"高温压力试验","绝缘高温压力(70℃,4h)",null,600,null,"2×0.08"]
["电线电缆检测中心",15,"高温压力试验","护套高温压力（温度：70℃； 时间： D≤15,4h D>15,6h）",null,600,null,"2×0.08"]
["电线电缆检测中心",16,"高温压力试验","绝缘高温压力(70℃,4h)",null,600,null,"2×2×0.12"]
["电线电缆检测中心",16,"高温压力试验","护套高温压力（温度：70℃； 时间： D≤15,4h D>15,6h）",null,600,null,"2×2×0.12"]
["电线电缆检测中心",18,"高温压力试验","压痕中间值/护套平均厚度",null,600,null,"3×300+1×150"]
["电线电缆检测中心",19,"高温压力试验","压痕中间值/护套平均厚度",null,600,null,"GB/T 33594-2017"]
["电线电缆检测中心",13,"高温压力试验 ","压痕中间值/绝缘平均厚度",null,600,null,"3×16"]
["电线电缆检测中心",14,"高温压力试验 ","压痕中间值/绝缘平均厚度",null,600,null,"3×300+1×150"]
["电线电缆检测中心",14,"高温压力试验 ","压痕中间值/绝缘平均厚度",null,600,null,"VLHV22"]
["电线电缆检测中心",15,"高温压力试验 ","压痕中间值/绝缘平均厚度",null,600,null,"3×300+1×150"]
["电线电缆检测中心",16,"高温压力试验 ","压痕中间值/绝缘平均厚度",null,600,null,"VLHVS2"]
["电线电缆检测中心",9,"高温压力试验（70℃；4h）",null,null,600,null,"2×1.5"]
["电线电缆检测中心",12,"高温压力试验（70℃；4h）",null,null,600,null,"1×0.5"]
["电线电缆检测中心",10,"高温压力试验（80℃；4h）",null,null,600,null,"1×1.5"]
["电线电缆检测中心",10,"高温压力试验（80℃；4h）",null,null,600,null,"1×0.5"]
["电线电缆检测中心",20,"高温压力试验（90℃，6h）","压痕中间值/护套平均厚度",null,600,null,"3×400"]
["电线电缆检测中心",21,"高温压力试验（90℃，6h）","压痕中间值/护套平均厚度",null,600,null,"YJLHVS2"]
["电线电缆检测中心",24,"高温压力试验（90℃，6h）","压痕中间值/护套平均厚度",null,600,null,"3×400"]
["电线电缆检测中心",24,"高温压力试验（90℃，6h）","压痕中间值/护套平均厚度",null,600,null,"YJLHV22"]
["电线电缆检测中心",25,"高温压力试验（90℃，6h）","压痕中间值/护套平均厚度",null,600,null,"YJLHVS2"]
["电线电缆检测中心",25,"高温压力试验（90℃，6h）","压痕中间值/护套平均厚度",null,600,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",26,"高温压力试验（90℃，6h）","压痕中间值/护套平均厚度",null,600,null,"3×400"]
["电线电缆检测中心",10,"高温压力试验（90℃；4h）",null,null,600,null,"1×0.5"]
["电线电缆检测中心",16,"高温压力试验-压痕中间值/护套平均厚度",null,null,600,null,"3×300+1×150"]
["电线电缆检测中心",18,"高温压力试验-压痕中间值/护套平均厚度",null,null,600,null,"3×300+1×150"]
["电线电缆检测中心",18,"高温压力试验-压痕中间值/护套平均厚度",null,null,600,null,"YJY22"]
["电线电缆检测中心",18,"高温压力试验-压痕中间值/护套平均厚度",null,null,600,null,"YJLHV22"]
["电线电缆检测中心",18,"高温压力试验-压痕中间值/护套平均厚度",null,null,600,null,"YJLHVS2"]
["电线电缆检测中心",8,"隔离套最薄处厚度(mm)",null,null,110,null,"YJV22-8.7/10"]
["电线电缆检测中心",8,"隔离套最薄处厚度(mm)",null,null,110,null,"3×400"]
["电线电缆检测中心",8,"隔离套最薄处厚度(mm)",null,null,110,null,"YJV22-26/35"]
["电线电缆检测中心",8,"隔离套最薄处厚度(mm)",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",8,"隔离套最薄处厚度(mm)",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",9,"隔离套最薄处厚度(mm)",null,null,110,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",12,"隔离套最薄处厚度(mm)",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",1,"工作电容",null,null,2800,null,"预支分支电缆"]
["电线电缆检测中心",3,"工作电容",null,null,2800,null,"各种单项试验"]
["电线电缆检测中心",26,"刮磨试验",null,null,2000,null,"3×400"]
["电线电缆检测中心",30,"刮磨试验",null,null,2000,null,"3×400"]
["电线电缆检测中心",31,"刮磨试验",null,null,2000,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",6,"光缆曲挠试验（100万次往复运动）",null,null,23450,null,"各种单项试验"]
["电线电缆检测中心",9,"过热试验","(温度: 105 ℃  时间: 48 h  室温  卷绕 芯轴直径: 30 mm  负荷:   30 kg  卷绕速度: 0.2 r/s  卷绕   圈数: 4） 卷绕后",null,720,null,"50黑"]
["电线电缆检测中心",13,"护套高温压力试验 ","压痕中间值/护套平均厚度",null,600,null,"3×300+1×150"]
["电线电缆检测中心",18,"护套高温压力试验 ","压痕中间值/护套平均厚度",null,600,null,"3×16"]
["电线电缆检测中心",19,"护套高温压力试验 ","压痕中间值/护套平均厚度",null,600,null,"3×300+1×150"]
["电线电缆检测中心",1,"护套机械物理性能","老化前拉力试验",null,250,null,"708.1-2015电力电缆"]
["电线电缆检测中心",1,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"708.1-2015电力电缆"]
["电线电缆检测中心",1,"护套机械物理性能","失重试验(100℃,7d)",null,600,null,"708.1-2015电力电缆"]
["电线电缆检测中心",1,"护套机械物理性能","高温压力 (温度：90℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,"护套为（S,S90,U）时做","708.1-2015电力电缆"]
["电线电缆检测中心",1,"护套机械物理性能","抗开裂试验 (150℃,1h)",null,400,null,"708.1-2015电力电缆"]
["电线电缆检测中心",1,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,"外径≤12.5时做","708.1-2015电力电缆"]
["电线电缆检测中心",1,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,"外径＞12.5时做","708.1-2015电力电缆"]
["电线电缆检测中心",13,"护套机械物理性能","老化前拉力试验",null,250,null,"KVV"]
["电线电缆检测中心",13,"护套机械物理性能","老化前拉力试验",null,250,null,"KVVR"]
["电线电缆检测中心",13,"护套机械物理性能","老化前拉力试验",null,250,null,"KYJV"]
["电线电缆检测中心",14,"护套机械物理性能","老化前拉力试验",null,250,null,"KVV22"]
["电线电缆检测中心",14,"护套机械物理性能","老化前拉力试验",null,250,null,"KYJV22"]
["电线电缆检测中心",14,"护套机械物理性能","老化前抗张强度",null,250,null,"YJV-8.7/10"]
["电线电缆检测中心",14,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJV-8.7/10"]
["电线电缆检测中心",14,"护套机械物理性能","老化前抗张强度",null,250,null,"YJV-26/35"]
["电线电缆检测中心",14,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJV-26/35"]
["电线电缆检测中心",15,"护套机械物理性能","老化前拉力试验",null,250,null,"2×0.5"]
["电线电缆检测中心",15,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.5"]
["电线电缆检测中心",15,"护套机械物理性能","失重试验(80℃,7d)",null,600,null,"2×0.5"]
["电线电缆检测中心",15,"护套机械物理性能","高温压力 (温度：70℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"2×0.5"]
["电线电缆检测中心",15,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"2×0.5"]
["电线电缆检测中心",15,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",15,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"2×0.5"]
["电线电缆检测中心",15,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",15,"护套机械物理性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","失重试验(80℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","高温压力 (温度：80℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","老化前拉力试验",null,250,null,"KVVP"]
["电线电缆检测中心",15,"护套机械物理性能","老化前拉力试验",null,250,null,"KVVP2-22"]
["电线电缆检测中心",15,"护套机械物理性能","老化前拉力试验",null,250,null,"KVVRP"]
["电线电缆检测中心",15,"护套机械物理性能","失重试验(100℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","高温压力 (温度：90℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"2×0.75"]
["电线电缆检测中心",15,"护套机械物理性能","老化前拉力试验",null,250,null,"KYJVP"]
["电线电缆检测中心",15,"护套机械物理性能","老化前拉力试验",null,250,null,"KYJVP2-22"]
["电线电缆检测中心",15,"护套机械物理性能","老化前拉力试验",null,250,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",15,"护套机械物理性能","老化前拉力试验",null,250,null,"KVV"]
["电线电缆检测中心",16,"护套机械物理性能","老化前拉力试验",null,250,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","失重试验(80℃,7d)",null,600,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","高温压力 (温度：80℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","失重试验(100℃,7d)",null,600,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","高温压力 (温度：90℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"4×0.75"]
["电线电缆检测中心",16,"护套机械物理性能","抗开裂试验 (150℃,1h)",null,400,null,"4×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","失重试验(80℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","高温压力 (温度：80℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","老化前拉力试验",null,250,null,"2×0.5"]
["电线电缆检测中心",17,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.5"]
["电线电缆检测中心",17,"护套机械物理性能","失重试验(80℃,7d)",null,600,null,"2×0.5"]
["电线电缆检测中心",17,"护套机械物理性能","高温压力 (温度：70℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"2×0.5"]
["电线电缆检测中心",17,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"2×0.5"]
["电线电缆检测中心",17,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",17,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"2×0.5"]
["电线电缆检测中心",17,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",17,"护套机械物理性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","失重试验(100℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","高温压力 (温度：90℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",17,"护套机械物理性能","老化前抗张强度",null,250,null,"YJLHV22常规"]
["电线电缆检测中心",17,"护套机械物理性能","老化前抗张强度",null,250,null,"YJLHS2常规"]
["电线电缆检测中心",17,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJLHS2常规"]
["电线电缆检测中心",17,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJLHV22常规"]
["电线电缆检测中心",17,"护套机械物理性能","老化前抗张强度",null,250,null,"YJLHVS2常规"]
["电线电缆检测中心",17,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJLHVS2常规"]
["电线电缆检测中心",18,"护套机械物理性能","老化前拉力试验",null,250,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","失重试验(80℃,7d)",null,600,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","高温压力 (温度：80℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","老化前拉力试验",null,250,null,"4×2.5"]
["电线电缆检测中心",18,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"4×2.5"]
["电线电缆检测中心",18,"护套机械物理性能","失重试验(100℃,7d)",null,600,null,"4×2.5"]
["电线电缆检测中心",18,"护套机械物理性能","高温压力 (温度：90℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"4×2.5"]
["电线电缆检测中心",18,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"4×2.5"]
["电线电缆检测中心",18,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"4×2.5"]
["电线电缆检测中心",18,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"4×2.5"]
["电线电缆检测中心",18,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"4×2.5"]
["电线电缆检测中心",18,"护套机械物理性能","失重试验(100℃,7d)",null,600,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","高温压力 (温度：90℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"4×4"]
["电线电缆检测中心",18,"护套机械物理性能","老化前断裂伸长率",null,250,null,"3×400"]
["电线电缆检测中心",18,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×400"]
["电线电缆检测中心",18,"护套机械物理性能","附加段老化试验(100℃,7d)",null,450,null,"3×400"]
["电线电缆检测中心",18,"护套机械物理性能","附加段老化试验(100℃,7d)",null,900,null,"3×400"]
["电线电缆检测中心",18,"护套机械物理性能","老化前抗张强度",null,250,null,"3×400"]
["电线电缆检测中心",18,"护套机械物理性能","老化前抗张强度",null,250,null,"YJV22-8.7/10"]
["电线电缆检测中心",18,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJV22-8.7/10"]
["电线电缆检测中心",18,"护套机械物理性能","老化前抗张强度",null,250,null,"YJV22-26/35"]
["电线电缆检测中心",18,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJV22-26/35"]
["电线电缆检测中心",18,"护套机械物理性能","老化前拉力试验",null,250,null,"TICW计算机"]
["电线电缆检测中心",18,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"TICW计算机"]
["电线电缆检测中心",18,"护套机械物理性能","高温压力 (温度：80℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"TICW计算机"]
["电线电缆检测中心",18,"护套机械物理性能","热冲击(150℃,1h)",null,400,null,"TICW计算机"]
["电线电缆检测中心",18,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"TICW计算机"]
["电线电缆检测中心",18,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"TICW计算机"]
["电线电缆检测中心",18,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"TICW计算机"]
["电线电缆检测中心",19,"护套机械物理性能","老化前拉力试验",null,250,null,"4×1.5"]
["电线电缆检测中心",19,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"4×1.5"]
["电线电缆检测中心",19,"护套机械物理性能","失重试验(80℃,7d)",null,600,null,"4×1.5"]
["电线电缆检测中心",19,"护套机械物理性能","高温压力 (温度：80℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"4×1.5"]
["电线电缆检测中心",19,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"4×1.5"]
["电线电缆检测中心",19,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"4×1.5"]
["电线电缆检测中心",19,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"4×1.5"]
["电线电缆检测中心",19,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"4×1.5"]
["电线电缆检测中心",19,"护套机械物理性能","老化前拉力试验",null,250,null,"4×2.5"]
["电线电缆检测中心",19,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"4×2.5"]
["电线电缆检测中心",19,"护套机械物理性能","失重试验(100℃,7d)",null,600,null,"4×2.5"]
["电线电缆检测中心",19,"护套机械物理性能","高温压力 (温度：90℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,null,"4×2.5"]
["电线电缆检测中心",19,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"4×2.5"]
["电线电缆检测中心",19,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"4×2.5"]
["电线电缆检测中心",19,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"4×2.5"]
["电线电缆检测中心",19,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"4×2.5"]
["电线电缆检测中心",19,"护套机械物理性能","老化前拉力试验",null,250,null,"48×1"]
["电线电缆检测中心",19,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"48×1"]
["电线电缆检测中心",19,"护套机械物理性能","失重试验(100℃,7d)",null,600,null,"48×1"]
["电线电缆检测中心",19,"护套机械物理性能","高温压力 (温度：80℃, 时间：外径D≤12.5mm，4h 外径D＞12.5mm，6h) -压痕中间值/护套平均厚度",null,600,null,"48×1"]
["电线电缆检测中心",19,"护套机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"48×1"]
["电线电缆检测中心",19,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"48×1"]
["电线电缆检测中心",19,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"48×1"]
["电线电缆检测中心",19,"护套机械物理性能","低温冲击试验 （-15℃）",null,400,null,"48×1"]
["电线电缆检测中心",19,"护套机械物理性能","老化前抗张强度",null,250,null,"YJLHVS2"]
["电线电缆检测中心",19,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJLHVS2"]
["电线电缆检测中心",19,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"YJLHVS2"]
["电线电缆检测中心",19,"护套机械物理性能","附加段老化试验(100℃,7d)",null,450,null,"YJLHVS2"]
["电线电缆检测中心",22,"护套机械物理性能","老化前抗张强度",null,250,null,"3×400"]
["电线电缆检测中心",22,"护套机械物理性能","老化前断裂伸长率",null,250,null,"3×400"]
["电线电缆检测中心",22,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×400"]
["电线电缆检测中心",22,"护套机械物理性能","附加段老化试验(100℃,7d)",null,450,null,"3×400"]
["电线电缆检测中心",22,"护套机械物理性能","老化前抗张强度",null,250,null,"YJLHV22"]
["电线电缆检测中心",22,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJLHV22"]
["电线电缆检测中心",22,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"YJLHV22"]
["电线电缆检测中心",22,"护套机械物理性能","附加段老化试验(100℃,7d)",null,450,null,"YJLHV22"]
["电线电缆检测中心",23,"护套机械物理性能","老化前抗张强度",null,250,null,"YJLHVS2"]
["电线电缆检测中心",23,"护套机械物理性能","老化前断裂伸长率",null,250,null,"YJLHVS2"]
["电线电缆检测中心",23,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"YJLHVS2"]
["电线电缆检测中心",23,"护套机械物理性能","附加段老化试验(100℃,7d)",null,450,null,"YJLHVS2"]
["电线电缆检测中心",23,"护套机械物理性能","老化前抗张强度",null,250,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",23,"护套机械物理性能","老化前断裂伸长率",null,250,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",23,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",23,"护套机械物理性能","附加段老化试验(100℃,7d)",null,450,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",24,"护套机械物理性能","老化前抗张强度",null,250,null,"3×400"]
["电线电缆检测中心",24,"护套机械物理性能","老化前断裂伸长率",null,250,null,"3×400"]
["电线电缆检测中心",24,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×400"]
["电线电缆检测中心",24,"护套机械物理性能","附加段老化试验(100℃,7d)",null,450,null,"3×400"]
["电线电缆检测中心",29,"护套机械物理性能","人工气候老化试验 （0ｈ～1008ｈ）",null,2625,null,"充电桩电缆"]
["电线电缆检测中心",29,"护套机械物理性能","人工气候老化试验 （504ｈ～1008ｈ）",null,2625,null,"充电桩电缆"]
["电线电缆检测中心",29,"护套机械物理性能","老化前拉力试验",null,250,null,"充电桩电缆"]
["电线电缆检测中心",29,"护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"充电桩电缆"]
["电线电缆检测中心",29,"护套机械物理性能","高温压力 (温度：90℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,"护套为（S,S90,U）时做","充电桩电缆"]
["电线电缆检测中心",29,"护套机械物理性能","抗开裂试验 (150℃,1h)",null,400,null,"充电桩电缆"]
["电线电缆检测中心",29,"护套机械物理性能","低温弯曲试验 （-15℃）",null,400,"外径≤12.5时做","充电桩电缆"]
["电线电缆检测中心",29,"护套机械物理性能","低温拉伸试验 (-15℃)",null,400,"外径＞12.5时做","充电桩电缆"]
["电线电缆检测中心",10,"护套机械性能","老化前拉力试验",null,250,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",10,"护套机械性能","老化前拉力试验",null,250,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",10,"护套机械性能","老化前拉力试验",null,250,null,"BVVB 300/500V"]
["电线电缆检测中心",10,"护套机械性能","老化前拉力试验",null,250,null,"RVV 300/500V"]
["电线电缆检测中心",10,"护套机械性能","老化前拉力试验",null,250,null,"YC 450/750V"]
["电线电缆检测中心",11,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",11,"护套机械性能","失重试验(80℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"1×0.75"]
["电线电缆检测中心",11,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"1×0.75"]
["电线电缆检测中心",11,"护套机械性能","失重试验(80℃,7d)",null,600,null,"1×0.75"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"1×1"]
["电线电缆检测中心",11,"护套机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"1×1"]
["电线电缆检测中心",11,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"1×1"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"2×0.3"]
["电线电缆检测中心",11,"护套机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"2×0.3"]
["电线电缆检测中心",11,"护套机械性能","浸矿物油后拉力试验（100℃,24h）",null,900,null,"2×0.3"]
["电线电缆检测中心",11,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×0.3"]
["电线电缆检测中心",11,"护套机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"2×0.75"]
["电线电缆检测中心",11,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×0.75"]
["电线电缆检测中心",11,"护套机械性能","热延伸试验(200℃,15min，0.3N/mm²)",null,410,null,"2×0.75"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",11,"护套机械性能","浸矿物油后拉力试验（100℃,24h）",null,900,null,"2×0.75"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"2×4"]
["电线电缆检测中心",11,"护套机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"2×4"]
["电线电缆检测中心",11,"护套机械性能","浸矿物油后拉力试验（100℃,24h）",null,900,null,"2×4"]
["电线电缆检测中心",11,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×4"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"VV"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"YJV"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"BVVB,BLVVB"]
["电线电缆检测中心",11,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"BVVB,BLVVB"]
["电线电缆检测中心",11,"护套机械性能","失重试验(80℃,7d)",null,600,null,"BVVB,BLVVB"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"RVV"]
["电线电缆检测中心",11,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"RVV"]
["电线电缆检测中心",11,"护套机械性能","失重试验(80℃,7d)",null,600,null,"RVV"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"YC"]
["电线电缆检测中心",11,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"YC"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"YZ"]
["电线电缆检测中心",11,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"YZ"]
["电线电缆检测中心",11,"护套机械性能","老化前拉力试验",null,250,null,"YJLHVS2常规"]
["电线电缆检测中心",12,"护套机械性能","老化前拉力试验",null,250,null,"2×1.5"]
["电线电缆检测中心",12,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×1.5"]
["电线电缆检测中心",12,"护套机械性能","失重试验(80℃,7d)",null,600,null,"2×1.5"]
["电线电缆检测中心",12,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.5"]
["电线电缆检测中心",12,"护套机械性能","失重试验(80℃,7d)",null,600,null,"2×0.5"]
["电线电缆检测中心",12,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",12,"护套机械性能","失重试验(80℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",12,"护套机械性能","老化前拉力试验",null,250,null,"2×0.5"]
["电线电缆检测中心",12,"护套机械性能","老化后拉力试验(135℃,10d)",null,450,null,"2×0.5"]
["电线电缆检测中心",12,"护套机械性能","失重试验(115℃,10d)",null,600,null,"2×0.5"]
["电线电缆检测中心",12,"护套机械性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",12,"护套机械性能","老化后拉力试验(135℃,10d)",null,450,null,"2×0.75"]
["电线电缆检测中心",12,"护套机械性能","失重试验(115℃,10d)",null,600,null,"2×0.75"]
["电线电缆检测中心",12,"护套机械性能","老化前拉力试验",null,250,null,"RVVP 300/300V"]
["电线电缆检测中心",12,"护套机械性能","老化前拉力试验",null,250,null,"VV22"]
["电线电缆检测中心",12,"护套机械性能","老化前拉力试验",null,250,null,"VLHVS2"]
["电线电缆检测中心",12,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"VLHVS2"]
["电线电缆检测中心",12,"护套机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"VLHVS2"]
["电线电缆检测中心",13,"护套机械性能","老化前拉力试验",null,250,null,"2×1.5"]
["电线电缆检测中心",13,"护套机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"2×1.5"]
["电线电缆检测中心",13,"护套机械性能","浸矿物油后拉力试验（100℃,24h）",null,900,null,"2×1.5"]
["电线电缆检测中心",13,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm² )",null,410,null,"2×1.5"]
["电线电缆检测中心",13,"护套机械性能","老化前拉力试验",null,250,null,"6×1"]
["电线电缆检测中心",13,"护套机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"6×1"]
["电线电缆检测中心",13,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"6×1"]
["电线电缆检测中心",13,"护套机械性能","浸矿物油后拉力试验（100℃,24h）",null,900,null,"6×1"]
["电线电缆检测中心",13,"护套机械性能","浸矿物油后拉力试验（100℃,25h）",null,900,null,"6×1"]
["电线电缆检测中心",13,"护套机械性能","老化前拉力试验",null,250,null,"WDZAN-YJY23"]
["电线电缆检测中心",13,"护套机械性能","老化前拉力试验",null,250,null,"YJV22"]
["电线电缆检测中心",13,"护套机械性能","老化前拉力试验",null,250,null,"YJV32"]
["电线电缆检测中心",13,"护套机械性能","老化前拉力试验",null,250,null,"YJY22"]
["电线电缆检测中心",13,"护套机械性能","老化前拉力试验",null,250,null,"AVVR"]
["电线电缆检测中心",13,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"AVVR"]
["电线电缆检测中心",13,"护套机械性能","失重试验(80℃,7d)",null,600,null,"AVVR"]
["电线电缆检测中心",13,"护套机械性能","老化前拉力试验",null,250,null,"RVVP"]
["电线电缆检测中心",13,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"RVVP"]
["电线电缆检测中心",13,"护套机械性能","失重试验(80℃,7d)",null,600,null,"RVVP"]
["电线电缆检测中心",14,"护套机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"2×0.75"]
["电线电缆检测中心",14,"护套机械性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",14,"护套机械性能","浸矿物油后拉力试验（100℃,24h）",null,900,null,"2×0.75"]
["电线电缆检测中心",14,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm² )",null,410,null,"2×0.75"]
["电线电缆检测中心",14,"护套机械性能","老化前拉力试验",null,250,null,"1×1.5"]
["电线电缆检测中心",14,"护套机械性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"1×1.5"]
["电线电缆检测中心",14,"护套机械性能","浸矿物油后拉力试验（100℃,24h）",null,900,null,"1×1.5"]
["电线电缆检测中心",14,"护套机械性能","热延伸试验(200℃,15min，0.2N/mm² )",null,410,null,"1×1.5"]
["电线电缆检测中心",14,"护套机械性能","老化前拉力试验",null,250,null,"2×0.08"]
["电线电缆检测中心",14,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.08"]
["电线电缆检测中心",14,"护套机械性能","失重试验(80℃,7d)",null,600,null,"2×0.08"]
["电线电缆检测中心",14,"护套机械性能","老化前拉力试验",null,250,null,"3×300+1×150"]
["电线电缆检测中心",14,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×300+1×150"]
["电线电缆检测中心",14,"护套机械性能","成品电缆段的附加老化试验(100℃,7d)",null,900,null,"3×300+1×150"]
["电线电缆检测中心",14,"护套机械性能","老化前拉力试验",null,250,null,"YJV,YJLV"]
["电线电缆检测中心",15,"护套机械性能","老化前拉力试验",null,250,null,"2×2×0.12"]
["电线电缆检测中心",15,"护套机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×2×0.12"]
["电线电缆检测中心",15,"护套机械性能","失重试验(80℃,7d)",null,600,null,"2×2×0.12"]
["电线电缆检测中心",15,"护套机械性能","老化前拉力试验",null,250,null,"3×300+1×150"]
["电线电缆检测中心",15,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×300+1×150"]
["电线电缆检测中心",15,"护套机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"3×300+1×150"]
["电线电缆检测中心",15,"护套机械性能","老化前拉力试验",null,250,null,"3×16"]
["电线电缆检测中心",15,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×16"]
["电线电缆检测中心",15,"护套机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"3×16"]
["电线电缆检测中心",15,"护套机械性能","老化前拉力试验",null,250,null,"VV,VLV"]
["电线电缆检测中心",15,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"VV,VLV"]
["电线电缆检测中心",16,"护套机械性能","老化前拉力试验",null,250,null,"3×300+1×150"]
["电线电缆检测中心",16,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×300+1×150"]
["电线电缆检测中心",16,"护套机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"3×300+1×150"]
["电线电缆检测中心",16,"护套机械性能","成品电缆段的附加老化试验(100℃,7d)",null,900,null,"3×300+1×150"]
["电线电缆检测中心",16,"护套机械性能","老化前拉力试验",null,250,null,"YJY22"]
["电线电缆检测中心",16,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"YJY22"]
["电线电缆检测中心",16,"护套机械性能","成品电缆段的附加老化试验(100℃,7d)",null,900,null,"YJY22"]
["电线电缆检测中心",16,"护套机械性能","老化前拉力试验",null,250,null,"VLHV22"]
["电线电缆检测中心",16,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"VLHV22"]
["电线电缆检测中心",16,"护套机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"VLHV22"]
["电线电缆检测中心",16,"护套机械性能","老化前拉力试验",null,250,null,"YJLHV22"]
["电线电缆检测中心",16,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"YJLHV22"]
["电线电缆检测中心",16,"护套机械性能","成品电缆段的附加老化试验(100℃,7d)",null,900,null,"YJLHV22"]
["电线电缆检测中心",16,"护套机械性能","老化前拉力试验",null,250,null,"YJLHVS2"]
["电线电缆检测中心",16,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"YJLHVS2"]
["电线电缆检测中心",16,"护套机械性能","成品电缆段的附加老化试验(100℃,7d)",null,900,null,"YJLHVS2"]
["电线电缆检测中心",17,"护套机械性能","老化前拉力试验",null,250,null,"VLHV22常规"]
["电线电缆检测中心",17,"护套机械性能","老化前拉力试验",null,250,null,"GB/T 33594-2017"]
["电线电缆检测中心",17,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"GB/T 33594-2017"]
["电线电缆检测中心",17,"护套机械性能","成品电缆段的附加老化试验(100℃,7d)",null,900,null,"GB/T 33594-2017"]
["电线电缆检测中心",18,"护套机械性能","老化前拉力试验",null,250,null,"YJY"]
["电线电缆检测中心",18,"护套机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"YJY"]
["电线电缆检测中心",18,"护套机械性能","老化前拉力试验",null,250,null,"YJLHV22常规"]
["电线电缆检测中心",43,"护套耐臭氧试验（25℃，24h，臭氧浓度0.025～0.030%）",null,null,500,"护套为（F,U，YJ）时做","充电桩电缆"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"1×0.75"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"BVVB 300/500V"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"RVV 300/500V"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"2×2×0.12"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"RVVP 300/300V"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"1×1"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"2×0.3"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"2×0.75"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"2×4"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"YC 450/750V"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"3×0.3"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"KVV"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"KVVR"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"KYJV"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"KYJV22"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"KYJVP2-22"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"YJV"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"BVVB,BLVVB"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"RVV"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"RVVP"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"YC"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"YJV,YJLV"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"YZ"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"YJLHVS2常规"]
["电线电缆检测中心",5,"护套平均厚度",null,null,110,null,"QC/T1037-2016"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"2×0.75"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"2×1.5"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"1×1.5"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"6×1"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"4×0.75"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"2×0.5"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"KVV22"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"KYJVP"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"3×16"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"VV"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"AVVR"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"VV,VLV"]
["电线电缆检测中心",6,"护套平均厚度",null,null,110,null,"TICW计算机"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"2×0.08"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"KVVP"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"KVVP2-22"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"KVVRP"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"2×0.75"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"YJY22"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"VV22"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"WDZAN-YJY23"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"YJV22"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"YJV32"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"VLHV22"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"VLHVS2"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",7,"护套平均厚度",null,null,110,null,"充电桩电缆"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"4×4"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"4×2.5"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"48×1"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"3×400"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"YJV-8.7/10"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"YJV-26/35"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"VLHV22常规"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"VLHVS2常规"]
["电线电缆检测中心",8,"护套平均厚度",null,null,110,null,"GB/T 33594-2017"]
["电线电缆检测中心",9,"护套平均厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",9,"护套平均厚度",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",9,"护套平均厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",11,"护套平均厚度",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",11,"护套平均厚度",null,null,110,null,"YJLHS2常规"]
["电线电缆检测中心",11,"护套平均厚度",null,null,110,null,"YJLHVS2常规"]
["电线电缆检测中心",12,"护套平均厚度",null,null,110,null,"3×400"]
["电线电缆检测中心",12,"护套平均厚度",null,null,110,null,"YJV22-8.7/10"]
["电线电缆检测中心",12,"护套平均厚度",null,null,110,null,"YJV22-26/35"]
["电线电缆检测中心",12,"护套平均厚度",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",13,"护套平均厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",13,"护套平均厚度",null,null,110,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",11,"护套平均厚度Temp1855793558637611602565050850",null,null,110,null,"YJY"]
["电线电缆检测中心",18,"护套热冲击试验(150℃,1h)",null,null,400,null,"VV,VLV"]
["电线电缆检测中心",15,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",17,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",18,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",19,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×16"]
["电线电缆检测中心",19,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"VLHV22"]
["电线电缆检测中心",20,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",20,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"VLHVS2"]
["电线电缆检测中心",23,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",23,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"YJLHV22"]
["电线电缆检测中心",23,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"YJLHVS2"]
["电线电缆检测中心",26,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×400"]
["电线电缆检测中心",27,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×400"]
["电线电缆检测中心",27,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"YJLHVS2"]
["电线电缆检测中心",30,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×400"]
["电线电缆检测中心",30,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"YJLHV22"]
["电线电缆检测中心",31,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×400"]
["电线电缆检测中心",31,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"YJLHVS2"]
["电线电缆检测中心",32,"护套热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×400"]
["电线电缆检测中心",2,"护套热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,"护套为（F,YJ）时做","708.1-2015电力电缆"]
["电线电缆检测中心",42,"护套热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,"护套为（F,YJ）时做","充电桩电缆"]
["电线电缆检测中心",42,"护套热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,"护套为（F,YJ）时做","充电桩电缆"]
["电线电缆检测中心",2,"护套收缩试验",null,null,600,null,"GB/T12706-2020护套收缩"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,100,null,"2×0.75"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"1×0.75"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"BVVB 300/500V"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"RVV 300/500V"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"2×2×0.12"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"RVVP 300/300V"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"1×1"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"2×0.3"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"2×4"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"YC 450/750V"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"3×0.3"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"KVV"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"KVVR"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"KYJV"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"KYJV22"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"KYJVP2-22"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"YJV"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,100,null,"BVVB,BLVVB"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"RVV"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"RVVP"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"YC"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"YJV,YJLV"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"YZ"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"YJLHVS2常规"]
["电线电缆检测中心",6,"护套最薄处厚度",null,null,110,null,"QC/T1037-2016"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"2×0.75"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"1×1.5"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"6×1"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"2×0.5"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"2×1.5"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"YCW"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"4×0.75"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"KVV22"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"3×16"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"VV"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"AVVR"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"VV,VLV"]
["电线电缆检测中心",7,"护套最薄处厚度",null,null,110,null,"TICW计算机"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"2×0.08"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"2×35"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"KVVP"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"KVVP2-22"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"KVVRP"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"KYJVP"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"YJY22"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"VV22"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"WDZAN-YJY23"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"YJV22"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"YJV32"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"VLHV22"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"VLHVS2"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",8,"护套最薄处厚度",null,null,110,null,"充电桩电缆"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"4×4"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"4×2.5"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"2×0.75"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"48×1"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"3×400"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"YJV-8.7/10"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"YJV-26/35"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"VLHV22常规"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"VLHVS2常规"]
["电线电缆检测中心",9,"护套最薄处厚度",null,null,110,null,"GB/T 33594-2017"]
["电线电缆检测中心",10,"护套最薄处厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",10,"护套最薄处厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",11,"护套最薄处厚度",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",12,"护套最薄处厚度",null,null,110,null,"YJLHS2常规"]
["电线电缆检测中心",12,"护套最薄处厚度",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",12,"护套最薄处厚度",null,null,110,null,"YJLHVS2常规"]
["电线电缆检测中心",13,"护套最薄处厚度",null,null,110,null,"3×400"]
["电线电缆检测中心",13,"护套最薄处厚度",null,null,110,null,"YJV22-8.7/10"]
["电线电缆检测中心",13,"护套最薄处厚度",null,null,110,null,"YJV22-26/35"]
["电线电缆检测中心",13,"护套最薄处厚度",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",14,"护套最薄处厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",14,"护套最薄处厚度",null,null,110,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",12,"护套最薄处厚度Temp1017481484637611602565651302",null,null,110,null,"YJY"]
["电线电缆检测中心",4,"护套最大厚度",null,null,110,null,"各种单项试验"]
["电线电缆检测中心",4,"化学性能","耐溶剂性 （标准溶剂温度60±3℃，铅笔硬度：H）",null,220,null,"全部参数"]
["电线电缆检测中心",4,"化学性能","耐冷冻剂 —萃取物  (%)（耐一氯二氟甲烷R22）",null,3000,null,"全部参数"]
["电线电缆检测中心",4,"化学性能","直焊性 (试验温度:（390±5）℃  试验时间：6s)",null,380,null,"全部参数"]
["电线电缆检测中心",7,"机械特性","绝缘拉伸试验  ",null,250,null,"1.25 黑白"]
["电线电缆检测中心",7,"机械特性","绝缘拉伸试验  ",null,1250,null,"1.25 黑白"]
["电线电缆检测中心",7,"机械特性","加热变形性（80 ℃ 4 h） 加热变形后, 耐电压试验 （1 kV  1 min）",null,200,null,"1.25 黑白"]
["电线电缆检测中心",7,"机械特性","耐绝缘体牵引和拉延",null,250,null,1]
["电线电缆检测中心",7,"机械特性","高温压力（131 ℃ ， 4 h） 高温压力后，介电硬度试验 （1 kV ，30 min）",null,600,null,1]
["电线电缆检测中心",7,"机械特性","耐缠绕性 （温度: -40 ℃  时间: 4 h        芯轴直径: 10 mm  重物: 2.5 kg      缠绕速度: 1 s-1  缠绕圈数: 3） 缠绕后 抗缠绕后, 介电硬度试验 （1 kV  30 min ）",null,480,null,1]
["电线电缆检测中心",7,"机械特性","刮擦导致的磨损 （负重：7 N  刮针直径: 0.45 mm              频率: 55 次/ min  行程: 15.5 mm）",null,500,null,1]
["电线电缆检测中心",7,"机械特性","导体在导体上的磨损 （移动幅度: 6.35 mm   振动频率: 10 Hz ）",null,600,null,1]
["电线电缆检测中心",8,"机械物理性能试验","高温压力（125 ℃ ，4 h） 高温压力后，耐电压试验 （1 kV ，1 min）",null,600,null,"0.75 白"]
["电线电缆检测中心",8,"机械物理性能试验","高温压力（125 ℃ ，4 h） 高温压力后，耐电压试验 （1 kV ，1 min）",null,600,null,1]
["电线电缆检测中心",2,"机械性能","抗拉强度",null,295,null,3]
["电线电缆检测中心",3,"机械性能","抗拉强度σ ",null,250,null,6]
["电线电缆检测中心",3,"机械性能","伸长率  ",null,250,null,"全部参数"]
["电线电缆检测中心",3,"机械性能","回弹性(圆棒直径：50mm)(负    荷： 15.0N )",null,300,null,"全部参数"]
["电线电缆检测中心",3,"机械性能","柔韧性和附着性",null,250,null,"全部参数"]
["电线电缆检测中心",3,"机械性能","刮漆",null,150,null,"全部参数"]
["电线电缆检测中心",4,"机械性能","布氏硬度（HB） （球直径：5mm,试验力：2452N）",null,400,null,"铜牌陕西军工"]
["电线电缆检测中心",4,"机械性能","弯曲 (宽边弯曲90°,弯曲圆柱直径:8mm)",null,450,null,"铜牌陕西军工"]
["电线电缆检测中心",5,"机械性能","布氏硬度（HB） （球直径：5mm,试验力：2452N）",null,580,null,"全部参数"]
["电线电缆检测中心",5,"机械性能","弯曲 (宽边弯曲90°,弯曲圆柱直径:8mm)",null,580,null,"全部参数"]
["电线电缆检测中心",11,"交流电压试验（18kV,1min）",null,null,1000,null,"1×25"]
["电线电缆检测中心",12,"交流电压试验（18kV,1min）",null,null,1000,null,"1×25"]
["电线电缆检测中心",14,"交流电压试验（18kV,1min）",null,null,1000,null,"1×25"]
["电线电缆检测中心",6,"绞合方向",null,null,110,null,"6×1"]
["电线电缆检测中心",6,"绞合方向",null,null,110,null,"2×1.0"]
["电线电缆检测中心",6,"绞合方向",null,null,110,null,"RVS 300/300V"]
["电线电缆检测中心",7,"绞合方向",null,null,110,null,"2×0.08"]
["电线电缆检测中心",8,"绞合方向",null,null,110,null,"6×1"]
["电线电缆检测中心",8,"绞合方向",null,null,110,null,"2×0.12"]
["电线电缆检测中心",8,"绞合方向",null,null,110,null,"3×0.3"]
["电线电缆检测中心",8,"绞合方向",null,null,110,null,"2×0.3"]
["电线电缆检测中心",9,"绞合方向",null,null,110,null,"2×0.75"]
["电线电缆检测中心",9,"绞合方向",null,null,110,null,"1×1.5"]
["电线电缆检测中心",9,"绞合方向",null,null,110,null,"2×0.08"]
["电线电缆检测中心",9,"绞合方向",null,null,110,null,"2×2×0.12"]
["电线电缆检测中心",9,"绞合方向",null,null,110,null,"RVVP 300/300V"]
["电线电缆检测中心",9,"绞合方向",null,null,110,null,"KVV"]
["电线电缆检测中心",9,"绞合方向",null,null,110,null,"KVVR"]
["电线电缆检测中心",9,"绞合方向",null,null,110,null,"KYJV"]
["电线电缆检测中心",10,"绞合方向",null,null,110,null,"2×0.5"]
["电线电缆检测中心",10,"绞合方向",null,null,110,null,"2×0.75"]
["电线电缆检测中心",10,"绞合方向",null,null,110,null,"KVV22"]
["电线电缆检测中心",10,"绞合方向",null,null,110,null,"KYJV22"]
["电线电缆检测中心",10,"绞合方向",null,null,110,null,"充电桩电缆"]
["电线电缆检测中心",11,"绞合方向",null,null,110,null,"4×0.75"]
["电线电缆检测中心",11,"绞合方向",null,null,110,null,"KVVP"]
["电线电缆检测中心",11,"绞合方向",null,null,110,null,"KVVP2-22"]
["电线电缆检测中心",11,"绞合方向",null,null,110,null,"KVVRP"]
["电线电缆检测中心",11,"绞合方向",null,null,110,null,"KYJVP"]
["电线电缆检测中心",11,"绞合方向",null,null,110,null,"KYJVP2-22"]
["电线电缆检测中心",11,"绞合方向",null,null,110,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",12,"绞合方向",null,null,110,null,"2×0.5"]
["电线电缆检测中心",12,"绞合方向",null,null,110,null,"2×0.75"]
["电线电缆检测中心",13,"绞合方向",null,null,110,null,"4×4"]
["电线电缆检测中心",13,"绞合方向",null,null,110,null,"4×2.5"]
["电线电缆检测中心",14,"绞合方向",null,null,110,null,"4×1.5"]
["电线电缆检测中心",14,"绞合方向",null,null,110,null,"4×2.5"]
["电线电缆检测中心",14,"绞合方向",null,null,110,null,"48×1"]
["电线电缆检测中心",9,"绞合节径比","钢丝6根层节径比",null,42.5,null,"630/35-45/7"]
["电线电缆检测中心",9,"绞合节径比","铝线内层节径比",null,42.5,null,"630/35-45/7"]
["电线电缆检测中心",9,"绞合节径比",null,null,42.5,null,"630/35-45/7"]
["电线电缆检测中心",9,"绞合节径比","铝线外层节径比",null,42.5,null,"630/35-45/7"]
["电线电缆检测中心",9,"绞合节径比","铝包钢线6根层节径比",null,42.5,null,"400/35-48/7"]
["电线电缆检测中心",9,"绞合节径比","铝线内层节径比",null,42.5,null,"400/35-48/7"]
["电线电缆检测中心",9,"绞合节径比",null,null,42.5,null,"400/35-48/7"]
["电线电缆检测中心",9,"绞合节径比","铝线外层节径比",null,42.5,null,"400/35-48/7"]
["电线电缆检测中心",9,"绞合节径比","钢丝6根层节径比",null,42.5,null,"300/20-45/7"]
["电线电缆检测中心",9,"绞合节径比","铝线内层节径比",null,42.5,null,"300/20-45/7"]
["电线电缆检测中心",9,"绞合节径比",null,null,42.5,null,"300/20-45/7"]
["电线电缆检测中心",9,"绞合节径比","铝线外层节径比",null,42.5,null,"300/20-45/7"]
["电线电缆检测中心",9,"绞合节径比","钢丝6根层节径比",null,42.5,null,"185/25-24/7"]
["电线电缆检测中心",9,"绞合节径比","钢丝12根层节径比",null,42.5,null,"185/25-24/7"]
["电线电缆检测中心",9,"绞合节径比","铝合金线内层节径比",null,42.5,null,"185/25-24/7"]
["电线电缆检测中心",9,"绞合节径比",null,null,42.5,null,"185/25-24/7"]
["电线电缆检测中心",9,"绞合节径比","铝合金线外层节径比",null,42.5,null,"185/25-24/7"]
["电线电缆检测中心",10,"绞合节径比",null,null,110,null,"KVV"]
["电线电缆检测中心",10,"绞合节径比",null,null,110,null,"KVVR"]
["电线电缆检测中心",10,"绞合节径比",null,null,110,null,"KYJV"]
["电线电缆检测中心",11,"绞合节径比",null,null,110,null,"2×0.5"]
["电线电缆检测中心",11,"绞合节径比",null,null,110,null,"2×0.75"]
["电线电缆检测中心",11,"绞合节径比",null,null,110,null,"KVV22"]
["电线电缆检测中心",11,"绞合节径比",null,null,110,null,"KYJV22"]
["电线电缆检测中心",11,"绞合节径比",null,null,110,null,"充电桩电缆"]
["电线电缆检测中心",12,"绞合节径比",null,null,110,null,"4×0.75"]
["电线电缆检测中心",12,"绞合节径比",null,null,110,null,"KVVP"]
["电线电缆检测中心",12,"绞合节径比",null,null,110,null,"KVVP2-22"]
["电线电缆检测中心",12,"绞合节径比",null,null,110,null,"KVVRP"]
["电线电缆检测中心",12,"绞合节径比",null,null,110,null,"KYJVP"]
["电线电缆检测中心",12,"绞合节径比",null,null,110,null,"KYJVP2-22"]
["电线电缆检测中心",12,"绞合节径比",null,null,110,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",13,"绞合节径比",null,null,110,null,"2×0.75"]
["电线电缆检测中心",13,"绞合节径比",null,null,110,null,"2×0.5"]
["电线电缆检测中心",14,"绞合节径比",null,null,110,null,"4×4"]
["电线电缆检测中心",14,"绞合节径比",null,null,110,null,"4×2.5"]
["电线电缆检测中心",15,"绞合节径比",null,null,110,null,"4×1.5"]
["电线电缆检测中心",15,"绞合节径比",null,null,110,null,"4×2.5"]
["电线电缆检测中心",15,"绞合节径比",null,null,110,null,"48×1"]
["电线电缆检测中心",7,"绞合节距与平均外径上限之比",null,null,110,null,"6×1"]
["电线电缆检测中心",8,"绞合节距与平均外径上限之比",null,null,110,null,"2×0.08"]
["电线电缆检测中心",9,"绞合节距与平均外径上限之比",null,null,110,null,"6×1"]
["电线电缆检测中心",10,"绞合节距与平均外径上限之比",null,null,110,null,"2×0.75"]
["电线电缆检测中心",10,"绞合节距与平均外径上限之比",null,null,110,null,"1×1.5"]
["电线电缆检测中心",10,"绞合节距与平均外径上限之比",null,null,110,null,"2×0.08"]
["电线电缆检测中心",7,"绞合截距与平均外径上限之比",null,null,110,null,"2×1.0"]
["电线电缆检测中心",7,"绞合截距与平均外径上限之比",null,null,110,null,"RVS 300/300V"]
["电线电缆检测中心",9,"绞合截距与平均外径上限之比",null,null,110,null,"2×0.12"]
["电线电缆检测中心",13,"绞线20℃时的直流电阻",null,null,220,null,"630/35-45/7"]
["电线电缆检测中心",13,"绞线20℃时的直流电阻",null,null,220,null,"400/35-48/7"]
["电线电缆检测中心",13,"绞线20℃时的直流电阻",null,null,220,null,"300/20-45/7"]
["电线电缆检测中心",13,"绞线20℃时的直流电阻",null,null,220,null,"185/25-24/7"]
["电线电缆检测中心",8,"绞制","绞向",null,220,null,"630/35-45/7"]
["电线电缆检测中心",8,"绞制","紧密性",null,110,null,"630/35-45/7"]
["电线电缆检测中心",8,"绞制","绞向",null,220,null,"400/35-48/7"]
["电线电缆检测中心",8,"绞制","紧密性",null,110,null,"400/35-48/7"]
["电线电缆检测中心",8,"绞制","绞向",null,220,null,"300/20-45/7"]
["电线电缆检测中心",8,"绞制","紧密性",null,110,null,"300/20-45/7"]
["电线电缆检测中心",8,"绞制","绞向",null,220,null,"185/25-24/7"]
["电线电缆检测中心",8,"绞制","紧密性",null,110,null,"185/25-24/7"]
["电线电缆检测中心",6,"截面积","总截面积",null,80,null,"630/35-45/7"]
["电线电缆检测中心",6,"截面积","总截面积",null,80,null,"400/35-48/7"]
["电线电缆检测中心",6,"截面积","总截面积",null,80,null,"300/20-45/7"]
["电线电缆检测中心",6,"截面积","总截面积",null,80,null,"185/25-24/7"]
["电线电缆检测中心",7,"金属屏蔽",null,null,110,null,"GB/T 33594-2017"]
["电线电缆检测中心",4,"卷绕试验(1 d卷绕8圈,退6圈,再紧密卷绕)",null,580,580,null,6]
["电线电缆检测中心",13,"绝缘剥离试验 剥离20 mm 长绝缘",null,null,400,null,"50黑"]
["电线电缆检测中心",17,"绝缘剥离试验 剥离20 mm 长绝缘",null,null,400,null,"DIN 72551-5/1991"]
["电线电缆检测中心",13,"绝缘高温压力试验 ","压痕中间值/绝缘平均厚度",null,600,null,"3×300+1×150"]
["电线电缆检测中心",16,"绝缘刮磨试验 （频率: 55 次/ min  砝码质量：1250 g）",null,null,500,null,"50黑"]
["电线电缆检测中心",7,"绝缘机械物理性能","老化前拉力试验",null,250,null,"JKLYJ-1"]
["电线电缆检测中心",7,"绝缘机械物理性能","热延伸试验（200℃,15min，20N/cm²）",null,410,null,"JKLYJ-1"]
["电线电缆检测中心",7,"绝缘机械物理性能","老化前拉力试验",null,250,null,"JKLYJ-10"]
["电线电缆检测中心",10,"绝缘机械物理性能","老化前拉力试验",null,250,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","人工气候老化试验 （0ｈ～1008ｈ）",null,2625,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","人工气候老化试验 （504ｈ～1008ｈ）",null,2625,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","收缩试验 (130℃,1h) 收缩率",null,600,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","空气烘箱老化试验(80℃,7d)",null,450,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","热失重试验（80℃,7d）",null,600,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","低温卷绕试验 （－35℃）",null,400,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","低温拉伸试验 （－35℃）",null,400,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","低温冲击试验 （－35℃）",null,400,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","吸水试验 (70℃,10d) 电压法 ",null,1200,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","收缩试验 (100℃,1h) 收缩率",null,600,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","熔融指数 (熔体质量流动速率)",null,600,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","抗开裂试验（150℃,1ｈ）",null,400,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","高温压力试验 （温度80℃, 时间：外径Ｄ≤１５ｍｍ，４ｈ； 外径Ｄ＞15ｍｍ，６ｈ）",null,600,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","热延伸试验（200℃,15min，20N/cm²）",null,410,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,10d)",null,1800,null,"1×10"]
["电线电缆检测中心",10,"绝缘机械物理性能","吸水试验 (85℃,14d) 重量变化 ",null,1200,null,"1×10"]
["电线电缆检测中心",11,"绝缘机械物理性能","老化前拉力试验",null,250,null,"JKLV"]
["电线电缆检测中心",11,"绝缘机械物理性能","老化前拉力试验",null,250,null,"JKLYJ-1"]
["电线电缆检测中心",11,"绝缘机械物理性能","收缩试验 (130℃,1h) 收缩率",null,600,null,"JKLYJ-1"]
["电线电缆检测中心",11,"绝缘机械物理性能","热延伸试验（200℃,15min，20N/cm²）",null,410,null,"JKLYJ-1"]
["电线电缆检测中心",12,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KVV"]
["电线电缆检测中心",12,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KVVR"]
["电线电缆检测中心",12,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KYJV"]
["电线电缆检测中心",12,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"KYJV"]
["电线电缆检测中心",12,"绝缘机械物理性能","老化前拉力试验",null,250,null,"1×10"]
["电线电缆检测中心",12,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"1×10"]
["电线电缆检测中心",12,"绝缘机械物理性能","人工气候老化试验 （0ｈ～1008ｈ）",null,2625,null,"1×10"]
["电线电缆检测中心",12,"绝缘机械物理性能","人工气候老化试验 （504ｈ～1008ｈ）",null,2625,null,"1×10"]
["电线电缆检测中心",12,"绝缘机械物理性能","吸水试验 (85℃,14d) 重量变化 ",null,1200,null,"1×10"]
["电线电缆检测中心",12,"绝缘机械物理性能","收缩试验 (130℃,1h) 收缩率",null,600,null,"1×10"]
["电线电缆检测中心",12,"绝缘机械物理性能","热延伸试验（200℃,15min，20N/cm²）",null,410,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KVV22"]
["电线电缆检测中心",13,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KYJV22"]
["电线电缆检测中心",13,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"KYJV22"]
["电线电缆检测中心",13,"绝缘机械物理性能","空气烘箱老化试验(80℃,7d)",null,450,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","人工气候老化试验 （504ｈ～1008ｈ）",null,2625,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","热失重试验（80℃,7d）",null,600,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","抗开裂试验（150℃,1ｈ）",null,400,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","高温压力试验 （温度80℃, 时间：外径Ｄ≤１５ｍｍ，４ｈ； 外径Ｄ＞15ｍｍ，６ｈ）",null,600,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","低温卷绕试验 （－35℃）",null,400,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","低温拉伸试验 （－35℃）",null,400,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","低温冲击试验 （－35℃）",null,400,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","吸水试验 (70℃,10d) 电压法 ",null,1200,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","老化前拉力试验",null,250,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,10d)",null,1800,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","人工气候老化试验 （0ｈ～1008ｈ）",null,2625,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","吸水试验 (85℃,14d) 重量变化 ",null,1200,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","收缩试验 (100℃,1h) 收缩率",null,600,null,"1×10"]
["电线电缆检测中心",13,"绝缘机械物理性能","熔融指数 (熔体质量流动速率)",null,600,null,"1×10"]
["电线电缆检测中心",14,"绝缘机械物理性能","老化前拉力试验",null,250,null,"2×0.5"]
["电线电缆检测中心",14,"绝缘机械物理性能","空气烘箱老化后拉力试验(80℃,7d)",null,450,null,"2×0.5"]
["电线电缆检测中心",14,"绝缘机械物理性能","失重试验(80℃,7d)",null,600,null,"2×0.5"]
["电线电缆检测中心",14,"绝缘机械物理性能","高温压力 (70℃,4h) -压痕中间值/护套平均厚度",null,600,null,"2×0.5"]
["电线电缆检测中心",14,"绝缘机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"2×0.5"]
["电线电缆检测中心",14,"绝缘机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",14,"绝缘机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"2×0.5"]
["电线电缆检测中心",14,"绝缘机械物理性能","低温冲击试验 （-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",14,"绝缘机械物理性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","失重试验(80℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","高温压力 (80℃,4h) -压痕中间值/护套平均厚度",null,600,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","低温冲击试验 （-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KVVP"]
["电线电缆检测中心",14,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KVVP2-22"]
["电线电缆检测中心",14,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KVVRP"]
["电线电缆检测中心",14,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"2×0.75"]
["电线电缆检测中心",14,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KYJVP"]
["电线电缆检测中心",14,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"KYJVP"]
["电线电缆检测中心",14,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KYJVP2-22"]
["电线电缆检测中心",14,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"KYJVP2-22"]
["电线电缆检测中心",14,"绝缘机械物理性能","老化前拉力试验",null,250,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",14,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",14,"绝缘机械物理性能","老化前拉力试验",null,250,null,"KVV"]
["电线电缆检测中心",15,"绝缘机械物理性能","老化前拉力试验",null,250,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","失重试验(80℃,7d)",null,600,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","高温压力 (80℃,4h) -压痕中间值/护套平均厚度",null,600,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","低温冲击试验 （-15℃）",null,400,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","失重试验(80℃,7d) -压痕中间值/护套平均厚度",null,600,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"4×0.75"]
["电线电缆检测中心",15,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"4×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","失重试验(80℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","高温压力 (80℃,4h) -压痕中间值/护套平均厚度",null,600,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","低温冲击试验 （-15℃）",null,400,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","老化前拉力试验",null,250,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","空气烘箱老化后拉力试验(80℃,7d)",null,450,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","空气烘箱老化后拉力试验(80℃,8d)",null,450,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","空气烘箱老化后拉力试验(80℃,9d)",null,450,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","空气烘箱老化后拉力试验(80℃,10d)",null,450,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","失重试验(80℃,7d)",null,600,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","高温压力 (70℃,4h) -压痕中间值/护套平均厚度",null,600,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","低温冲击试验 （-15℃）",null,400,null,"2×0.5"]
["电线电缆检测中心",16,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"2×0.75"]
["电线电缆检测中心",16,"绝缘机械物理性能","老化前拉力试验",null,250,null,"1×25"]
["电线电缆检测中心",16,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"1×25"]
["电线电缆检测中心",16,"绝缘机械物理性能","人工气候老化试验 （0d～42d）",null,2625,null,"1×25"]
["电线电缆检测中心",16,"绝缘机械物理性能","人工气候老化试验 （21d～42d）",null,2625,null,"1×25"]
["电线电缆检测中心",16,"绝缘机械物理性能","老化前拉力试验",null,250,null,"JKLYJ-10"]
["电线电缆检测中心",17,"绝缘机械物理性能","老化前拉力试验",null,250,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","失重试验(80℃,7d)",null,600,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","高温压力 (80℃,4h) -压痕中间值/护套平均厚度",null,600,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","低温冲击试验 （-15℃）",null,400,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","老化前拉力试验",null,250,null,"4×2.5"]
["电线电缆检测中心",17,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,450,null,"4×2.5"]
["电线电缆检测中心",17,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,450,null,"4×2.5"]
["电线电缆检测中心",17,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"4×4"]
["电线电缆检测中心",17,"绝缘机械物理性能","老化前拉力试验",null,250,null,"1×25"]
["电线电缆检测中心",17,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,10d)",null,1800,null,"1×25"]
["电线电缆检测中心",17,"绝缘机械物理性能","人工气候老化试验 （0d～42d）",null,2625,null,"1×25"]
["电线电缆检测中心",17,"绝缘机械物理性能","人工气候老化试验 （21d～42d）",null,2625,null,"1×25"]
["电线电缆检测中心",17,"绝缘机械物理性能","老化前拉力试验",null,250,null,"TICW计算机"]
["电线电缆检测中心",17,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"TICW计算机"]
["电线电缆检测中心",18,"绝缘机械物理性能","老化前拉力试验",null,250,null,"4×1.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"4×1.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","高温压力 (80℃,4h) -压痕中间值/护套平均厚度",null,600,null,"4×1.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","热冲击试验（抗开裂试验）(150℃,1h)",null,400,null,"4×1.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","低温弯曲试验 （-15℃）",null,400,null,"4×1.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","低温拉伸试验 (-15℃)",null,400,null,"4×1.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","低温冲击试验 （-15℃）",null,400,null,"4×1.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","失重试验(80℃,7d)",null,600,null,"4×1.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","老化前拉力试验",null,250,null,"4×2.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"4×2.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"4×2.5"]
["电线电缆检测中心",18,"绝缘机械物理性能","老化前拉力试验",null,250,null,"48×1"]
["电线电缆检测中心",18,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"48×1"]
["电线电缆检测中心",18,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,null,"48×1"]
["电线电缆检测中心",19,"绝缘机械物理性能","老化前拉力试验",null,250,null,"1×25"]
["电线电缆检测中心",19,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"1×25"]
["电线电缆检测中心",19,"绝缘机械物理性能","人工气候老化试验 （0d～42d）",null,2625,null,"1×25"]
["电线电缆检测中心",19,"绝缘机械物理性能","人工气候老化试验 （21d～42d）",null,2625,null,"1×25"]
["电线电缆检测中心",19,"绝缘机械物理性能","空气烘箱老化后拉力试验(100℃,10d)",null,1800,null,"1×25"]
["电线电缆检测中心",25,"绝缘机械物理性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,"绝缘为乙丙橡胶时做空气弹老化（E）","充电桩电缆"]
["电线电缆检测中心",25,"绝缘机械物理性能","绝缘热收缩试验(130℃,1h)",null,600,null,"充电桩电缆"]
["电线电缆检测中心",25,"绝缘机械物理性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,"绝缘为乙丙橡胶时做热延伸（E,EY）","充电桩电缆"]
["电线电缆检测中心",25,"绝缘机械物理性能","老化前拉力试验",null,250,null,"充电桩电缆"]
["电线电缆检测中心",25,"绝缘机械物理性能","热延伸试验(200℃,15min，20N/cm²)",null,410,"绝缘为乙丙橡胶时做热延伸（E,EY）","充电桩电缆"]
["电线电缆检测中心",25,"绝缘机械物理性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"充电桩电缆"]
["电线电缆检测中心",25,"绝缘机械物理性能","高温压力-压痕中间值/绝缘平均厚度",null,600,"绝缘为热塑性弹性体时（S,S90）做","充电桩电缆"]
["电线电缆检测中心",25,"绝缘机械物理性能","低温卷绕试验",null,400,"外径≤12.5时做","充电桩电缆"]
["电线电缆检测中心",25,"绝缘机械物理性能","低温拉伸试验",null,400,"外径＞12.5时做","充电桩电缆"]
["电线电缆检测中心",30,"绝缘机械物理性能","人工气候老化试验 （0ｈ～1008ｈ）",null,2625,null,"GB/T 33594-2017"]
["电线电缆检测中心",30,"绝缘机械物理性能","人工气候老化试验 （504ｈ～1008ｈ）",null,2625,null,"GB/T 33594-2017"]
["电线电缆检测中心",7,"绝缘机械性能","老化前拉力试验",null,250,null,"60227 IEC 01（BV） 450/750V"]
["电线电缆检测中心",7,"绝缘机械性能","老化前拉力试验",null,250,null,"BVR 450/750V"]
["电线电缆检测中心",7,"绝缘机械性能","老化前拉力试验",null,250,null,"BYJ"]
["电线电缆检测中心",7,"绝缘机械性能","老化前拉力试验",null,250,null,"全项WDZAN-BYJ-105 450/750 1×2.5"]
["电线电缆检测中心",7,"绝缘机械性能","老化前拉力试验",null,250,null,"常规WDZA-BYJ 450/750V  1×2.5"]
["电线电缆检测中心",8,"绝缘机械性能","老化前拉力试验",null,250,null,"2×1.5"]
["电线电缆检测中心",8,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×1.5"]
["电线电缆检测中心",8,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×1.5"]
["电线电缆检测中心",8,"绝缘机械性能","老化前拉力试验",null,250,null,"1×2.5"]
["电线电缆检测中心",8,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"1×2.5"]
["电线电缆检测中心",8,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"1×2.5"]
["电线电缆检测中心",8,"绝缘机械性能","老化前拉力试验",null,250,null,"1×0.75"]
["电线电缆检测中心",8,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,45,null,"1×0.75"]
["电线电缆检测中心",8,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"1×0.75"]
["电线电缆检测中心",8,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"1×0.75"]
["电线电缆检测中心",8,"绝缘机械性能","老化前拉力试验",null,250,null,"02RV"]
["电线电缆检测中心",8,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"02RV"]
["电线电缆检测中心",8,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"02RV"]
["电线电缆检测中心",8,"绝缘机械性能","老化前拉力试验",null,250,null,"06RV"]
["电线电缆检测中心",8,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"06RV"]
["电线电缆检测中心",8,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"06RV"]
["电线电缆检测中心",8,"绝缘机械性能","老化前拉力试验",null,250,null,"BLV"]
["电线电缆检测中心",8,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"BLV"]
["电线电缆检测中心",8,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"BLV"]
["电线电缆检测中心",8,"绝缘机械性能","老化前拉力试验",null,250,null,"BV"]
["电线电缆检测中心",8,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"BV"]
["电线电缆检测中心",8,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"BV"]
["电线电缆检测中心",8,"绝缘机械性能","老化前拉力试验",null,250,null,"BVR"]
["电线电缆检测中心",8,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"BVR"]
["电线电缆检测中心",8,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"BVR"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","空气烘箱老化后拉力试验(200℃,10d)",null,450,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,450,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"1×1.5"]
["电线电缆检测中心",9,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"1×1.5"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"1×1.5"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"1×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"1×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"1×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","老化后拉力试验(135℃,10d)",null,450,null,"1×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","失重试验(115℃,10d)",null,600,null,"1×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"BVVB 300/500V"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×0.5"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"RVS 300/300V"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"RVV 300/500V"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"YC 450/750V"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"YJV"]
["电线电缆检测中心",9,"绝缘机械性能","老化前拉力试验",null,250,null,"YJLHVS2常规"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"6×1"]
["电线电缆检测中心",10,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"6×1"]
["电线电缆检测中心",10,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"6×1"]
["电线电缆检测中心",10,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"6×1"]
["电线电缆检测中心",10,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"6×1"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"1×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"1×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"1×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"2×1.0"]
["电线电缆检测中心",10,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×1.0"]
["电线电缆检测中心",10,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×1.0"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"1×0.08"]
["电线电缆检测中心",10,"绝缘机械性能","老化后拉力试验(135℃,10d)",null,450,null,"1×0.08"]
["电线电缆检测中心",10,"绝缘机械性能","失重试验(115℃,10d)",null,600,null,"1×0.08"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.12"]
["电线电缆检测中心",10,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.12"]
["电线电缆检测中心",10,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×0.12"]
["电线电缆检测中心",10,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"1×0.08"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"1×1"]
["电线电缆检测中心",10,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"1×1"]
["电线电缆检测中心",10,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"1×1"]
["电线电缆检测中心",10,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"1×1"]
["电线电缆检测中心",10,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"1×1"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.3"]
["电线电缆检测中心",10,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.3"]
["电线电缆检测中心",10,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×0.3"]
["电线电缆检测中心",10,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"2×0.3"]
["电线电缆检测中心",10,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"2×0.3"]
["电线电缆检测中心",10,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"2×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"2×0.75"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"2×4"]
["电线电缆检测中心",10,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×4"]
["电线电缆检测中心",10,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"2×4"]
["电线电缆检测中心",10,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×4"]
["电线电缆检测中心",10,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"2×4"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"YCW"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"3×300+1×150"]
["电线电缆检测中心",10,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"3×300+1×150"]
["电线电缆检测中心",10,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"3×300+1×150"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"VV"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"BVVB,BLVVB"]
["电线电缆检测中心",10,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"BVVB,BLVVB"]
["电线电缆检测中心",10,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"BVVB,BLVVB"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"RVS"]
["电线电缆检测中心",10,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"RVS"]
["电线电缆检测中心",10,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"RVS"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"RVV"]
["电线电缆检测中心",10,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"RVV"]
["电线电缆检测中心",10,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"RVV"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"YC"]
["电线电缆检测中心",10,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"YC"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"YJV,YJLV"]
["电线电缆检测中心",10,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"YJV,YJLV"]
["电线电缆检测中心",10,"绝缘机械性能","老化前拉力试验",null,250,null,"YZ"]
["电线电缆检测中心",10,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"YZ"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"1×95"]
["电线电缆检测中心",11,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"1×95"]
["电线电缆检测中心",11,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"1×95"]
["电线电缆检测中心",11,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"1×95"]
["电线电缆检测中心",11,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"1×95"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×1.5"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"1×0.5"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"1×0.5"]
["电线电缆检测中心",11,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"1×0.5"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.5"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.5"]
["电线电缆检测中心",11,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×0.5"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",11,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×0.75"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(135℃,10d)",null,450,null,"2×0.5"]
["电线电缆检测中心",11,"绝缘机械性能","失重试验(115℃,10d)",null,600,null,"2×0.5"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(135℃,10d)",null,450,null,"2×0.75"]
["电线电缆检测中心",11,"绝缘机械性能","绝缘非污染试验(100℃,10d)",null,450,null,"2×0.75"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"2×1.5"]
["电线电缆检测中心",11,"绝缘机械性能","空气烘箱老化后拉力试验(80℃,7d)",null,450,null,"2×1.5"]
["电线电缆检测中心",11,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×1.5"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"1×0.08"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.08"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(135℃,10d)",null,450,null,"2×0.08"]
["电线电缆检测中心",11,"绝缘机械性能","失重试验(115℃,10d)",null,600,null,"2×0.08"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.08"]
["电线电缆检测中心",11,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×0.08"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"RVVP 300/300V"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"3×300+1×150"]
["电线电缆检测中心",11,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×300+1×150"]
["电线电缆检测中心",11,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"3×300+1×150"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"3×16"]
["电线电缆检测中心",11,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×16"]
["电线电缆检测中心",11,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"3×16"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"VV22"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"WDZAN-YJY23"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"YJV32"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"YJY22"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"AVVR"]
["电线电缆检测中心",11,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"AVVR"]
["电线电缆检测中心",11,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"AVVR"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"VV,VLV"]
["电线电缆检测中心",11,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"VV,VLV"]
["电线电缆检测中心",11,"绝缘机械性能","老化前拉力试验",null,250,null,"VLHVS2"]
["电线电缆检测中心",11,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"VLHVS2"]
["电线电缆检测中心",11,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"VLHVS2"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×1.5"]
["电线电缆检测中心",12,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"2×1.5"]
["电线电缆检测中心",12,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm² )",null,410,null,"2×1.5"]
["电线电缆检测中心",12,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"2×1.5"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"2×1.5"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"6×1"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"6×1"]
["电线电缆检测中心",12,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"6×1"]
["电线电缆检测中心",12,"绝缘机械性能","热延伸试验 (200℃,15min，0.2N/mm)",null,410,null,"6×1"]
["电线电缆检测中心",12,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"6×1"]
["电线电缆检测中心",12,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"6×1"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.12"]
["电线电缆检测中心",12,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.12"]
["电线电缆检测中心",12,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×0.12"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.08"]
["电线电缆检测中心",12,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.08"]
["电线电缆检测中心",12,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×0.08"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"2×35"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,250,null,"2×35"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×35"]
["电线电缆检测中心",12,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,450,null,"2×35"]
["电线电缆检测中心",12,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×35"]
["电线电缆检测中心",12,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"2×35"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"3×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"3×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"2×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"2×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"3×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"3×0.3"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"3×300+1×150"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"3×300+1×150"]
["电线电缆检测中心",12,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"3×300+1×150"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"3×300+1×150"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"YJY22"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"YJY22"]
["电线电缆检测中心",12,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"YJY22"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"RVVP"]
["电线电缆检测中心",12,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"RVVP"]
["电线电缆检测中心",12,"绝缘机械性能","失重试验(80℃,7d)",null,450,null,"RVVP"]
["电线电缆检测中心",12,"绝缘机械性能","老化前抗张强度",null,250,null,"YJV-8.7/10"]
["电线电缆检测中心",12,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJV-8.7/10"]
["电线电缆检测中心",12,"绝缘机械性能","老化前抗张强度",null,250,null,"YJV-26/35"]
["电线电缆检测中心",12,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJV-26/35"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"VLHV22"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"VLHV22"]
["电线电缆检测中心",12,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"VLHV22"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"YJLHV22"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"YJLHV22"]
["电线电缆检测中心",12,"绝缘机械性能","老化前拉力试验",null,250,null,"YJLHVS2"]
["电线电缆检测中心",12,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"YJLHVS2"]
["电线电缆检测中心",12,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"YJLHVS2"]
["电线电缆检测中心",13,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"2×0.75"]
["电线电缆检测中心",13,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"2×0.75"]
["电线电缆检测中心",13,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"2×0.75"]
["电线电缆检测中心",13,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.75"]
["电线电缆检测中心",13,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,900,null,"2×0.75"]
["电线电缆检测中心",13,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm² )",null,410,null,"2×0.75"]
["电线电缆检测中心",13,"绝缘机械性能","老化前拉力试验",null,250,null,"1×1.5"]
["电线电缆检测中心",13,"绝缘机械性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"1×1.5"]
["电线电缆检测中心",13,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"1×1.5"]
["电线电缆检测中心",13,"绝缘机械性能","热延伸试验(200℃,15min，0.2N/mm² )",null,410,null,"1×1.5"]
["电线电缆检测中心",13,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"1×1.5"]
["电线电缆检测中心",13,"绝缘机械性能","老化前拉力试验",null,250,null,"2×0.08"]
["电线电缆检测中心",13,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×0.08"]
["电线电缆检测中心",13,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×0.08"]
["电线电缆检测中心",13,"绝缘机械性能","老化前拉力试验",null,250,null,"GB/T 33594-2017"]
["电线电缆检测中心",13,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"GB/T 33594-2017"]
["电线电缆检测中心",13,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"GB/T 33594-2017"]
["电线电缆检测中心",13,"绝缘机械性能","空气弹老化后拉力试验 (127℃,40ｈ)",null,1075,null,"GB/T 33594-2017"]
["电线电缆检测中心",13,"绝缘机械性能","耐臭氧试验 （25℃，24h，臭氧浓度0.025～0.030%）",null,500,null,"GB/T 33594-2017"]
["电线电缆检测中心",14,"绝缘机械性能","老化前拉力试验",null,250,null,"2×2×0.12"]
["电线电缆检测中心",14,"绝缘机械性能","老化后拉力试验(80℃,7d)",null,450,null,"2×2×0.12"]
["电线电缆检测中心",14,"绝缘机械性能","失重试验(80℃,7d)",null,600,null,"2×2×0.12"]
["电线电缆检测中心",14,"绝缘机械性能","老化前断裂伸长率",null,250,null,"3×400"]
["电线电缆检测中心",14,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"3×400"]
["电线电缆检测中心",14,"绝缘机械性能","附加段老化后试验(100℃ 7d)",null,900,null,"3×400"]
["电线电缆检测中心",14,"绝缘机械性能","老化前抗张强度",null,250,null,"3×400"]
["电线电缆检测中心",15,"绝缘机械性能","老化前拉力试验",null,250,null,"YJY"]
["电线电缆检测中心",15,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"YJY"]
["电线电缆检测中心",15,"绝缘机械性能","老化前抗张强度",null,250,null,"YJLHV22常规"]
["电线电缆检测中心",15,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJLHV22常规"]
["电线电缆检测中心",15,"绝缘机械性能","老化前抗张强度",null,250,null,"YJLHS2常规"]
["电线电缆检测中心",15,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJLHS2常规"]
["电线电缆检测中心",15,"绝缘机械性能","老化前抗张强度",null,250,null,"YJLHVS2"]
["电线电缆检测中心",15,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJLHVS2"]
["电线电缆检测中心",15,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"YJLHVS2"]
["电线电缆检测中心",15,"绝缘机械性能","附加段老化后试验(100℃ 7d)",null,900,null,"YJLHVS2"]
["电线电缆检测中心",15,"绝缘机械性能","老化前抗张强度",null,250,null,"YJLHVS2常规"]
["电线电缆检测中心",15,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJLHVS2常规"]
["电线电缆检测中心",16,"绝缘机械性能","老化前抗张强度",null,250,null,"YJV22-8.7/10"]
["电线电缆检测中心",16,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJV22-8.7/10"]
["电线电缆检测中心",16,"绝缘机械性能","老化前抗张强度",null,250,null,"YJV22-26/35"]
["电线电缆检测中心",16,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJV22-26/35"]
["电线电缆检测中心",16,"绝缘机械性能","老化前拉力试验",null,250,null,"VLHV22常规"]
["电线电缆检测中心",16,"绝缘机械性能","老化前拉力试验",null,250,null,"YJLHV22常规"]
["电线电缆检测中心",16,"绝缘机械性能","老化前拉力试验",null,250,null,"VLHVS2常规"]
["电线电缆检测中心",18,"绝缘机械性能","老化前抗张强度",null,250,null,"3×400"]
["电线电缆检测中心",18,"绝缘机械性能","老化前断裂伸长率",null,250,null,"3×400"]
["电线电缆检测中心",18,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"3×400"]
["电线电缆检测中心",18,"绝缘机械性能","附加段老化后试验(100℃ 7d)",null,900,null,"3×400"]
["电线电缆检测中心",18,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"YJLHV22"]
["电线电缆检测中心",18,"绝缘机械性能","附加段老化后试验(100℃ 7d)",null,900,null,"YJLHV22"]
["电线电缆检测中心",18,"绝缘机械性能","老化前抗张强度",null,250,null,"YJLHV22"]
["电线电缆检测中心",18,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJLHV22"]
["电线电缆检测中心",19,"绝缘机械性能","老化前抗张强度",null,250,null,"YJLHVS2"]
["电线电缆检测中心",19,"绝缘机械性能","老化前断裂伸长率",null,250,null,"YJLHVS2"]
["电线电缆检测中心",19,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"YJLHVS2"]
["电线电缆检测中心",19,"绝缘机械性能","附加段老化后试验(100℃ 7d)",null,900,null,"YJLHVS2"]
["电线电缆检测中心",19,"绝缘机械性能","老化前抗张强度",null,250,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",19,"绝缘机械性能","老化前断裂伸长率",null,250,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",19,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",19,"绝缘机械性能","附加段老化后试验(100℃ 7d)",null,900,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",20,"绝缘机械性能","老化前抗张强度",null,250,null,"3×400"]
["电线电缆检测中心",20,"绝缘机械性能","老化前断裂伸长率",null,250,null,"3×400"]
["电线电缆检测中心",20,"绝缘机械性能","空气烘箱老化后拉力试验(135℃,7d)",null,900,null,"3×400"]
["电线电缆检测中心",20,"绝缘机械性能","附加段老化后试验(100℃ 7d)",null,900,null,"3×400"]
["电线电缆检测中心",27,"绝缘机械性能","成品电缆段的附加老化试验(100℃ 7d)",null,900,null,"充电桩电缆"]
["电线电缆检测中心",15,"绝缘耐漏电痕迹试验(4kV,101次喷水)",null,null,500,null,"1×25"]
["电线电缆检测中心",16,"绝缘耐漏电痕迹试验(4kV,101次喷水)",null,null,500,null,"1×25"]
["电线电缆检测中心",18,"绝缘耐漏电痕迹试验(4kV,101次喷水)",null,null,500,null,"1×25"]
["电线电缆检测中心",1,"绝缘平均厚度",null,null,110,null,"KYJV22"]
["电线电缆检测中心",1,"绝缘平均厚度",null,null,110,null,"50黑"]
["电线电缆检测中心",1,"绝缘平均厚度",null,null,110,null,"1.25 黑白"]
["电线电缆检测中心",1,"绝缘平均厚度",null,null,110,null,1]
["电线电缆检测中心",1,"绝缘平均厚度",null,null,110,null,"0.75 白"]
["电线电缆检测中心",1,"绝缘平均厚度",null,"DIN 72551-5/1991",110,null,"DIN 72551-5/1991"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"60227 IEC 01（BV） 450/750V"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"2×1.5"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"2×0.75"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"1×0.75"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"1×2.5"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"BVVB 300/500V"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"2×1.0"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"RVS 300/300V"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"RVV 300/500V"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"2×0.08"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"2×2×0.12"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"RVVP 300/300V"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"2×35"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"1×1"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"2×0.3"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"2×4"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YC 450/750V"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YCW"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"3×0.3"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"KVV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"KVV22"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"KVVP"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"KVVP2-22"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"KVVR"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"KVVRP"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"KYJV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"KYJVP"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"KYJVP2-22"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"1×10"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"JKLYJ-1"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"3×16"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJY22"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"VV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"VV22"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"WDZAN-YJY23"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJV22"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJV32"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"3×400"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"02RV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"06RV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"BLV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"BV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"BVR"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"BVVB,BLVVB"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"BYJ"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"RVS"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"RVV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"RVVP"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"VV,VLV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YC"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJV,YJLV"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YZ"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJV22-8.7/10"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJV-8.7/10"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJV22-26/35"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJV-26/35"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"全项WDZAN-BYJ-105 450/750 1×2.5"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"常规WDZA-BYJ 450/750V  1×2.5"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"VLHV22"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"VLHVS2"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJLHVS2常规"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJLHS2常规"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",3,"绝缘平均厚度",null,null,110,null,"充电桩电缆"]
["电线电缆检测中心",3,"绝缘平均厚度",null,"QC/T1037-2016",110,null,"QC/T1037-2016"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"2×0.75"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"1×1.5"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"6×1"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"1×0.5"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"2×0.5"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"BVR 450/750V"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"2×1.5"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,100,null,"4×4"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"4×0.75"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"4×2.5"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"48×1"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"1×10"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"1×25"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"JKLYJ-10"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"AVVR"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"JKLV"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"VLHV22常规"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"VLHVS2常规"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"TICW计算机"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"GB/T 33594-2017"]
["电线电缆检测中心",4,"绝缘平均厚度",null,null,110,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",5,"绝缘平均厚度",null,null,110,null,"1×0.08"]
["电线电缆检测中心",5,"绝缘平均厚度",null,null,110,null,"2×0.12"]
["电线电缆检测中心",5,"绝缘平均厚度",null,null,110,null,"2×0.08"]
["电线电缆检测中心",5,"绝缘平均厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",7,"绝缘平均厚度",null,null,110,null,"YJY"]
["电线电缆检测中心",7,"绝缘平均厚度",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",6,"绝缘平均总厚度",null,null,110,null,"1×0.5"]
["电线电缆检测中心",24,"绝缘屏蔽剥离试验","老化前",null,482.5,null,"3×400"]
["电线电缆检测中心",24,"绝缘屏蔽剥离试验","附加段老化试验后(100℃,7d)",null,482.5,null,"3×400"]
["电线电缆检测中心",25,"绝缘屏蔽剥离试验","老化前",null,482.5,null,"YJLHVS2"]
["电线电缆检测中心",25,"绝缘屏蔽剥离试验","附加段老化试验后(100℃,7d)",null,482.5,null,"YJLHVS2"]
["电线电缆检测中心",28,"绝缘屏蔽剥离试验","老化前",null,482.5,null,"3×400"]
["电线电缆检测中心",28,"绝缘屏蔽剥离试验","附加段老化试验后(100℃,7d)",null,482.5,null,"3×400"]
["电线电缆检测中心",28,"绝缘屏蔽剥离试验","附加段老化试验后(100℃,7d)",null,48235,null,"3×400"]
["电线电缆检测中心",28,"绝缘屏蔽剥离试验","老化前",null,482.5,null,"YJLHV22"]
["电线电缆检测中心",28,"绝缘屏蔽剥离试验","附加段老化试验后(100℃,7d)",null,482.5,null,"YJLHV22"]
["电线电缆检测中心",29,"绝缘屏蔽剥离试验","老化前",null,482.5,null,"YJLHVS2"]
["电线电缆检测中心",29,"绝缘屏蔽剥离试验","附加段老化试验后(100℃,7d)",null,482.5,null,"YJLHVS2"]
["电线电缆检测中心",29,"绝缘屏蔽剥离试验","老化前",null,482.5,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",29,"绝缘屏蔽剥离试验","附加段老化试验后(100℃,7d)",null,482.5,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",30,"绝缘屏蔽剥离试验","老化前",null,482.5,null,"3×400"]
["电线电缆检测中心",30,"绝缘屏蔽剥离试验","附加段老化试验后(100℃,7d)",null,482.5,null,"3×400"]
["电线电缆检测中心",13,"绝缘热冲击试验(150℃,1h)",null,null,400,null,"VV,VLV"]
["电线电缆检测中心",12,"绝缘热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×16"]
["电线电缆检测中心",13,"绝缘热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",14,"绝缘热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"3×300+1×150"]
["电线电缆检测中心",11,"绝缘热收缩试验 (150℃,15min, L=200mm)",null,null,600,null,"1×0.08"]
["电线电缆检测中心",13,"绝缘热收缩试验(130℃,1h)",null,null,600,null,"3×300+1×150"]
["电线电缆检测中心",13,"绝缘热收缩试验(130℃,1h)",null,null,600,null,"YJV,YJLV"]
["电线电缆检测中心",15,"绝缘热收缩试验(130℃,1h)",null,null,600,null,"3×300+1×150"]
["电线电缆检测中心",15,"绝缘热收缩试验(130℃,1h)",null,null,600,null,"YJY22"]
["电线电缆检测中心",15,"绝缘热收缩试验(130℃,1h)",null,null,600,null,"YJLHV22"]
["电线电缆检测中心",16,"绝缘热收缩试验(130℃,1h)",null,null,600,null,"GB/T 33594-2017"]
["电线电缆检测中心",17,"绝缘热收缩试验(130℃,1h)",null,null,600,null,"YJY"]
["电线电缆检测中心",11,"绝缘热收缩试验(150℃,15min, L=200mm)",null,null,600,null,"1×0.08"]
["电线电缆检测中心",11,"绝缘热收缩试验(150℃,15min, L=200mm)",null,null,600,null,"2×0.12"]
["电线电缆检测中心",12,"绝缘热收缩试验(150℃,15min, L=200mm)",null,null,600,null,"2×0.08"]
["电线电缆检测中心",13,"绝缘热收缩试验(150℃,15min, L=200mm)",null,null,600,null,"2×0.12"]
["电线电缆检测中心",13,"绝缘热收缩试验(150℃,15min, L=200mm)",null,null,600,null,"2×0.08"]
["电线电缆检测中心",8,"绝缘热延伸试验(200℃,15min,0.2MPa)","载荷下延伸率",null,410,null,"JKLYJ-10"]
["电线电缆检测中心",8,"绝缘热延伸试验(200℃,15min,0.2MPa)","冷却后永久伸长率",null,410,null,"JKLYJ-10"]
["电线电缆检测中心",18,"绝缘热延伸试验(200℃,15min,0.2MPa)","载荷下延伸率",null,410,null,"1×25"]
["电线电缆检测中心",18,"绝缘热延伸试验(200℃,15min,0.2MPa)","冷却后永久伸长率",null,410,null,"1×25"]
["电线电缆检测中心",18,"绝缘热延伸试验(200℃,15min,0.2MPa)","载荷下延伸率",null,410,null,"JKLYJ-10"]
["电线电缆检测中心",18,"绝缘热延伸试验(200℃,15min,0.2MPa)","冷却后永久伸长率",null,410,null,"JKLYJ-10"]
["电线电缆检测中心",22,"绝缘热延伸试验(200℃,15min,0.2MPa)","载荷下延伸率",null,410,null,"1×25"]
["电线电缆检测中心",22,"绝缘热延伸试验(200℃,15min,0.2MPa)","冷却后永久伸长率",null,410,null,"1×25"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm2)","载荷下延伸率",null,410,null,"YJV-8.7/10"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm2)","冷却后永久伸长率",null,410,null,"YJV-8.7/10"]
["电线电缆检测中心",10,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJV"]
["电线电缆检测中心",10,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJV"]
["电线电缆检测中心",10,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHVS2常规"]
["电线电缆检测中心",10,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHVS2常规"]
["电线电缆检测中心",11,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"3×300+1×150"]
["电线电缆检测中心",11,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"3×300+1×150"]
["电线电缆检测中心",11,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJV,YJLV"]
["电线电缆检测中心",11,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJV,YJLV"]
["电线电缆检测中心",12,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"WDZAN-YJY23"]
["电线电缆检测中心",12,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"WDZAN-YJY23"]
["电线电缆检测中心",12,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJV22"]
["电线电缆检测中心",12,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJV22"]
["电线电缆检测中心",12,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJV32"]
["电线电缆检测中心",12,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJV32"]
["电线电缆检测中心",12,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJY22"]
["电线电缆检测中心",12,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJY22"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"3×300+1×150"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"3×300+1×150"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJY22"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJY22"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJV-26/35"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJV-26/35"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHV22"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHV22"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHVS2"]
["电线电缆检测中心",13,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHVS2"]
["电线电缆检测中心",14,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"GB/T 33594-2017"]
["电线电缆检测中心",14,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"GB/T 33594-2017"]
["电线电缆检测中心",15,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"3×400"]
["电线电缆检测中心",15,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"3×400"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJY"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJY"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHV22常规"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHV22常规"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHS2常规"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHS2常规"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHVS2"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHVS2"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHVS2常规"]
["电线电缆检测中心",16,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHVS2常规"]
["电线电缆检测中心",17,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJV22-8.7/10"]
["电线电缆检测中心",17,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJV22-8.7/10"]
["电线电缆检测中心",17,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJV22-26/35"]
["电线电缆检测中心",17,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJV22-26/35"]
["电线电缆检测中心",17,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHV22常规"]
["电线电缆检测中心",17,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHV22常规"]
["电线电缆检测中心",19,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"3×400"]
["电线电缆检测中心",19,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"3×400"]
["电线电缆检测中心",19,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHV22"]
["电线电缆检测中心",19,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHV22"]
["电线电缆检测中心",20,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"YJLHVS2"]
["电线电缆检测中心",20,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"YJLHVS2"]
["电线电缆检测中心",20,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",20,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",21,"绝缘热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,null,"3×400"]
["电线电缆检测中心",21,"绝缘热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,null,"3×400"]
["电线电缆检测中心",8,"绝缘热延伸试验(200℃,15min,20N/cm)","载荷下延伸率",null,410,null,"BYJ"]
["电线电缆检测中心",8,"绝缘热延伸试验(200℃,15min,20N/cm)","冷却后永久伸长率",null,410,null,"BYJ"]
["电线电缆检测中心",8,"绝缘热延伸试验(200℃,15min,20N/cm)","载荷下延伸率",null,410,null,"全项WDZAN-BYJ-105 450/750 1×2.5"]
["电线电缆检测中心",8,"绝缘热延伸试验(200℃,15min,20N/cm)","冷却后永久伸长率",null,410,null,"全项WDZAN-BYJ-105 450/750 1×2.5"]
["电线电缆检测中心",8,"绝缘热延伸试验(200℃,15min,20N/cm)","载荷下延伸率",null,410,null,"常规WDZA-BYJ 450/750V  1×2.5"]
["电线电缆检测中心",8,"绝缘热延伸试验(200℃,15min,20N/cm)","冷却后永久伸长率",null,410,null,"常规WDZA-BYJ 450/750V  1×2.5"]
["电线电缆检测中心",16,"绝缘收缩试验(130℃,1h) ",null,null,600,null,"3×400"]
["电线电缆检测中心",17,"绝缘收缩试验(130℃,1h) ",null,null,600,null,"YJLHVS2"]
["电线电缆检测中心",20,"绝缘收缩试验(130℃,1h) ",null,null,600,null,"3×400"]
["电线电缆检测中心",20,"绝缘收缩试验(130℃,1h) ",null,null,600,null,"YJLHV22"]
["电线电缆检测中心",21,"绝缘收缩试验(130℃,1h) ",null,null,600,null,"YJLHVS2"]
["电线电缆检测中心",21,"绝缘收缩试验(130℃,1h) ",null,null,600,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",22,"绝缘收缩试验(130℃,1h) ",null,null,600,null,"3×400"]
["电线电缆检测中心",17,"绝缘吸水试验(85℃,14d)","重量变化",null,1200,null,"3×400"]
["电线电缆检测中心",18,"绝缘吸水试验(85℃,14d)","重量变化",null,1200,null,"YJLHVS2"]
["电线电缆检测中心",21,"绝缘吸水试验(85℃,14d)","重量变化",null,1200,null,"3×400"]
["电线电缆检测中心",21,"绝缘吸水试验(85℃,14d)","重量变化",null,1200,null,"YJLHV22"]
["电线电缆检测中心",22,"绝缘吸水试验(85℃,14d)","重量变化",null,1200,null,"YJLHVS2"]
["电线电缆检测中心",22,"绝缘吸水试验(85℃,14d)","重量变化",null,1200,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",23,"绝缘吸水试验(85℃,14d)","重量变化",null,1200,null,"3×400"]
["电线电缆检测中心",12,"绝缘吸水试验(85℃,14d) 重量变化",null,null,1200,null,"3×300+1×150"]
["电线电缆检测中心",14,"绝缘吸水试验(85℃,14d) 重量变化",null,null,1200,null,"3×300+1×150"]
["电线电缆检测中心",14,"绝缘吸水试验(85℃,14d) 重量变化",null,null,1200,null,"YJY22"]
["电线电缆检测中心",14,"绝缘吸水试验(85℃,14d) 重量变化",null,null,1200,null,"YJLHV22"]
["电线电缆检测中心",14,"绝缘吸水试验(85℃,14d) 重量变化",null,null,1200,null,"YJLHVS2"]
["电线电缆检测中心",15,"绝缘吸水试验(85℃,14d) 重量变化",null,null,1200,null,"GB/T 33594-2017"]
["电线电缆检测中心",15,"绝缘线芯撕离试验","拉力机5mm/s的速度撕离绝缘所需的力",null,300,null,"2×0.12"]
["电线电缆检测中心",15,"绝缘线芯撕离试验","绝缘线芯撕离后浸水试验(2000V， 5min)",null,400,null,"2×0.12"]
["电线电缆检测中心",17,"绝缘粘附力(滑脱)试验",null,null,490,null,"1×25"]
["电线电缆检测中心",19,"绝缘粘附力(滑脱)试验",null,null,490,null,"1×25"]
["电线电缆检测中心",21,"绝缘粘附力(滑脱)试验",null,null,490,null,"1×25"]
["电线电缆检测中心",3,"绝缘最薄处厚度",null,null,110,null,"BVR 450/750V"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"60227 IEC 01（BV） 450/750V"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"2×1.5"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"2×0.75"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"1×0.75"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"1×2.5"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"BVVB 300/500V"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"2×1.0"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"RVS 300/300V"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"RVV 300/500V"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"2×2×0.12"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"RVVP 300/300V"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"2×35"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"1×1"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"2×0.3"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"2×4"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YC 450/750V"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YCW"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"3×0.3"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KVV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KVV22"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KVVP"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KVVP2-22"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KVVR"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KVVRP"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KYJV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KYJV22"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KYJVP"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"KYJVP2-22"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"JKLYJ-1"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"3×16"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJY22"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"VV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"VV22"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"WDZAN-YJY23"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJV22"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJV32"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"3×400"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"02RV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"06RV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"BLV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"BV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"BVR"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"BVVB,BLVVB"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"BYJ"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"RVS"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"RVV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"RVVP"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"VV,VLV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YC"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJV,YJLV"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YZ"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJV22-8.7/10"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJV-8.7/10"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJV22-26/35"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJV-26/35"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"全项WDZAN-BYJ-105 450/750 1×2.5"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"常规WDZA-BYJ 450/750V  1×2.5"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"VLHV22"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"VLHVS2"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJLHVS2常规"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJLHS2常规"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"充电桩电缆"]
["电线电缆检测中心",4,"绝缘最薄处厚度",null,null,110,null,"QC/T1037-2016"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"2×0.75"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"1×1.5"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"6×1"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"1×0.5"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"2×0.5"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"2×1.5"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"4×4"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"4×0.75"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"4×2.5"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"48×1"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"1×10"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"1×25"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"AVVR"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"JKLV"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"VLHV22常规"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"TICW计算机"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"GB/T 33594-2017"]
["电线电缆检测中心",5,"绝缘最薄处厚度",null,null,110,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",6,"绝缘最薄处厚度",null,null,110,null,"1×0.08"]
["电线电缆检测中心",6,"绝缘最薄处厚度",null,null,110,null,"2×0.12"]
["电线电缆检测中心",6,"绝缘最薄处厚度",null,null,110,null,"2×0.08"]
["电线电缆检测中心",6,"绝缘最薄处厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",7,"绝缘最薄处厚度",null,null,110,null,"1×0.5"]
["电线电缆检测中心",7,"绝缘最薄处厚度",null,null,110,null,"VLHVS2常规"]
["电线电缆检测中心",8,"绝缘最薄处厚度",null,null,110,null,"YJY"]
["电线电缆检测中心",8,"绝缘最薄处厚度",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",2,"绝缘最薄厚度",null,null,110,null,"50黑"]
["电线电缆检测中心",2,"绝缘最薄厚度",null,null,110,null,"1.25 黑白"]
["电线电缆检测中心",2,"绝缘最薄厚度",null,null,110,null,"0.75 白"]
["电线电缆检测中心",2,"绝缘最薄厚度",null,null,110,null,1]
["电线电缆检测中心",2,"绝缘最薄厚度",null,null,110,null,"DIN 72551-5/1991"]
["电线电缆检测中心",5,"绝缘最大厚度",null,null,110,null,"各种单项试验"]
["电线电缆检测中心",9,"铠装层：钢带层数",null,null,55,null,"YJV22-8.7/10"]
["电线电缆检测中心",9,"铠装层：钢带层数",null,null,55,null,"3×400"]
["电线电缆检测中心",9,"铠装层：钢带层数",null,null,55,null,"YJV22-26/35"]
["电线电缆检测中心",9,"铠装层：钢带层数",null,null,55,null,"YJLHV22"]
["电线电缆检测中心",10,"铠装层：钢带层数",null,null,55,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",6,"铠装金属带尺寸","层",null,55,null,"3×300+1×150"]
["电线电缆检测中心",6,"铠装金属带尺寸","厚",null,55,null,"3×300+1×150"]
["电线电缆检测中心",6,"铠装金属带尺寸","包带间隙与金属带宽度之比",null,55,null,"3×300+1×150"]
["电线电缆检测中心",6,"铠装金属带尺寸","层",null,55,null,"YJY22"]
["电线电缆检测中心",6,"铠装金属带尺寸","厚",null,55,null,"YJY22"]
["电线电缆检测中心",6,"铠装金属带尺寸","包带间隙与金属带宽度之比",null,55,null,"YJY22"]
["电线电缆检测中心",6,"铠装金属带尺寸","层",null,55,null,"VV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","包带间隙与金属带宽度之比",null,55,null,"VV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","层",null,55,null,"WDZAN-YJY23"]
["电线电缆检测中心",6,"铠装金属带尺寸","厚",null,55,null,"WDZAN-YJY23"]
["电线电缆检测中心",6,"铠装金属带尺寸","包带间隙与金属带宽度之比",null,55,null,"WDZAN-YJY23"]
["电线电缆检测中心",6,"铠装金属带尺寸","层",null,55,null,"YJV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","厚",null,55,null,"YJV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","包带间隙与金属带宽度之比",null,55,null,"YJV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","层",null,55,null,"VLHV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","厚",null,55,null,"VLHV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","包带间隙与金属带宽度之比",null,55,null,"VLHV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","层",null,55,null,"YJLHV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","厚",null,55,null,"YJLHV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","包带间隙与金属带宽度之比",null,55,null,"YJLHV22"]
["电线电缆检测中心",6,"铠装金属带尺寸","层",null,55,null,"YJLHVS2"]
["电线电缆检测中心",6,"铠装金属带尺寸","厚",null,55,null,"YJLHVS2"]
["电线电缆检测中心",6,"铠装金属带尺寸","包带间隙与金属带宽度之比",null,55,null,"YJLHVS2"]
["电线电缆检测中心",7,"铠装金属带尺寸","层",null,55,null,"VLHV22常规"]
["电线电缆检测中心",7,"铠装金属带尺寸","厚",null,55,null,"VLHV22常规"]
["电线电缆检测中心",7,"铠装金属带尺寸","包带间隙与金属带宽度之比",null,55,null,"VLHV22常规"]
["电线电缆检测中心",6,"铠装金属丝直径",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",6,"铠装金属丝直径",null,null,110,null,"YJV32"]
["电线电缆检测中心",26,"抗开裂试验(150℃,1h)",null,null,400,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",4,"抗拉强度",null,null,250,null,"全部参数"]
["电线电缆检测中心",11,"抗延燃试验（15 s）","移去火焰后自行熄灭时间",null,300,null,"0.75 白"]
["电线电缆检测中心",11,"抗延燃试验（15 s）","试样上端剩余绝缘长度",null,300,null,"0.75 白"]
["电线电缆检测中心",13,"抗延燃试验（15 s）","移去火焰后自行熄灭时间(s)",null,300,null,1]
["电线电缆检测中心",13,"抗延燃试验（15 s）","上支架下缘与炭化部分起点间距离(mm)",null,300,null,1]
["电线电缆检测中心",15,"抗延燃试验（15 s）","移去火焰后自行熄灭时间(s)",null,600,null,"DIN 72551-5/1991"]
["电线电缆检测中心",11,"缆芯绞合方向",null,null,110,null,"QC/T1037-2016"]
["电线电缆检测中心",13,"缆芯绞合方向",null,null,110,null,"TICW计算机"]
["电线电缆检测中心",12,"缆芯绞合节径比",null,null,110,null,"QC/T1037-2016"]
["电线电缆检测中心",15,"缆芯绞合节径比",null,null,110,null,"TICW计算机"]
["电线电缆检测中心",2,"力学性能","伸长率(L0 =200 mm)",null,250,null,"全部参数"]
["电线电缆检测中心",2,"力学性能","抗拉强度σ ",null,250,null,"全部参数"]
["电线电缆检测中心",2,"力学性能","伸长率(L0 =200 mm)",null,250,null,"全部参数"]
["电线电缆检测中心",8,"铝/塑复合薄膜带厚度",null,null,110,null,"4×0.75"]
["电线电缆检测中心",12,"铝包钢线单线性能","最小铝层厚度",null,270,null,"400/35-48/7"]
["电线电缆检测中心",12,"铝包钢线单线性能","抗拉强度（绞后）",null,250,null,"400/35-48/7"]
["电线电缆检测中心",12,"铝包钢线单线性能","1%伸长时的应力",null,390,null,"400/35-48/7"]
["电线电缆检测中心",12,"铝包钢线单线性能","断裂后伸长率",null,250,null,"400/35-48/7"]
["电线电缆检测中心",12,"铝包钢线单线性能","电阻率(20℃)",null,220,null,"400/35-48/7"]
["电线电缆检测中心",12,"铝包钢线单线性能",null,null,385,null,"400/35-48/7"]
["电线电缆检测中心",12,"铝包钢线单线性能","扭转(100d)",null,385,null,"400/35-48/7"]
["电线电缆检测中心",2,"铝包钢线根数",null,null,110,null,"400/35-48/7"]
["电线电缆检测中心",2,"铝包钢线直径",null,null,75,null,"全部参数"]
["电线电缆检测中心",4,"铝包钢线直径",null,null,110,null,"400/35-48/7"]
["电线电缆检测中心",3,"铝合金带联锁铠装","紧密性试验（砝码拉力133N，悬挂时间60s）",null,800,null,"特殊性能-铝单线-连锁铠装"]
["电线电缆检测中心",11,"铝合金线单线性能（绞后）","抗拉强度",null,250,null,"185/25-24/7"]
["电线电缆检测中心",11,"铝合金线单线性能（绞后）","断裂伸长率",null,250,null,"185/25-24/7"]
["电线电缆检测中心",11,"铝合金线单线性能（绞后）","电阻率(20℃)",null,220,null,"185/25-24/7"]
["电线电缆检测中心",11,"铝合金线单线性能（绞后）","卷绕(1 d，卷绕8圈,)",null,580,null,"185/25-24/7"]
["电线电缆检测中心",1,"铝合金线根数",null,null,110,null,"185/25-24/7"]
["电线电缆检测中心",3,"铝合金线直径",null,null,110,null,"185/25-24/7"]
["电线电缆检测中心",1,"铝线根数",null,null,110,null,"630/35-45/7"]
["电线电缆检测中心",1,"铝线根数",null,null,110,null,"400/35-48/7"]
["电线电缆检测中心",1,"铝线根数",null,null,110,null,"300/20-45/7"]
["电线电缆检测中心",3,"铝线直径",null,null,110,null,"630/35-45/7"]
["电线电缆检测中心",3,"铝线直径",null,null,110,null,"400/35-48/7"]
["电线电缆检测中心",3,"铝线直径",null,null,110,null,"300/20-45/7"]
["电线电缆检测中心",3,"母线截面积S",null,null,80,null,"全部参数"]
["电线电缆检测中心",1,"耐火试验 （供火时间90 min +冷却时间15 min）","2A熔断器不断，指示灯未熄",null,3500,null,"耐火试验"]
["电线电缆检测中心",26,"耐火试验 （供火时间90 min +冷却时间15 min）",null,null,3500,null,"3×300+1×150"]
["电线电缆检测中心",11,"耐磨性能 ","负荷下至试样露出导体时耐磨次数 （导体标称截面积16mm及以上：50N 导体标称截面积16mm以下：30N）",null,500,null,"1×10"]
["电线电缆检测中心",12,"耐磨性能 ","负荷下至试样露出导体时耐磨次数 （导体标称截面积16mm及以上：50N 导体标称截面积16mm以下：30N）",null,500,null,"1×10"]
["电线电缆检测中心",14,"耐磨性能 ","负荷下至试样露出导体时耐磨次数 （导体标称截面积16mm及以上：50N 导体标称截面积16mm以下：30N）",null,500,null,"1×10"]
["电线电缆检测中心",15,"耐磨性能 ","负荷下至试样露出导体时耐磨次数 （导体标称截面积16mm及以上：50N 导体标称截面积16mm以下：30N）",null,500,null,"1×10"]
["电线电缆检测中心",9,"耐磨性试验","拖磨试验 （纱布移动速度: 1500 mm/ min    附加重量: 0.2 kg ）",null,500,null,"1.25 黑白"]
["电线电缆检测中心",9,"耐磨性试验","刮磨试验 （刮针直径: 0.45 mm                 运行速度: 55 次/ min   负荷：7 N ）",null,500,null,"1.25 黑白"]
["电线电缆检测中心",15,"耐燃料试验 (室温浸液: 30 min  室温卷绕 芯轴直径: 30 mm  负荷: 30 kg  卷绕  速度: 0.2 r/s  卷绕圈数: 4） 卷绕后",null,null,2000,null,"50黑"]
["电线电缆检测中心",10,"耐热试验Ⅰ","耐热性（A） （温度: 120 ℃ 时间: 120 h        芯轴直径: 165 mm ） 卷绕后, 耐电压试验 （1 kV  1 min ）",null,2000,null,"1.25 黑白"]
["电线电缆检测中心",14,"耐油试验 (温度: 90 ℃  时间: 48 h  室温卷绕芯轴直径: 30 mm 负荷: 30 kg       卷绕速度: 0.2 r/s  卷绕圈数: 4） 卷绕后",null,null,720,null,"50黑"]
["电线电缆检测中心",12,"难燃性试验（30 s ） 移去火焰后自行熄灭时间",null,null,600,null,"1.25 黑白"]
["电线电缆检测中心",6,"内衬层平均厚度",null,null,110,null,"4×4"]
["电线电缆检测中心",6,"内衬层平均厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",6,"内衬层平均厚度",null,null,110,null,"4×2.5"]
["电线电缆检测中心",6,"内衬层平均厚度",null,null,110,null,"48×1"]
["电线电缆检测中心",7,"内衬层平均厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"3×300+1×150"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"3×16"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"YJY22"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"VV22"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"WDZAN-YJY23"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"YJV22"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"YJV32"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"VLHV22"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",5,"内衬层最薄处厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",6,"内衬层最薄处厚度",null,null,110,null,"VLHV22常规"]
["电线电缆检测中心",6,"内衬层最薄处厚度",null,null,110,null,"VLHVS2"]
["电线电缆检测中心",6,"内衬层最薄处厚度",null,null,110,null,"GB/T 33594-2017"]
["电线电缆检测中心",5,"内衬层最薄厚度",null,null,110,null,"充电桩电缆"]
["电线电缆检测中心",7,"内衬层最薄厚度",null,null,110,null,"4×4"]
["电线电缆检测中心",7,"内衬层最薄厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",7,"内衬层最薄厚度",null,null,110,null,"4×2.5"]
["电线电缆检测中心",7,"内衬层最薄厚度",null,null,110,null,"48×1"]
["电线电缆检测中心",8,"内衬层最薄厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",13,"内护套机械物理性能","老化前拉力试验",null,250,null,"2×35"]
["电线电缆检测中心",13,"内护套机械物理性能","空气烘箱老化后拉力试验(70℃,10d)",null,450,null,"2×35"]
["电线电缆检测中心",13,"内护套机械物理性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×35"]
["电线电缆检测中心",20,"内护套机械物理性能","老化前拉力试验",null,250,null,"充电桩电缆"]
["电线电缆检测中心",20,"内护套机械物理性能","空气烘箱老化后拉力试验(100℃,7d)",null,450,null,"充电桩电缆"]
["电线电缆检测中心",20,"内护套机械物理性能","失重试验(100℃,7d)",null,600,null,"充电桩电缆"]
["电线电缆检测中心",20,"内护套机械物理性能","高温压力 (温度：90℃, 时间：外径D≤15mm，4h 外径D＞15mm，6h) -压痕中间值/护套平均厚度",null,600,"护套为（S,S90,U）时做","充电桩电缆"]
["电线电缆检测中心",20,"内护套机械物理性能","抗开裂试验 (150℃,1h)",null,400,null,"充电桩电缆"]
["电线电缆检测中心",20,"内护套机械物理性能","低温弯曲试验 （-15℃）",null,400,"外径≤12.5时做","充电桩电缆"]
["电线电缆检测中心",20,"内护套机械物理性能","低温拉伸试验 (-15℃)",null,400,"外径＞12.5时做","充电桩电缆"]
["电线电缆检测中心",3,"内护套耐臭氧试验（25℃，24h，臭氧浓度0.025～0.030%）",null,null,500,"护套为（F,U，YJ）时做","708.1-2015电力电缆"]
["电线电缆检测中心",44,"内护套耐臭氧试验（25℃，24h，臭氧浓度0.025～0.030%）",null,null,500,"护套为（F,U，YJ）时做","充电桩电缆"]
["电线电缆检测中心",7,"内护套平内均厚度",null,null,110,null,"2×35"]
["电线电缆检测中心",23,"内护套热延伸试验(200℃,15min,20N/cm²)","冷却后永久伸长率",null,410,"护套为（F,YJ）时做","充电桩电缆"]
["电线电缆检测中心",23,"内护套热延伸试验(200℃,15min,20N/cm²)","载荷下延伸率",null,410,"护套为（F,YJ）时做","充电桩电缆"]
["电线电缆检测中心",5,"捻向",null,null,220,null,"全部参数"]
["电线电缆检测中心",6,"捻制质量","钢绞线内钢丝（含中心钢丝）的一致性",null,240,null,"全部参数"]
["电线电缆检测中心",6,"捻制质量","捻制",null,240,null,"全部参数"]
["电线电缆检测中心",8,"扭转（L=100d) ",null,null,770,null,"全部参数"]
["电线电缆检测中心",3,"扭转性能",null,null,770,null,"全部参数"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"3×400"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"YJV22-8.7/10"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"YJV-8.7/10"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"YJV22-26/35"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"YJV-26/35"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"YJLHS2常规"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",5,"偏心度",null,null,110,null,"YJLHVS2常规"]
["电线电缆检测中心",6,"偏心度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",6,"偏心度",null,null,110,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",4,"平直度","窄边平直度",null,120,null,"全部参数"]
["电线电缆检测中心",6,"平直度","窄边平直度",null,120,null,"铜牌陕西军工"]
["电线电缆检测中心",5,"屏蔽编织密度",null,null,110,null,"2×0.08"]
["电线电缆检测中心",7,"屏蔽编织密度",null,null,110,null,"1×0.08"]
["电线电缆检测中心",11,"燃烧性能","电缆单根垂直燃烧试验",null,300,null,"1×10"]
["电线电缆检测中心",14,"燃烧性能","电缆单根垂直燃烧试验",null,300,null,"1×10"]
["电线电缆检测中心",11,"热冲击试验","绝缘热冲击试验(150℃,1h)",null,400,null,"BLV"]
["电线电缆检测中心",11,"热冲击试验","绝缘热冲击试验(150℃,1h)",null,400,null,"BVR"]
["电线电缆检测中心",13,"热冲击试验","绝缘热冲击试验(150℃,1h)",null,400,null,"RVS"]
["电线电缆检测中心",14,"热冲击试验","绝缘热冲击(150℃,1h)",null,400,null,"BVVB,BLVVB"]
["电线电缆检测中心",14,"热冲击试验","护套热冲击(150℃,1h)",null,400,null,"BVVB,BLVVB"]
["电线电缆检测中心",15,"热冲击试验","绝缘热冲击(150℃,1h)",null,400,null,"RVV"]
["电线电缆检测中心",16,"热冲击试验","绝缘热冲击(150℃,1h)",null,400,null,"AVVR"]
["电线电缆检测中心",16,"热冲击试验","护套热冲击(150℃,1h)",null,400,null,"AVVR"]
["电线电缆检测中心",16,"热冲击试验","绝缘热冲击(150℃,1h)",null,400,null,"RVVP"]
["电线电缆检测中心",16,"热冲击试验","护套热冲击(150℃,1h)",null,400,null,"RVVP"]
["电线电缆检测中心",11,"热冲击试验(150℃,1h)",null,null,400,null,"02RV"]
["电线电缆检测中心",11,"热冲击试验(150℃,1h)",null,null,400,null,"06RV"]
["电线电缆检测中心",11,"热冲击试验(150℃,1h)",null,null,400,null,"BV"]
["电线电缆检测中心",15,"热冲击试验(150℃,1h)",null,null,400,null,"YJV,YJLV"]
["电线电缆检测中心",17,"热冲击试验(150℃,1h)",null,null,400,null,"YJY22"]
["电线电缆检测中心",11,"热冲击试验（抗开裂试验）","绝缘热冲击试验(150℃,1h)",null,400,null,"1×2.5"]
["电线电缆检测中心",11,"热冲击试验（抗开裂试验）","绝缘热冲击试验(150℃,1h)",null,400,null,"1×0.75"]
["电线电缆检测中心",12,"热冲击试验（抗开裂试验）","绝缘热冲击试验(150℃,1h)",null,400,null,"2×0.5"]
["电线电缆检测中心",13,"热冲击试验（抗开裂试验）","绝缘热冲击试验(150℃,1h)",null,400,null,"2×1.0"]
["电线电缆检测中心",14,"热冲击试验（抗开裂试验）","绝缘热冲击(150℃,1h)",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"热冲击试验（抗开裂试验）","护套热冲击(150℃,1h)",null,400,null,"2×0.75"]
["电线电缆检测中心",14,"热冲击试验（抗开裂试验）","绝缘热冲击(150℃,1h)",null,400,null,"1×0.75"]
["电线电缆检测中心",14,"热冲击试验（抗开裂试验）","护套热冲击(150℃,1h)",null,400,null,"1×0.75"]
["电线电缆检测中心",14,"热冲击试验（抗开裂试验）","绝缘热冲击试验(150℃,1h)",null,400,null,"2×0.12"]
["电线电缆检测中心",14,"热冲击试验（抗开裂试验）","绝缘热冲击试验(150℃,1h)",null,400,null,"1×0.08"]
["电线电缆检测中心",15,"热冲击试验（抗开裂试验）","绝缘热冲击(150℃,1h)",null,400,null,"2×0.5"]
["电线电缆检测中心",15,"热冲击试验（抗开裂试验）","绝缘热冲击(150℃,1h)",null,400,null,"2×0.75"]
["电线电缆检测中心",15,"热冲击试验（抗开裂试验）","绝缘热冲击(150℃,1h)",null,400,null,"2×1.5"]
["电线电缆检测中心",15,"热冲击试验（抗开裂试验）","绝缘热冲击试验(150℃,1h)",null,400,null,"1×0.08"]
["电线电缆检测中心",15,"热冲击试验（抗开裂试验）","绝缘热冲击试验(150℃,1h)",null,400,null,"2×0.08"]
["电线电缆检测中心",16,"热冲击试验（抗开裂试验）","绝缘热冲击(150℃,1h)",null,400,null,"2×1.5"]
["电线电缆检测中心",16,"热冲击试验（抗开裂试验）","护套热冲击(150℃,1h)",null,400,null,"2×1.5"]
["电线电缆检测中心",16,"热冲击试验（抗开裂试验）","绝缘热冲击(150℃,1h)",null,400,null,"2×0.75"]
["电线电缆检测中心",16,"热冲击试验（抗开裂试验）","护套热冲击(150℃,1h)",null,400,null,"2×0.75"]
["电线电缆检测中心",16,"热冲击试验（抗开裂试验）","绝缘热冲击试验(150℃,1h)",null,400,null,"2×0.12"]
["电线电缆检测中心",17,"热冲击试验（抗开裂试验）","绝缘热冲击(150℃,1h)",null,400,null,"2×0.08"]
["电线电缆检测中心",17,"热冲击试验（抗开裂试验）","护套热冲击(150℃,1h)",null,400,null,"2×0.08"]
["电线电缆检测中心",18,"热冲击试验（抗开裂试验）","绝缘热冲击(150℃,1h)",null,400,null,"2×2×0.12"]
["电线电缆检测中心",18,"热冲击试验（抗开裂试验）","护套热冲击(150℃,1h)",null,400,null,"2×2×0.12"]
["电线电缆检测中心",11,"热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"2×1.5"]
["电线电缆检测中心",12,"热冲击试验（抗开裂试验）(150℃,1h)",null,null,600,null,"1×1.5"]
["电线电缆检测中心",12,"热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"1×1.5"]
["电线电缆检测中心",12,"热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"1×0.5"]
["电线电缆检测中心",14,"热冲击试验（抗开裂试验）(150℃,1h)",null,null,400,null,"1×0.5"]
["电线电缆检测中心",12,"热收缩―绝缘任意一端收缩（mm） （150 ℃ ，15 min）",null,null,600,null,1]
["电线电缆检测中心",14,"热收缩―绝缘任意一端收缩（mm） （150 ℃ ，15 min）",null,null,600,null,"DIN 72551-5/1991"]
["电线电缆检测中心",11,"热收缩―两端收缩长度 （150 ℃，15 min）",null,null,600,null,"1.25 黑白"]
["电线电缆检测中心",10,"热收缩试验 （150 ℃ ，15 min）",null,null,600,null,"50黑"]
["电线电缆检测中心",16,"热稳定性试验","绝缘热稳定性 (200℃)",null,240,null,"2×0.5"]
["电线电缆检测中心",16,"热稳定性试验","护套热稳定性 (200℃)",null,240,null,"2×0.5"]
["电线电缆检测中心",16,"热稳定性试验","绝缘热稳定性 (200℃)",null,240,null,"2×0.75"]
["电线电缆检测中心",16,"热稳定性试验","护套热稳定性 (200℃)",null,240,null,"2×0.75"]
["电线电缆检测中心",14,"热稳定性试验（200℃）",null,null,240,null,"1×0.5"]
["电线电缆检测中心",15,"热稳定性试验（200℃）",null,null,240,null,"1×0.08"]
["电线电缆检测中心",16,"热稳定性试验（200℃）",null,null,240,null,"1×0.08"]
["电线电缆检测中心",16,"热稳定性试验（200℃）",null,null,240,null,"2×0.08"]
["电线电缆检测中心",6,"热性能","热冲击 (圆棒直径:2.240mm)（拉伸 / %）（试验温度:175℃）",null,600,null,"全部参数"]
["电线电缆检测中心",6,"热性能","软化击穿 （试验温度：270℃  试验时间：2min  负荷：10.00N）",null,380,null,"全部参数"]
["电线电缆检测中心",6,"热性能","热冲击 （圆棒直径:1.800mm） （试验温度:175℃）",null,600,null,"全部参数"]
["电线电缆检测中心",6,"热性能","软化击穿 （试验温度：200℃，试验时间：2min， 负荷：9.00N）",null,380,null,"全部参数"]
["电线电缆检测中心",10,"热性能试验","短期老化 （150 ℃ ，240 h 短期老化后在   -25 ℃ 下卷绕 ，芯轴直径:   6 mm ）",null,1200,null,"0.75 白"]
["电线电缆检测中心",10,"热性能试验","短期老化 （150 ℃ ，240 h 短期老化后在   -25 ℃ 下卷绕 ，芯轴直径:   6 mm ）",null,1200,null,"0.75 白"]
["电线电缆检测中心",10,"热性能试验","热过载 （175 ℃ ，6 h 热过载试验后在室   温度下卷绕 ，芯轴直径: 2 mm ，   重物: 0.5 kg ）",null,600,null,"0.75 白"]
["电线电缆检测中心",10,"热性能试验","热过载 （175 ℃ ，6 h 热过载试验后在室   温度下卷绕 ，芯轴直径: 2 mm ，   重物: 0.5 kg ）",null,600,null,"0.75 白"]
["电线电缆检测中心",10,"热性能试验","热收缩―绝缘任意一端收缩（mm） （150 ℃ ，15 min）",null,600,null,"0.75 白"]
["电线电缆检测中心",11,"热性能试验","短期老化",null,1200,null,1]
["电线电缆检测中心",11,"热性能试验","（150 ℃ ，240 h 短期老化后在 -25 ℃ 下卷绕 ，芯轴直径: 10 mm ）",null,1200,null,1]
["电线电缆检测中心",11,"热性能试验","短期老化 （150 ℃ ，240 h 短期老化后在 -25 ℃ 下卷绕 ，芯轴直径: 10 mm ）",null,1200,null,1]
["电线电缆检测中心",11,"热性能试验","热过载 （175 ℃ ，6 h 热过载试验后在室温下卷绕 ，芯轴直径: 3 mm ，砝码: 2.5 kg）",null,600,null,1]
["电线电缆检测中心",11,"热性能试验","热过载 （175 ℃ ，6 h 热过载试验后在室温下卷绕 ，芯轴直径: 3 mm ，砝码: 2.5 kg）",null,600,null,1]
["电线电缆检测中心",13,"热性能试验","热过载 （175 ℃ ，6 h 热过载试验后在室温下卷绕 ，芯轴直径: 3 mm ，砝码: 2.5 kg）",null,600,null,"DIN 72551-5/1991"]
["电线电缆检测中心",13,"热性能试验","热过载 （175 ℃ ，6 h 热过载试验后在室温下卷绕 ，芯轴直径: 3 mm ，砝码: 2.5 kg）",null,600,null,"DIN 72551-5/1991"]
["电线电缆检测中心",10,"热压试验",null,null,600,null,"DIN 72551-5/1991"]
["电线电缆检测中心",18,"失重试验(100℃,7d)",null,null,600,null,"3×300+1×150"]
["电线电缆检测中心",18,"失重试验(100℃,7d)",null,null,600,null,"YJV,YJLV"]
["电线电缆检测中心",19,"失重试验(100℃,7d)",null,null,600,null,"3×400"]
["电线电缆检测中心",20,"失重试验(100℃,7d)",null,null,600,null,"3×300+1×150"]
["电线电缆检测中心",20,"失重试验(100℃,7d)",null,null,600,null,"YJY22"]
["电线电缆检测中心",20,"失重试验(100℃,7d)",null,null,600,null,"YJLHV22"]
["电线电缆检测中心",20,"失重试验(100℃,7d)",null,null,600,null,"YJLHVS2"]
["电线电缆检测中心",23,"失重试验(100℃,7d)",null,null,600,null,"3×400"]
["电线电缆检测中心",23,"失重试验(100℃,7d)",null,null,600,null,"YJLHV22"]
["电线电缆检测中心",24,"失重试验(100℃,7d)",null,null,600,null,"YJLHVS2"]
["电线电缆检测中心",24,"失重试验(100℃,7d)",null,null,600,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",25,"失重试验(100℃,7d)",null,null,600,null,"3×400"]
["电线电缆检测中心",5,"双钢带铠装","金属带层数",null,55,null,"KVV22"]
["电线电缆检测中心",5,"双钢带铠装","厚度",null,55,null,"KVV22"]
["电线电缆检测中心",5,"双钢带铠装","宽度",null,55,null,"KVV22"]
["电线电缆检测中心",5,"双钢带铠装","包带间隙比金属带宽度",null,55,null,"KVV22"]
["电线电缆检测中心",5,"双钢带铠装","厚度",null,55,null,"KVVP2-22"]
["电线电缆检测中心",5,"双钢带铠装","金属带层数",null,55,null,"KVVP2-22"]
["电线电缆检测中心",5,"双钢带铠装","宽度",null,55,null,"KVVP2-22"]
["电线电缆检测中心",5,"双钢带铠装","包带间隙比金属带宽度",null,55,null,"KVVP2-22"]
["电线电缆检测中心",7,"双钢带铠装","金属带层数",null,55,null,"KYJV22"]
["电线电缆检测中心",7,"双钢带铠装","厚度",null,55,null,"KYJV22"]
["电线电缆检测中心",7,"双钢带铠装","宽度",null,55,null,"KYJV22"]
["电线电缆检测中心",7,"双钢带铠装","包带间隙比金属带宽度",null,55,null,"KYJV22"]
["电线电缆检测中心",8,"双钢带铠装","金属带层数",null,55,null,"KYJVP2-22"]
["电线电缆检测中心",8,"双钢带铠装","厚度",null,55,null,"KYJVP2-22"]
["电线电缆检测中心",8,"双钢带铠装","宽度",null,55,null,"KYJVP2-22"]
["电线电缆检测中心",8,"双钢带铠装","包带间隙比金属带宽度",null,55,null,"KYJVP2-22"]
["电线电缆检测中心",8,"双钢带铠装","金属带层数",null,55,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",8,"双钢带铠装","厚度",null,55,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",8,"双钢带铠装","宽度",null,55,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",8,"双钢带铠装","包带间隙比金属带宽度",null,55,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",10,"双钢带铠装","金属带层数",null,55,null,"4×2.5"]
["电线电缆检测中心",10,"双钢带铠装","厚度",null,55,null,"4×2.5"]
["电线电缆检测中心",10,"双钢带铠装","宽度",null,55,null,"4×2.5"]
["电线电缆检测中心",11,"双钢带铠装","宽度",null,55,null,"4×1.5"]
["电线电缆检测中心",11,"双钢带铠装","包带间隙比金属带宽度",null,55,null,"4×1.5"]
["电线电缆检测中心",11,"双钢带铠装","金属带层数",null,55,null,"4×1.5"]
["电线电缆检测中心",11,"双钢带铠装","厚度",null,55,null,"4×1.5"]
["电线电缆检测中心",11,"双钢带铠装","金属带层数",null,55,null,"4×2.5"]
["电线电缆检测中心",11,"双钢带铠装","厚度",null,55,null,"4×2.5"]
["电线电缆检测中心",11,"双钢带铠装","宽度",null,55,null,"4×2.5"]
["电线电缆检测中心",11,"双钢带铠装","包带间隙比金属带宽度",null,55,null,"4×2.5"]
["电线电缆检测中心",11,"双钢带铠装","金属带层数",null,55,null,"48×1"]
["电线电缆检测中心",11,"双钢带铠装","厚度",null,55,null,"48×1"]
["电线电缆检测中心",11,"双钢带铠装","宽度",null,55,null,"48×1"]
["电线电缆检测中心",11,"双钢带铠装","包带间隙比金属带宽度",null,55,null,"48×1"]
["电线电缆检测中心",24,"酸气含量",null,null,1000,"1000/每层","3×300+1×150"]
["电线电缆检测中心",25,"酸气含量",null,null,1000,"1000/每层","GB/T 33594-2017"]
["电线电缆检测中心",38,"酸气含量-护套",null,null,1000,"护套为（U,YJ）时做","充电桩电缆"]
["电线电缆检测中心",35,"酸气含量-绝缘",null,null,1000,"绝缘为（EY）时做","充电桩电缆"]
["电线电缆检测中心",4,"同心度",null,null,110,null,"DIN 72551-5/1991"]
["电线电缆检测中心",7,"铜带厚度",null,null,110,null,"3×400"]
["电线电缆检测中心",7,"铜带厚度",null,null,110,null,"YJV22-8.7/10"]
["电线电缆检测中心",7,"铜带厚度",null,null,110,null,"YJV-8.7/10"]
["电线电缆检测中心",7,"铜带厚度",null,null,110,null,"YJV22-26/35"]
["电线电缆检测中心",7,"铜带厚度",null,null,110,null,"YJV-26/35"]
["电线电缆检测中心",7,"铜带厚度",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",7,"铜带厚度",null,null,110,null,"YJLHS2常规"]
["电线电缆检测中心",7,"铜带厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",7,"铜带厚度",null,null,110,null,"YJLHVS2常规"]
["电线电缆检测中心",8,"铜带厚度",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",8,"铜带厚度",null,null,110,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",6,"铜带屏蔽搭盖率",null,null,110,null,"3×400"]
["电线电缆检测中心",6,"铜带屏蔽搭盖率",null,null,110,null,"YJV22-8.7/10"]
["电线电缆检测中心",6,"铜带屏蔽搭盖率",null,null,110,null,"YJV-8.7/10"]
["电线电缆检测中心",6,"铜带屏蔽搭盖率",null,null,110,null,"YJV22-26/35"]
["电线电缆检测中心",6,"铜带屏蔽搭盖率",null,null,110,null,"YJV-26/35"]
["电线电缆检测中心",6,"铜带屏蔽搭盖率",null,null,110,null,"YJLHV22"]
["电线电缆检测中心",6,"铜带屏蔽搭盖率",null,null,110,null,"YJLHV22常规"]
["电线电缆检测中心",6,"铜带屏蔽搭盖率",null,null,110,null,"YJLHS2常规"]
["电线电缆检测中心",6,"铜带屏蔽搭盖率",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",7,"铜带屏蔽搭盖率",null,null,110,null,"YJLHVS2"]
["电线电缆检测中心",7,"铜带屏蔽搭盖率",null,null,110,null,"GB/T 11017.2-20141"]
["电线电缆检测中心",6,"铜带屏蔽厚度",null,null,110,null,"KVVP2-22"]
["电线电缆检测中心",7,"铜带屏蔽厚度",null,null,110,null,"KYJVP2-22"]
["电线电缆检测中心",7,"铜带屏蔽厚度",null,null,110,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",8,"铜带屏蔽厚度",null,null,110,null,"4×0.75"]
["电线电缆检测中心",10,"铜带屏蔽厚度",null,null,110,null,"4×1.5"]
["电线电缆检测中心",10,"铜带屏蔽厚度",null,null,110,null,"4×2.5"]
["电线电缆检测中心",10,"铜带屏蔽厚度",null,null,110,null,"48×1"]
["电线电缆检测中心",10,"拖磨试验 （附加重物: 0.2 kg   带子移动速率: 1500 mm / min）",null,null,500,null,1]
["电线电缆检测中心",12,"拖磨试验或者刮磨",null,null,500,null,"DIN 72551-5/1991"]
["电线电缆检测中心",5,"外层绝缘最小厚度",null,null,110,null,"1×0.5"]
["电线电缆检测中心",1,"外观","应光洁，并且不得有可能影响产品性能的所有缺陷，如裂纹、粗糙、划痕和杂质等。",null,270,null,"全部参数"]
["电线电缆检测中心",1,"外观","表面质量",null,270,null,"全部参数"]
["电线电缆检测中心",2,"外观",null," ",270,null,6]
["电线电缆检测中心",4,"外观",null,null,270,null,3]
["电线电缆检测中心",4,"外观质量",null,null,270,null,"全部参数"]
["电线电缆检测中心",11,"外护套的机械物理性能","老化前拉力试验",null,250,null,"YCW"]
["电线电缆检测中心",14,"外护套的机械物理性能","老化前拉力试验",null,250,null,"2×35"]
["电线电缆检测中心",14,"外护套的机械物理性能","空气烘箱老化后拉力试验(70℃,10d)",null,600,null,"2×35"]
["电线电缆检测中心",14,"外护套的机械物理性能","浸矿物油后拉力试验（100℃,24h）",null,900,null,"2×35"]
["电线电缆检测中心",14,"外护套的机械物理性能","浸矿物油后拉力试验（100℃,24h）",null,410,null,"2×35"]
["电线电缆检测中心",14,"外护套的机械物理性能","热延伸试验(200℃,15min，0.2N/mm²)",null,410,null,"2×35"]
["电线电缆检测中心",5,"外护套平均厚度",null,null,110,null,"2×35"]
["电线电缆检测中心",5,"外护套平均厚度",null,null,110,null,"YCW"]
["电线电缆检测中心",6,"外护套最薄处厚度",null,null,110,null,"2×35"]
["电线电缆检测中心",6,"外护套最薄处厚度",null,null,110,null,"YCW"]
["电线电缆检测中心",8,"外径",null,null,75,null,"KVV22"]
["电线电缆检测中心",13,"外径",null,null,75,null,"4×1.5"]
["电线电缆检测中心",5,"外径测量",null,null,75,null,"60227 IEC 01（BV） 450/750V"]
["电线电缆检测中心",5,"外径测量",null,null,75,null,"1×2.5"]
["电线电缆检测中心",5,"外径测量",null,null,75,null,"1×0.75"]
["电线电缆检测中心",5,"外径测量",null,null,75,null,"BVR 450/750V"]
["电线电缆检测中心",5,"外径测量",null,null,75,null,"2×1.0"]
["电线电缆检测中心",5,"外径测量",null,null,75,null,"RVS 300/300V"]
["电线电缆检测中心",5,"外径测量",null,null,75,null,"BYJ"]
["电线电缆检测中心",5,"外径测量",null,null,75,null,"全项WDZAN-BYJ-105 450/750 1×2.5"]
["电线电缆检测中心",5,"外径测量",null,null,75,null,"常规WDZA-BYJ 450/750V  1×2.5"]
["电线电缆检测中心",6,"外径测量","平均值",null,75,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",6,"外径测量","椭圆度",null,110,null,"GB/T 5013.3-2008 60245 IEC 03（YG） 300/500V 1×0.5"]
["电线电缆检测中心",6,"外径测量","平均值",null,75,null,"1×16"]
["电线电缆检测中心",6,"外径测量","椭圆度",null,110,null,"1×16"]
["电线电缆检测中心",6,"外径测量",null,null,75,null,"1×1.5"]
["电线电缆检测中心",6,"外径测量",null,null,75,null,"1×0.5"]
["电线电缆检测中心",7,"外径测量","平均值",null,75,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",7,"外径测量","椭圆度",null,110,null,"60227 IEC 10（BVV） 300/500V"]
["电线电缆检测中心",7,"外径测量","平均值",null,75,null,"1×0.75"]
["电线电缆检测中心",7,"外径测量","椭圆度",null,110,null,"1×0.75"]
["电线电缆检测中心",7,"外径测量",null,null,75,null,"1×0.08"]
["电线电缆检测中心",7,"外径测量",null,null,75,null,"2×0.12"]
["电线电缆检测中心",7,"外径测量","平均值",null,75,null,"1×1"]
["电线电缆检测中心",7,"外径测量","椭圆度",null,110,null,"1×1"]
["电线电缆检测中心",7,"外径测量","平均值",null,75,null,"2×0.3"]
["电线电缆检测中心",7,"外径测量","椭圆度",null,110,null,"2×0.3"]
["电线电缆检测中心",7,"外径测量","平均值",null,75,null,"2×4"]
["电线电缆检测中心",7,"外径测量","椭圆度",null,110,null,"2×4"]
["电线电缆检测中心",7,"外径测量","平均值",null,75,null,"YC 450/750V"]
["电线电缆检测中心",7,"外径测量","椭圆度",null,110,null,"YC 450/750V"]
["电线电缆检测中心",7,"外径测量","平均值",null,75,null,"3×0.3"]
["电线电缆检测中心",7,"外径测量","每跟编织绝缘线芯平均外径",null,75,null,"2×0.3"]
["电线电缆检测中心",7,"外径测量",null,null,75,null,"KVV"]
["电线电缆检测中心",7,"外径测量",null,null,75,null,"KVVR"]
["电线电缆检测中心",7,"外径测量",null,null,75,null,"KYJV"]
["电线电缆检测中心",7,"外径测量","平均值",null,75,null,"YC"]
["电线电缆检测中心",7,"外径测量","椭圆度",null,110,null,"YC"]
["电线电缆检测中心",7,"外径测量","平均值",null,75,null,"YZ"]
["电线电缆检测中心",7,"外径测量","椭圆度",null,110,null,"YZ"]
["电线电缆检测中心",7,"外径测量",null,null,75,null,"QC/T1037-2016"]
["电线电缆检测中心",8,"外径测量","平均值",null,75,null,"2×0.75"]
["电线电缆检测中心",8,"外径测量","椭圆度",null,110,null,"2×0.75"]
["电线电缆检测中心",8,"外径测量","平均值",null,75,null,"2×1.5"]
["电线电缆检测中心",8,"外径测量","椭圆度",null,110,null,"2×1.5"]
["电线电缆检测中心",8,"外径测量","平均值",null,75,null,"1×1.5"]
["电线电缆检测中心",8,"外径测量","椭圆度",null,110,null,"1×1.5"]
["电线电缆检测中心",8,"外径测量","平均值",null,75,null,"1×95"]
["电线电缆检测中心",8,"外径测量","椭圆度",null,110,null,"1×95"]
["电线电缆检测中心",8,"外径测量",null,null,75,null,"1×0.5"]
["电线电缆检测中心",8,"外径测量",null,null,75,null,"1×0.08"]
["电线电缆检测中心",8,"外径测量","平均值",null,75,null,"2×2×0.12"]
["电线电缆检测中心",8,"外径测量","椭圆度",null,110,null,"2×2×0.12"]
["电线电缆检测中心",8,"外径测量","平均值",null,75,null,"YCW"]
["电线电缆检测中心",8,"外径测量","椭圆度",null,110,null,"YCW"]
["电线电缆检测中心",8,"外径测量",null,null,75,null,"2×0.5"]
["电线电缆检测中心",8,"外径测量",null,null,75,null,"2×0.75"]
["电线电缆检测中心",8,"外径测量",null,null,75,null,"KYJV22"]
["电线电缆检测中心",8,"外径测量",null,null,75,null,"KVV"]
["电线电缆检测中心",8,"外径测量",null,null,75,null,"TICW计算机"]
["电线电缆检测中心",9,"外径测量","平均值",null,75,null,"2×35"]
["电线电缆检测中心",9,"外径测量","椭圆度",null,110,null,"2×35"]
["电线电缆检测中心",9,"外径测量",null,null,110,null,"4×0.75"]
["电线电缆检测中心",9,"外径测量",null,null,75,null,"4×0.75"]
["电线电缆检测中心",9,"外径测量",null,null,75,null,"KVVP2-22"]
["电线电缆检测中心",9,"外径测量",null,null,75,null,"KYJVP2-22"]
["电线电缆检测中心",9,"外径测量",null,null,75,null,"WDZA-KYJVP2-23"]
["电线电缆检测中心",9,"外径测量",null,null,75,null,"充电桩电缆"]
["电线电缆检测中心",10,"外径测量",null,null,75,null,"2×0.5"]
["电线电缆检测中心",10,"外径测量",null,null,75,null,"KVVP"]
["电线电缆检测中心",10,"外径测量",null,null,75,null,"KVVRP"]
["电线电缆检测中心",10,"外径测量",null,null,75,null,"KYJVP"]
["电线电缆检测中心",11,"外径测量",null,null,75,null,"4×4"]
["电线电缆检测中心",11,"外径测量",null,null,75,null,"2×0.75"]
["电线电缆检测中心",11,"外径测量",null,null,75,null,"4×2.5"]
["电线电缆检测中心",12,"外径测量",null,null,75,null,"4×1.5"]
["电线电缆检测中心",12,"外径测量",null,null,75,null,"4×2.5"]
["电线电缆检测中心",12,"外径测量",null,null,75,null,"48×1"]
["电线电缆检测中心",6,"外径或外形尺寸",null,null,75,null,"2×0.08"]
["电线电缆检测中心",7,"外径或外形尺寸","平均值",null,75,null,"RVV 300/500V"]
["电线电缆检测中心",8,"外径或外形尺寸","平均值",null,75,null,"2×1.5"]
["电线电缆检测中心",8,"外径或外形尺寸","平均值",null,75,null,"2×0.08"]
["电线电缆检测中心",8,"外径或外形尺寸","椭圆度",null,110,null,"2×0.08"]
["电线电缆检测中心",8,"外径或外形尺寸","平均值",null,75,null,"RVVP 300/300V"]
["电线电缆检测中心",8,"外径或外形尺寸","椭圆度",null,110,null,"RVVP 300/300V"]
["电线电缆检测中心",9,"外径或外形尺寸","平均值",null,75,null,"2×0.08"]
["电线电缆检测中心",9,"外径或外形尺寸","椭圆度",null,110,null,"2×0.08"]
["电线电缆检测中心",6,"外形尺寸",null,null,75,null,"2×0.5"]
["电线电缆检测中心",7,"外形尺寸",null,null,75,null,"BVVB 300/500V"]
["电线电缆检测中心",7,"外形尺寸",null,null,75,null,"2×0.12"]
["电线电缆检测中心",5,"外形尺寸测量",null,null,75,null,"2×1.5"]
["电线电缆检测中心",7,"外形尺寸测量","平均值",null,75,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",7,"外形尺寸测量","椭圆度",null,110,null,"60227 IEC 53（RVV） 300/500V"]
["电线电缆检测中心",7,"外形尺寸测量","平均值",null,75,null,"2×0.75"]
["电线电缆检测中心",8,"外形尺寸测量","平均值",null,75,null,"2×0.5"]
["电线电缆检测中心",8,"外形尺寸测量","平均值",null,75,null,"2×0.75"]
["电线电缆检测中心",8,"外形尺寸测量","椭圆度",null,110,null,"2×0.75"]
["电线电缆检测中心",8,"外形尺寸测量","椭圆度",null,110,null,"2×0.5"]
["电线电缆检测中心",13,"弯曲试验 (正反弯曲三次)",null,null,470,null,"1×25"]
["电线电缆检测中心",14,"弯曲试验 (正反弯曲三次)",null,null,470,null,"1×25"]
["电线电缆检测中心",16,"弯曲试验 (正反弯曲三次)",null,null,470,null,"1×25"]
["电线电缆检测中心",7,"温度指数","恒温寿命试验(h) （扭绞数：8圈，负荷砝码：13.50N） （老化温度Th：250℃）",null,1000,null,"全部参数"]
["电线电缆检测中心",7,"温度指数","动态热重试验 (升温速度β1=180℃/h, β2=240℃/h, β3=300℃/h）",null,1000,null,"全部参数"]
["电线电缆检测中心",7,"温度指数","最小温度指数-5000h对应的温度t",null,1000,null,"全部参数"]
["电线电缆检测中心",7,"温度指数","恒温寿命试验(h) （扭绞数：8圈，负荷砝码：13.50N） （老化温度Th：245℃）",null,1000,null,"全部参数"]
["电线电缆检测中心",7,"温度指数","动态热重试验(cal/mol) (升温速度β1=180℃/h, β2=240℃/h, β3=300℃/h）",null,1000,null,"全部参数"]
["电线电缆检测中心",7,"温度指数","相关系数r",null,5000,null,"全部参数"]
["电线电缆检测中心",7,"温度指数","最小温度指数-20000h对应的温度t ",null,1000,null,"全部参数"]
["电线电缆检测中心",8,"物理—化学特性","热老化 （150 ℃ ，240 h 抗热老化后在 -25 ℃ 下缠绕） ",null,1200,null,1]
["电线电缆检测中心",8,"物理—化学特性","热老化 （150 ℃ ，240 h 抗热老化后在 -25 ℃ 下缠绕） ",null,800,null,1]
["电线电缆检测中心",8,"物理—化学特性","热超负荷试验（175 ℃ ，6 h 热超负荷试验后在室温下缠绕 ，芯轴直径: 3 mm ，   重物: 2.5 kg ，缠绕圈数: 3）",null,600,null,1]
["电线电缆检测中心",8,"物理—化学特性","热超负荷试验（175 ℃ ，6 h 热超负荷试验后在室温下缠绕 ，芯轴直径: 3 mm ，   重物: 2.5 kg ，缠绕圈数: 3）",null,1000,null,1]
["电线电缆检测中心",8,"物理—化学特性","火焰的不传播试验（15 s） 停止供火后试样上R1R2间有焰       持续燃烧时间",null,400,null,1]
["电线电缆检测中心",17,"吸水试验 (70℃,24h)",null,null,1200,null,"3×300+1×150"]
["电线电缆检测中心",18,"吸水试验 (70℃,24h)",null,null,1200,null,"GB/T 33594-2017"]
["电线电缆检测中心",23,"烟密度试验","最小透光率",null,3000,null,"3×300+1×150"]
["电线电缆检测中心",11,"硬铝线单线性能（绞后)","抗拉强度",null,250,null,"400/35-48/7"]
["电线电缆检测中心",11,"硬铝线单线性能（绞后)","电阻率(20℃)",null,220,null,"400/35-48/7"]
["电线电缆检测中心",11,"硬铝线单线性能（绞后)","卷绕(1 d卷绕8圈,退6圈,再紧密卷绕)",null,580,null,"400/35-48/7"]
["电线电缆检测中心",11,"硬铝线单线性能（绞后）","抗拉强度",null,250,null,"630/35-45/7"]
["电线电缆检测中心",11,"硬铝线单线性能（绞后）","电阻率(20℃)",null,220,null,"630/35-45/7"]
["电线电缆检测中心",11,"硬铝线单线性能（绞后）","卷绕(1 d卷绕8圈,退6圈,再紧密卷绕)",null,580,null,"630/35-45/7"]
["电线电缆检测中心",11,"硬铝线单线性能（绞后）","抗拉强度",null,250,null,"300/20-45/7"]
["电线电缆检测中心",11,"硬铝线单线性能（绞后）","电阻率(20℃)",null,220,null,"300/20-45/7"]
["电线电缆检测中心",11,"硬铝线单线性能（绞后）","卷绕(1 d卷绕8圈,退6圈,再紧密卷绕)",null,580,null,"300/20-45/7"]
["电线电缆检测中心",2,"圆角半径r",null,null,120,null,"全部参数"]
["电线电缆检测中心",15,"增值服务","翻译",null,500,null,"各种单项试验"]
["电线电缆检测中心",3,"最小铝层厚度",null,null,270,null,"全部参数"]