{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["Sheet1","Sheet2","Sheet3","轻工"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"轻工","index":3,"n_rows":951,"n_cols":9,"rows_kept":951,"merged":[[0,0,1,8]]}
["轻工中心一次性告知清单"]
[]
["检验部门","一级项目序号","一级项目名称","二级项目名称","检验方法","检验方法简称","收费标准","项目备注","类别名称"]
["轻工及机械检测中心",1,"外观"," ","建筑排水用硬聚氯乙烯（PVC-U）管材 GB/T 5836.1-2018 6.2"," ",50," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",2,"平均外径"," ","塑料管材尺寸测量方法 GB/T 8806-2008 6.3.1"," ",50," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",3,"壁厚"," ","塑料管材尺寸测量方法 GB/T 8806-2008 6.3.2"," ",50," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",4,"不圆度"," ","塑料管材尺寸测量方法 GB/T 8806-2008 6.3.4"," ",50," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",5,"密度"," ","塑料密度和相对密度试验方法 GB/T1033-2008 6.4"," ",150," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",6,"维卡软化温度（VST）"," ","热塑性塑料光彩、管件 维卡软化温度的测定 GB/T8802-2001 6.5"," ",300," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",7,"纵向回缩率"," ","热塑性塑料管材 纵向回缩率的测定 GB/T6671-2001 6.6"," ",220," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",8,"拉伸屈服强度"," ","热塑性塑料管材拉伸性能测定第2部分硬聚氯乙烯(PVC-U)、氯化聚氯乙烯(PVC-C)和高抗冲聚氯乙烯(PVC-HI)管材 GB/T 8804.2-2003  6.8"," ",500," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",9,"落锤冲击试验TIR"," ","热塑性塑料管材耐性外冲击性能 试验方法 时针旋转法 GB/T14152-2001 6.9"," ",950," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",10,"断裂伸长率"," ","塑料管材尺寸测量方法 GB/T 8806-2008"," ",300," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",11,"弯曲度"," ","塑料管材尺寸测量方法 GB/T 8806-2008"," ",100," "," 塑料管材——PVC-U排水管  "]
["轻工及机械检测中心",1,"颜色与外观"," ","冷热水用聚丙烯管道系统 第2部分：管材 GB/T 18742.2-2017 8.2"," ",50," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",2,"平均外径"," ","塑料管材尺寸测量方法 GB/T 8806-2008 8.4.2"," ",50," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",3,"壁厚"," ","塑料管材尺寸测量方法 GB/T 8806-2008 8.4.3"," ",50," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",4,"纵向回缩率"," ","热塑性塑料管材 纵向回缩率的测定 GB/T6671-2001 8.5"," ",220," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",5,"简支梁冲击试验"," ","流体输送用热塑性塑料管材简支梁冲击试验方法 GB/T 18743-2002 8.6"," ",300," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",6,"静液压强度（1h 20℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 8.7"," ",615," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",7,"静液压强度（22h 95℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 8.7"," ",1150," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",8,"静液压强度（165h 95℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 8.7"," ",4725," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",9,"静液压强度（1000h 95℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 8.7"," ",25600," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",10,"熔融温度"," ","塑料差示扫描量热法(DSC)第3部分:熔融和结晶温度及热焓的测定 GB/T 19466.3-2004"," ",500," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",11,"氧化诱导时间"," ","塑料差示扫描量热法(DSC)第6部分:氧化诱导时间(等温OIT)和氧化诱导温度(动态OIT)的测定 GB/T 19466.6-2009 "," ",500," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",12,"灰分"," ","塑料灰分的测定第1部分:通用方法 GB/T9345.1-2008"," ",500," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",13,"卫生性能","铅","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",150," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",13,"卫生性能","镉","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",150," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",13,"卫生性能","高锰酸钾消耗量（以氧气（O2记））","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",120," "," 塑料管材——PP-R给水管  "]
["轻工及机械检测中心",1,"外观"," ","给水用聚乙烯(PE)管道系统第2部分:管材 GB∕T 13663.2-2018 "," ",25," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",2,"颜色"," ","给水用聚乙烯(PE)管道系统第2部分:管材 GB∕T 13663.2-2018 "," ",25," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",3,"平均外径"," ","塑料管材尺寸测量方法 GB/T 8806-2008 7.3.2"," ",50," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",4,"壁厚及偏差"," ","塑料管材尺寸测量方法 GB/T 8806-2008 7.3.3"," ",50," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",5,"静液压强度（100h 20℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 7.8"," ",2100," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",6,"静液压强度（165h 80℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 7.8"," ",4725," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",7,"静液压强度（1000h 80℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 7.8"," ",25600," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",8,"纵向回缩率"," ","热塑性塑料管材 纵向回缩率的测定 GB/T6671-2001 6.6"," ",220," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",9,"氧化诱导时间"," ","塑料差示扫描量热法(DSC)第6部分:氧化诱导时间(等温OIT)和氧化诱导温度(动态OIT)的测定 GB/T 19466.6-2009 "," ",1200," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",10,"断裂伸长率"," ","热塑性塑料管材拉伸性能测定第3部分:聚烯烃管材 GB/T 8804.3-2003 "," ",300," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",11,"卫生性能","铅","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",150," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",11,"卫生性能","镉","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",150," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",11,"卫生性能","高锰酸钾消耗量（以氧气（O2记））","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",120," "," 塑料管材——给水用聚乙烯（PE）管材  "]
["轻工及机械检测中心",1,"外观及颜色"," ","埋地排水用硬聚氯乙烯(PVC-U)结构壁管道系统第1部分:双壁波纹管材 GB/T 18477.1-2007 "," ",50," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",2,"最小平均内径"," ","塑料管材尺寸测量方法 GB/T 8806-2008 8.3"," ",50," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",3,"最小平均外径"," ","塑料管材尺寸测量方法 GB/T 8806-2008 8.3"," ",50," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",4,"最小压层壁厚"," ","塑料管材尺寸测量方法 GB/T 8806-2008 8.3"," ",50," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",5,"最小内层壁厚"," ","塑料管材尺寸测量方法 GB/T 8806-2008 8.3"," ",50," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",6,"最小承口接合长度"," ","塑料管材尺寸测量方法 GB/T 8806-2008 8.3"," ",50," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",7,"密度"," ","塑料密度和相对密度试验方法 GB/T1033-2008 6.4"," ",150," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",8,"环刚度"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.5"," ",400," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",9,"环柔性"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.7"," ",200," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",10,"冲击性能"," ","热塑性塑料管材耐性外冲击性能 试验方法 时针旋转法 GB/T14152-2001 6.9"," ",950," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",11,"烘箱试验"," ","注射成型硬质聚氯乙烯(PVC-U)、氯化聚氯乙烯(PVC-C)、丙烯腈-丁二烯-苯乙烯三元共聚物(ABS)和丙烯腈-苯乙烯-丙烯酸盐三元共聚物(ASA)管件 热烘箱试验方法 GB/T8803-2001 8.8"," ",200," "," 塑料管材——PVC-U 双壁波纹管材  "]
["轻工及机械检测中心",1,"外观"," ","埋地用聚乙烯（PE）结构壁管道系统　第2部分　聚乙烯缠绕结构壁管材  GB/T　19472.2-2017  8.2"," ",50," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",2,"平均内径"," ","埋地用聚乙烯（PE）结构壁管道系统　第2部分　聚乙烯缠绕结构壁管材  GB/T　19472.2-2017  8.3"," ",50," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",3,"承口内径"," ","埋地用聚乙烯（PE）结构壁管道系统　第2部分　聚乙烯缠绕结构壁管材  GB/T　19472.2-2017  8.3"," ",50," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",4,"纵向回缩率"," ","热塑性塑料管材 纵向回缩率的测定 GB/T6671-2001 8.4"," ",220," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",5,"环刚度"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.9"," ",400," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",6,"环柔性"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.11"," ",200," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",7,"烘箱实验"," ","埋地用聚乙烯（PE）结构壁管道系统  第2部分　聚乙烯缠绕结构壁管材  GB/T  19472.2-2017  8.5"," ",200," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",8,"冲击性能"," ","热塑性塑料管材耐性外冲击性能 试验方法 时针旋转法 GB/T14152-2001 8.10"," ",950," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",9,"密度"," ","塑料密度和相对密度试验方法 GB/T1033-2008 8.8"," ",150," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",10,"氧化诱导时间"," ","塑料差示扫描量热法(DSC)第6部分:氧化诱导时间(等温OIT)和氧化诱导温度(动态OIT)的测定 GB/T 19466.6-2009 8.7"," ",500," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",11,"灰分"," ","塑料灰分的测定第1部分:通用方法 GB/T9345.1-2008 8.6"," ",500," "," 塑料管材——聚乙烯缠绕结构壁管材  "]
["轻工及机械检测中心",1,"外观"," ","埋地用聚乙烯（PE）结构壁管道系统 第1部分：聚乙烯双壁波纹管材 GB/T 19472.1-2004 8.2"," ",50," "," 塑料管材——聚乙烯双壁波纹管材  "]
["轻工及机械检测中心",2,"平均内径"," ","埋地用聚乙烯（PE）结构壁管道系统 第1部分：聚乙烯双壁波纹管材 GB/T 19472.1-2004 8.3"," ",50," "," 塑料管材——聚乙烯双壁波纹管材  "]
["轻工及机械检测中心",3,"环刚度"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.9"," ",400," "," 塑料管材——聚乙烯双壁波纹管材  "]
["轻工及机械检测中心",4,"环柔性"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.11"," ",200," "," 塑料管材——聚乙烯双壁波纹管材  "]
["轻工及机械检测中心",5,"烘箱实验"," ","埋地用聚乙烯（PE）结构壁管道系统 第1部分：聚乙烯双壁波纹管材 GB/T 19472.1-2004 8.7"," ",200," "," 塑料管材——聚乙烯双壁波纹管材  "]
["轻工及机械检测中心",6,"冲击性能"," ","热塑性塑料管材耐性外冲击性能 试验方法 时针旋转法 GB/T14152-2001 8.10"," ",950," "," 塑料管材——聚乙烯双壁波纹管材  "]
["轻工及机械检测中心",1,"外观"," ","埋地排水用钢带增强聚乙烯（PE）螺旋波纹管 CJ/T 225-2011　 8.2"," ",50," "," 塑料管材——埋地排水用钢带增强聚乙烯（PE）螺旋波纹管  "]
["轻工及机械检测中心",2,"平均内径"," ","埋地排水用钢带增强聚乙烯（PE）螺旋波纹管 CJ/T 225-2011　 8.3"," ",50," "," 塑料管材——埋地排水用钢带增强聚乙烯（PE）螺旋波纹管  "]
["轻工及机械检测中心",3,"环刚度"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.9"," ",400," "," 塑料管材——埋地排水用钢带增强聚乙烯（PE）螺旋波纹管  "]
["轻工及机械检测中心",4,"环柔性"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.11"," ",200," "," 塑料管材——埋地排水用钢带增强聚乙烯（PE）螺旋波纹管  "]
["轻工及机械检测中心",5,"烘箱实验"," ","埋地排水用钢带增强聚乙烯（PE）螺旋波纹管 CJ/T 225-2011　 8.4.5"," ",200," "," 塑料管材——埋地排水用钢带增强聚乙烯（PE）螺旋波纹管  "]
["轻工及机械检测中心",6,"冲击性能"," ","热塑性塑料管材耐性外冲击性能 试验方法 时针旋转法 GB/T14152-2001 8.10"," ",950," "," 塑料管材——埋地排水用钢带增强聚乙烯（PE）螺旋波纹管  "]
["轻工及机械检测中心",1,"外观"," ","聚乙烯塑钢缠绕排水管　 CJ/T　270-2017 7.2"," ",50," "," 塑料管材——聚乙烯塑钢缠绕管  "]
["轻工及机械检测中心",2,"平均内径"," ","聚乙烯塑钢缠绕排水管　 CJ/T　270-2017 7.3"," ",50," "," 塑料管材——聚乙烯塑钢缠绕管  "]
["轻工及机械检测中心",3,"环刚度"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.9"," ",400," "," 塑料管材——聚乙烯塑钢缠绕管  "]
["轻工及机械检测中心",4,"环柔性"," ","热塑性塑料管材 环刚度的测定 GB/T9647-2015 8.11"," ",200," "," 塑料管材——聚乙烯塑钢缠绕管  "]
["轻工及机械检测中心",5,"烘箱实验"," ","聚乙烯塑钢缠绕排水管　 CJ/T　270-2017 7.4"," ",200," "," 塑料管材——聚乙烯塑钢缠绕管  "]
["轻工及机械检测中心",6,"冲击性能"," ","热塑性塑料管材耐性外冲击性能 试验方法 时针旋转法 GB/T14152-2001 8.10"," ",950," "," 塑料管材——聚乙烯塑钢缠绕管  "]
["轻工及机械检测中心",1,"外观"," ","钢丝网骨架塑料(聚乙烯)复合管材及管件  CJ/T 189-2007 7.2"," ",50," "," 塑料管材——钢丝网骨架塑料(聚乙烯)复合管材及管件  "]
["轻工及机械检测中心",2,"外径"," ","塑料管材尺寸测量方法 GB/T 8806-2008 8.3"," ",50," "," 塑料管材——钢丝网骨架塑料(聚乙烯)复合管材及管件  "]
["轻工及机械检测中心",3,"壁厚"," ","塑料管材尺寸测量方法 GB/T 8806-2008 8.3"," ",50," "," 塑料管材——钢丝网骨架塑料(聚乙烯)复合管材及管件  "]
["轻工及机械检测中心",4,"短期静液压强度"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 7.5.1"," ",615," "," 塑料管材——钢丝网骨架塑料(聚乙烯)复合管材及管件  "]
["轻工及机械检测中心",5,"受压开裂稳定性"," ","钢丝网骨架塑料(聚乙烯)复合管材及管件  CJ/T 189-2007 7.5.2"," ",300," "," 塑料管材——钢丝网骨架塑料(聚乙烯)复合管材及管件  "]
["轻工及机械检测中心",6,"爆破压试验力"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 7.5.1"," ",600," "," 塑料管材——钢丝网骨架塑料(聚乙烯)复合管材及管件  "]
["轻工及机械检测中心",7,"卫生性能","铅","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",150," "," 塑料管材——钢丝网骨架塑料(聚乙烯)复合管材及管件  "]
["轻工及机械检测中心",7,"卫生性能","镉","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",150," "," 塑料管材——钢丝网骨架塑料(聚乙烯)复合管材及管件  "]
["轻工及机械检测中心",7,"卫生性能","高锰酸钾消耗量（以氧气（O2记））","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",120," "," 塑料管材——钢丝网骨架塑料(聚乙烯)复合管材及管件  "]
["轻工及机械检测中心",1,"外观"," ","给水用硬聚氯乙烯（PVC-U）管材 GB/T 10002.1-2006 7.2"," ",50," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",2,"不透光性"," ","给水用硬聚氯乙烯（PVC-U）管材 GB/T 10002.1-2006 7.3"," ",200," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",3,"外径"," ","塑料管材尺寸测量方法 GB/T 8806-2008 7.4.3"," ",50," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",4,"壁厚"," ","塑料管材尺寸测量方法 GB/T 8806-2008 7.4.4"," ",50," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",5,"密度"," ","塑料密度和相对密度试验方法 GB/T1033-2008 6.4"," ",150," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",6,"维卡软化温度（VST）"," ","热塑性塑料光彩、管件 维卡软化温度的测定 GB/T8802-2001 6.5"," ",110," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",7,"纵向回缩率"," ","热塑性塑料管材 纵向回缩率的测定 GB/T6671-2001 6.6"," ",220," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",8,"落锤冲击试验TIR"," ","热塑性塑料管材耐性外冲击性能 试验方法 时针旋转法 GB/T14152-2001 6.9"," ",950," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",9,"二氯甲烷浸渍试验"," ","硬聚氯乙烯（PVC-U）管材 二氯甲烷浸渍试验方法 GB/T13526-2007 6.7"," ",280," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",10,"液压试验（1h 20℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 7.8"," ",615," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",11,"液压试验（100h 20℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 7.8"," ",2100," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",12,"液压试验（1000h 60℃）"," ","流体输送用热塑性塑料管材耐内压试验方法 GB/T6111-2003 7.8"," ",25600," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",13,"卫生性能","铅","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",150," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",13,"卫生性能","镉","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",150," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",13,"卫生性能","高锰酸钾消耗量（以氧气（O2记））","生活饮用水输配水设备及防护材料的安全性评价标准 GB/T17219-1998 8.10"," ",120," "," 塑料管材——给水用硬聚氯乙烯（PVC-U）管材  "]
["轻工及机械检测中心",1,"颜色"," ","QB/T 2479-2005 5.2",null,50," "," 塑料管材——pvc-c套管"]
["轻工及机械检测中心",2,"外观"," ","QB/T 2479-2005 5.2",null,50," "," 塑料管材——pvc-c套管"]
["轻工及机械检测中心",3,"平均外径"," ","GB/T 8806-1988",null,100," "," 塑料管材——pvc-c套管"]
["轻工及机械检测中心",4,"壁厚偏差"," ","GB/T 8806-1988",null,100," "," 塑料管材——pvc-c套管"]
["轻工及机械检测中心",5,"弯曲度"," ","GB/T 8805-1988",null,100," "," 塑料管材——pvc-c套管"]
["轻工及机械检测中心",6,"维卡软化温度"," ","GB/T 8802-2001",null,300," "," 塑料管材——pvc-c套管"]
["轻工及机械检测中心",7,"环段热压缩力"," ","GB/T 9467-2003",null,500," "," 塑料管材——pvc-c套管"]
["轻工及机械检测中心",8,"落锤冲击试验"," ","GB/T 14152-2001",null,800," "," 塑料管材——pvc-c套管"]
["轻工及机械检测中心",9,"纵向回缩率"," ","GB/T 6671-2001",null,300," "," 塑料管材——pvc-c套管"]
["轻工及机械检测中心",1,"表面质量"," ","钢筋混凝土用钢 第2部分：热轧带肋钢筋  GB/T 1499.2-2018 7.10"," ",100," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",2,"内径偏差"," ","钢筋混凝土用钢 第2部分：热轧带肋钢筋  GB/T 1499.2-2018 8.3"," ",200," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",3,"重量偏差"," ","钢筋混凝土用钢 第2部分：热轧带肋钢筋  GB/T 1499.2-2018 8.4"," ",300," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",4,"力学性能","下屈服强度","钢筋混凝土用钢材试验方法 GB/T 28900-2012  8.2"," ",300," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",4,"力学性能","抗拉强度","钢筋混凝土用钢材试验方法 GB/T 28900-2012  8.2"," ",300," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",4,"力学性能","断后伸长率","钢筋混凝土用钢材试验方法 GB/T 28900-2012  8.2"," ",200," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",5,"弯曲性能"," ","钢筋混凝土用钢材试验方法 GB/T 28900-2012  8.2"," ",300," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",6,"反向弯曲性能"," ","钢筋混凝土用钢材试验方法 GB/T 28900-2012  8.2"," ",300," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",7,"化学成分","C","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",7,"化学成分","Si","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",7,"化学成分","Mn","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",7,"化学成分","P","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",7,"化学成分","S","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",7,"化学成分","Ceq","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",840," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",8,"最大力总延伸率"," ","GB/T 28900-2022"," ",400," "," 金属材料及制品——热轧带肋钢筋  "]
["轻工及机械检测中心",1,"表面质量"," ","钢筋混凝土用钢 第2部分：热轧带肋钢筋  GB/T 1499.1-2017 7.10"," ",50," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",2,"公称直径"," ","钢筋混凝土用钢 第2部分：热轧带肋钢筋  GB/T 1499.1-2017 8.3"," ",100," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",3,"重量偏差"," ","钢筋混凝土用钢 第2部分：热轧带肋钢筋  GB/T 1499.1-2017 8.4"," ",100," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",4,"力学性能","下屈服强度","钢筋混凝土用钢材试验方法 GB/T 28900-2012  8.2"," ",200," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",4,"力学性能","抗拉强度","钢筋混凝土用钢材试验方法 GB/T 28900-2012  8.2"," ",200," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",4,"力学性能","断后伸长率","钢筋混凝土用钢材试验方法 GB/T 28900-2012  8.2"," ",100," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",5,"弯曲性能"," ","钢筋混凝土用钢材试验方法 GB/T 28900-2012  8.2"," ",200," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",6,"化学成分","C","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",6,"化学成分","Si","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",6,"化学成分","Mn","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",6,"化学成分","P","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",6,"化学成分","S","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——热轧光圆钢筋  "]
["轻工及机械检测中心",1,"力学性能","屈服强度","金属材料 室温拉伸试验方法 GB/T 228.1-2010 5.4"," ",200," "," 金属材料及制品——碳素结构钢  "]
["轻工及机械检测中心",1,"力学性能","抗拉强度","金属材料 室温拉伸试验方法 GB/T 228.1-2010 5.4"," ",200," "," 金属材料及制品——碳素结构钢  "]
["轻工及机械检测中心",1,"力学性能","断后伸长率","金属材料 室温拉伸试验方法 GB/T 228.1-2010 5.4"," ",100," "," 金属材料及制品——碳素结构钢  "]
["轻工及机械检测中心",2,"冷弯试验"," ","金属材料 弯曲试验方法 GB/T 232-2010 5.4"," ",200," "," 金属材料及制品——碳素结构钢  "]
["轻工及机械检测中心",3,"化学成分","C","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——碳素结构钢  "]
["轻工及机械检测中心",3,"化学成分","Si","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——碳素结构钢  "]
["轻工及机械检测中心",3,"化学成分","Mn","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——碳素结构钢  "]
["轻工及机械检测中心",3,"化学成分","P","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——碳素结构钢  "]
["轻工及机械检测中心",3,"化学成分","S","碳素钢和中低合金钢火花源原子发射光谱分析法（常规法） GB/T 4336-2016 7.1.1"," ",120," "," 金属材料及制品——碳素结构钢  "]
["轻工及机械检测中心",1,"外观质量"," ","铝合金建筑型材 第2部分：阳极氧化型材 GB/T 5237.2-2017"," ",50," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",2,"壁厚偏差"," ","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 5.3"," ",50," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",3,"膜厚","平均膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",3,"膜厚","局部膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",5,"力学性能","规定非比例延伸强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",5,"力学性能","抗拉强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",5,"力学性能","断后伸长率","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",100," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",6,"化学成分","Si","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",6,"化学成分","Fe","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",6,"化学成分","Cu","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",6,"化学成分","Mn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",6,"化学成分","Mg","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",6,"化学成分","Cr","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",6,"化学成分","Zn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",6,"化学成分","Ti","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——阳极氧化型材"]
["轻工及机械检测中心",1,"外观质量"," ","铝合金建筑型材 第3部分：电泳涂漆型材 GB/T 5237.3-2017"," ",50," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",2,"壁厚偏差"," ","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 5.3"," ",50," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",3,"膜厚","阳极氧化局部膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",3,"膜厚","漆膜局部膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",3,"膜厚","复合膜局部膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",4,"漆膜硬度"," ","色漆和清漆 铅笔法测定漆膜硬度 GB/T 6739-2006 5.4.3"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",5,"漆膜附着性","干附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",5,"漆膜附着性","湿附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",6,"力学性能","规定非比例延伸强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",6,"力学性能","抗拉强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",6,"力学性能","断后伸长率","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",100," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",7,"耐沸水性"," ","铝合金建筑型材 第3部分：电泳涂漆型材 GB/T 5237.3-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",8,"耐盐酸性"," ","铝合金建筑型材 第3部分：电泳涂漆型材 GB/T 5237.3-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",9,"耐碱性"," ","铝合金建筑型材 第3部分：电泳涂漆型材 GB/T 5237.3-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",10,"化学成分","Si","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",10,"化学成分","Fe","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",10,"化学成分","Cu","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",10,"化学成分","Mn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",10,"化学成分","Mg","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",10,"化学成分","Cr","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",10,"化学成分","Zn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",10,"化学成分","Ti","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——电泳涂漆型材"]
["轻工及机械检测中心",1,"外观质量"," ","铝合金建筑型材 第4部分：喷粉型材 GB/T 5237.4-2017"," ",50," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",2,"壁厚偏差"," ","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 5.3"," ",50," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",3,"力学性能","规定非比例延伸强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",3,"力学性能","抗拉强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",3,"力学性能","断后伸长率","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",100," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",4,"膜厚","局部膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",4,"膜厚","平均膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",5,"附着性","干附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",5,"附着性","湿附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",5,"附着性","沸水附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",6,"耐沸水性"," ","铝合金建筑型材 第4部分：喷粉型材 GB/T 5237.4-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",7,"耐冲击性"," ","铝合金建筑型材 第4部分：喷粉型材 GB/T 5237.4-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",8,"抗弯曲性"," ","铝合金建筑型材 第4部分：喷粉型材 GB/T 5237.4-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",9,"耐盐酸性"," ","铝合金建筑型材 第4部分：喷粉型材 GB/T 5237.4-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",10,"化学成分","Si","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",10,"化学成分","Fe","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",10,"化学成分","Cu","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",10,"化学成分","Mn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",10,"化学成分","Mg","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",10,"化学成分","Cr","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",10,"化学成分","Zn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",10,"化学成分","Ti","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷粉型材"]
["轻工及机械检测中心",1,"外观质量"," ","铝合金建筑型材 第5部分：喷漆型材 GB/T 5237.5-2017"," ",50," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",2,"壁厚偏差"," ","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 5.3"," ",50," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",3,"力学性能","规定非比例延伸强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",3,"力学性能","抗拉强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",3,"力学性能","断后伸长率","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",100," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",4,"膜厚","局部膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",4,"膜厚","平均膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",5,"硬度"," ","色漆和清漆 铅笔法测定漆膜硬度 GB/T 6739-2006 5.4.3"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",6,"附着性","干附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",6,"附着性","湿附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",6,"附着性","沸水附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",7,"耐沸水性"," ","铝合金建筑型材 第5部分：喷漆型材 GB/T 5237.5-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",8,"耐冲击性"," ","铝合金建筑型材 第5部分：喷漆型材 GB/T 5237.5-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",9,"耐盐酸性"," ","铝合金建筑型材 第5部分：喷漆型材 GB/T 5237.5-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",10,"化学成分","Si","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",10,"化学成分","Fe","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",10,"化学成分","Cu","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",10,"化学成分","Mn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",10,"化学成分","Mg","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",10,"化学成分","Cr","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",10,"化学成分","Zn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",10,"化学成分","Ti","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——喷漆型材"]
["轻工及机械检测中心",1,"外观质量"," ","铝合金建筑型材 第6部分：隔热型材 GB/T 5237.6-2017"," ",50," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",2,"壁厚偏差"," ","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 5.3"," ",50," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",3,"力学性能","规定非比例延伸强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",3,"力学性能","抗拉强度","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",3,"力学性能","断后伸长率","铝合金建筑型材 第1部分：基材 GB/T  5237.1-2017 4.5"," ",100," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",4,"室温纵向抗剪特征值"," ","铝合金隔热型材复合性能试验方法  GB/T 28289-2012"," ",500," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",5,"室温横向抗拉特征值"," ","铝合金隔热型材复合性能试验方法  GB/T 28289-2012"," ",500," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",6,"膜厚","局部膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",6,"膜厚","平均膜厚","非磁性基体金属上非导电覆盖层 覆盖层厚度测量 涡流法 GB/T 4957-2003 5.4.1"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",7,"附着性","干附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",7,"附着性","湿附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",7,"附着性","沸水附着性","色漆和清漆 漆膜的划格试验GB/T 9286-1998"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",8,"耐沸水性"," ","铝合金建筑型材 第6部分：隔热型材 GB/T 5237.6-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",9,"耐冲击性"," ","铝合金建筑型材 第6部分：隔热型材 GB/T 5237.6-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",10,"抗弯曲性"," ","铝合金建筑型材 第6部分：隔热型材 GB/T 5237.6-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",11,"耐盐酸性"," ","铝合金建筑型材 第6部分：隔热型材 GB/T 5237.6-2017"," ",200," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",12,"化学成分","Si","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",12,"化学成分","Fe","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",12,"化学成分","Cu","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",12,"化学成分","Mn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",12,"化学成分","Mg","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",12,"化学成分","Cr","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",12,"化学成分","Zn","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",12,"化学成分","Ti","铝及铝合金化学分析方法 第1部分：汞含量的测定 冷原子吸收光谱法  GB/T 20975.1-2007 5.1"," ",120," "," 金属材料及制品——铝合金建筑型材——隔热型材"]
["轻工及机械检测中心",1,"外观要求"," ","包装容器 钢提桶 GB/T 13252-2008 "," ",50," "," 金属材料及制品——钢提桶  "]
["轻工及机械检测中心",2,"气密性能"," ","包装 包装容器 气密试验方法 GB/T 17344-1998"," ",200," "," 金属材料及制品——钢提桶  "]
["轻工及机械检测中心",3,"耐液压性"," ","包装容器 钢提桶 GB/T 13252-2008 "," ",200," "," 金属材料及制品——钢提桶  "]
["轻工及机械检测中心",4,"耐跌落性"," ","包装 运输包装件 跌落试验方法 GB/T 4857.5-1992 "," ",200," "," 金属材料及制品——钢提桶  "]
["轻工及机械检测中心",5,"耐堆码性"," ","包装 运输包装件 第3部分：静载荷堆码试验方法 GB/T 4857.3-2008"," ",200," "," 金属材料及制品——钢提桶  "]
["轻工及机械检测中心",6,"提梁、提环强度"," ","包装容器 钢提桶 GB/T 13252-2008 "," ",200," "," 金属材料及制品——钢提桶  "]
["轻工及机械检测中心",7,"涂膜附着力"," ","漆膜附着力测定法 GB/T 1720-1979"," ",200," "," 金属材料及制品——钢提桶  "]
["轻工及机械检测中心",1,"外观要求"," ","包装容器工业用薄钢板圆罐  GB/T 15170-2007"," ",50," "," 金属材料及制品——工业用薄钢板圆罐  "]
["轻工及机械检测中心",2,"气密试验"," ","包装 包装容器 气密试验方法 GB/T 17344-1998"," ",200," "," 金属材料及制品——工业用薄钢板圆罐  "]
["轻工及机械检测中心",3,"液压实验"," ","包装容器工业用薄钢板圆罐  GB/T 15170-2007"," ",200," "," 金属材料及制品——工业用薄钢板圆罐  "]
["轻工及机械检测中心",4,"跌落实验"," ","包装 运输包装件 跌落试验方法 GB/T 4857.5-1992 "," ",200," "," 金属材料及制品——工业用薄钢板圆罐  "]
["轻工及机械检测中心",5,"堆码试验"," ","包装 运输包装件 第3部分：静载荷堆码试验方法 GB/T 4857.3-2008"," ",200," "," 金属材料及制品——工业用薄钢板圆罐  "]
["轻工及机械检测中心",6,"提梁、提环强度试验"," ","包装容器工业用薄钢板圆罐  GB/T 15170-2007"," ",200," "," 金属材料及制品——工业用薄钢板圆罐  "]
["轻工及机械检测中心",1,"外观要求"," ","包装容器 方罐与扁圆罐  BB/T0019-2013 "," ",50," "," 金属材料及制品——方罐与扁圆罐  "]
["轻工及机械检测中心",2,"气密试验"," ","包装 包装容器 气密试验方法 GB/T 17344-1998"," ",200," "," 金属材料及制品——方罐与扁圆罐  "]
["轻工及机械检测中心",3,"液压实验"," ","包装容器 方罐与扁圆罐  BB/T0019-2013 "," ",200," "," 金属材料及制品——方罐与扁圆罐  "]
["轻工及机械检测中心",4,"跌落实验"," ","包装 运输包装件 跌落试验方法 GB/T 4857.5-1992 "," ",200," "," 金属材料及制品——方罐与扁圆罐  "]
["轻工及机械检测中心",5,"堆码试验"," ","包装 运输包装件 第3部分：静载荷堆码试验方法 GB/T 4857.3-2008"," ",200," "," 金属材料及制品——方罐与扁圆罐  "]
["轻工及机械检测中心",6,"提梁、提环强度试验"," ","包装容器 方罐与扁圆罐  BB/T0019-2013 "," ",200," "," 金属材料及制品——方罐与扁圆罐  "]
["轻工及机械检测中心",1,"产品标记"," ","钢管脚手架扣件 GB 15831-2006"," ",50," "," 金属材料及制品——钢管脚手架扣件——直角扣件"]
["轻工及机械检测中心",2,"抗滑性能试验"," ","钢管脚手架扣件 GB 15831-2006"," ",600," "," 金属材料及制品——钢管脚手架扣件——直角扣件"]
["轻工及机械检测中心",3,"抗破坏性能试验"," ","钢管脚手架扣件 GB 15831-2006"," ",200," "," 金属材料及制品——钢管脚手架扣件——直角扣件"]
["轻工及机械检测中心",4,"扭转刚度性能试验"," ","钢管脚手架扣件 GB 15831-2006"," ",400," "," 金属材料及制品——钢管脚手架扣件——直角扣件"]
["轻工及机械检测中心",1,"产品标记"," ","钢管脚手架扣件 GB 15831-2006"," ",50," "," 金属材料及制品——钢管脚手架扣件——旋转扣件"]
["轻工及机械检测中心",2,"抗滑性能试验"," ","钢管脚手架扣件 GB 15831-2006"," ",600," "," 金属材料及制品——钢管脚手架扣件——旋转扣件"]
["轻工及机械检测中心",3,"抗破坏性能试验"," ","钢管脚手架扣件 GB 15831-2006"," ",200," "," 金属材料及制品——钢管脚手架扣件——旋转扣件"]
["轻工及机械检测中心",1,"产品标记"," ","钢管脚手架扣件 GB 15831-2006"," ",50," "," 金属材料及制品——钢管脚手架扣件——对接扣件"]
["轻工及机械检测中心",2,"抗拉性能试验"," ","钢管脚手架扣件 GB 15831-2006"," ",800," "," 金属材料及制品——钢管脚手架扣件——对接扣件"]
["轻工及机械检测中心",1,"外观质量"," ","GB/T 23444-2024 7.3"," ",50," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",2,"尺寸偏差","最小厚度  ","GB/T 23444-2024 7.4"," ",100," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",2,"尺寸偏差","长度偏差","GB/T 23444-2024 7.4"," ",100," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",2,"尺寸偏差","宽度偏差","GB/T 23444-2024 7.4"," ",100," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",2,"尺寸偏差","折边高度偏差","GB/T 23444-2024 7.4"," ",100," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",2,"尺寸偏差","挠度","GB/T23444-2024 7.4.5"," ",100," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",2,"尺寸偏差","棱边最大弯曲","GB/T 23444-2024 7.4.4"," ",100," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",3,"膜厚","平均膜厚","GB/T 4957-2003 "," ",200," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",3,"膜厚","最小局部膜厚","GB/T 4957-2003 "," ",200," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",4,"60°光泽度偏差"," ","GB/T 9754-2007"," ",200," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",5,"附着力"," ","GB/T 9286-2021"," ",200," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",6,"漆膜硬度"," ","GB/T 6739-2022"," ",200," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",7,"耐冲击性"," ","GB/T 23444-2024 7.9"," ",200," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",8,"耐酸性"," ","GB/T 23444-2024 7.10"," ",200," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",9,"耐碱性"," ","GB/T 23444-2024 7.10"," ",200," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",10,"耐油性"," ","GB/T 23444-2024 7.10"," ",200," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",12,"耐沸水性"," ","GB/T 23444-2024 7.13"," ",500," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",13,"平面拉伸粘结强度"," ","GB/T 1452-2018","GB/T 1452-2018",800," "," 金属材料及制品——金属及金属复合材料吊顶板  "]
["轻工及机械检测中心",1,"力学性能","下屈服强度"," GB/T 228.1-2021"," ",200," "," 金属材料及制品——冷弯型钢"]
["轻工及机械检测中心",1,"力学性能","抗拉强度","GB/T 228.1-2021"," ",200," "," 金属材料及制品——冷弯型钢"]
["轻工及机械检测中心",1,"力学性能","断后伸长率"," GB/T 228.1-2021"," ",100," "," 金属材料及制品——冷弯型钢"]
["轻工及机械检测中心",2,"表面质量"," ","GB/T 6725-2017 条款7"," ",100," "," 金属材料及制品——冷弯型钢"]
["轻工及机械检测中心",3,"尺寸"," ","GB/T 6725-2017 条款7"," ",200," "," 金属材料及制品——冷弯型钢"]
["轻工及机械检测中心",4,"镀锌层厚度（实测值）"," ","GB/T 4956-2003"," ",300,"只出实测值不下结论"," 金属材料及制品——冷弯型钢"]
["轻工及机械检测中心",1,"外观"," ","检查井盖 GB/T 23858-2009 "," ",50," "," 机械产品——检查井盖  "]
["轻工及机械检测中心",2,"嵌入深度"," ","检查井盖 GB/T 23858-2009 "," ",100," "," 机械产品——检查井盖  "]
["轻工及机械检测中心",3,"总间隙"," ","检查井盖 GB/T 23858-2009 "," ",100," "," 机械产品——检查井盖  "]
["轻工及机械检测中心",4,"井座支承面宽度"," ","检查井盖 GB/T 23858-2009 "," ",100," "," 机械产品——检查井盖  "]
["轻工及机械检测中心",5,"承载能力","承载能力试验","检查井盖 GB/T 23858-2009 "," ",800," "," 机械产品——检查井盖  "]
["轻工及机械检测中心",5,"承载能力","残留变形","检查井盖 GB/T 23858-2009 "," ",200," "," 机械产品——检查井盖  "]
["轻工及机械检测中心",1,"全项"," ","GB 17565-2007-防盗安全门通用技术条件"," ",2500," "," 机械产品——防盗安全门"]
["轻工及机械检测中心",1,"尺寸","壁厚","GB/T 3091-2015",null,50," "," 机械产品——焊接钢管"]
["轻工及机械检测中心",1,"尺寸","外径","GB/T 3091-2015",null,50," "," 机械产品——焊接钢管"]
["轻工及机械检测中心",1,"尺寸","不圆度","GB/T 3091-2015",null,50," "," 机械产品——焊接钢管"]
["轻工及机械检测中心",2,"力学性能","下屈服强度","GB/T 3091-2015",null,200," "," 机械产品——焊接钢管"]
["轻工及机械检测中心",2,"力学性能","抗拉强度","GB/T 3091-2015",null,200," "," 机械产品——焊接钢管"]
["轻工及机械检测中心",2,"力学性能","断后伸长率","GB/T 3091-2015",null,100," "," 机械产品——焊接钢管"]
["轻工及机械检测中心",3,"化学分析"," ","GB/T 3091-2015",null,120," "," 机械产品——焊接钢管"]
["轻工及机械检测中心",1,"外观质量",null,"塑料编织袋通用技术要求 GB/T 8946-2013 "," ",100," "," 其他——塑料编织袋  "]
["轻工及机械检测中心",2,"有效长度偏差"," ","塑料编织袋通用技术要求 GB/T 8946-2013 "," ",100," "," 其他——塑料编织袋  "]
["轻工及机械检测中心",3,"有效宽度偏差"," ","塑料编织袋通用技术要求 GB/T 8946-2013 "," ",100," "," 其他——塑料编织袋  "]
["轻工及机械检测中心",4,"拉伸负荷","经向","塑料编织袋通用技术要求 GB/T 8946-2013 "," ",200," "," 其他——塑料编织袋  "]
["轻工及机械检测中心",4,"拉伸负荷","纬向","塑料编织袋通用技术要求 GB/T 8946-2013 "," ",200," "," 其他——塑料编织袋  "]
["轻工及机械检测中心",4,"拉伸负荷","缝底向","塑料编织袋通用技术要求 GB/T 8946-2013 "," ",200," "," 其他——塑料编织袋  "]
["轻工及机械检测中心",5,"耐热性能"," ","塑料编织袋通用技术要求 GB/T 8946-2013 "," ",200," "," 其他——塑料编织袋  "]
["轻工及机械检测中心",6,"跌落性能"," ","塑料编织袋通用技术要求 GB/T 8946-2013 "," ",200," "," 其他——塑料编织袋  "]
["轻工及机械检测中心",1,"外观"," ","包装用聚乙烯吹塑薄膜 GB/T 4456-2008 "," ",50," "," 其他——包装用聚乙烯吹塑薄膜  "]
["轻工及机械检测中心",2,"厚度极限偏差"," ","塑料薄膜和薄片厚度测定 机械测量法  GB/T 6672-2001"," ",100," "," 其他——包装用聚乙烯吹塑薄膜  "]
["轻工及机械检测中心",3,"厚度平均偏差"," ","塑料薄膜和薄片厚度测定 机械测量法  GB/T 6672-2001"," ",100," "," 其他——包装用聚乙烯吹塑薄膜  "]
["轻工及机械检测中心",4,"拉伸强度","纵向","塑料 拉伸性能的测定 第3部分：薄膜和薄片的试验条件  GB/T 1040.3-2006"," ",200," "," 其他——包装用聚乙烯吹塑薄膜  "]
["轻工及机械检测中心",4,"拉伸强度","横向","塑料 拉伸性能的测定 第3部分：薄膜和薄片的试验条件  GB/T 1040.3-2006"," ",200," "," 其他——包装用聚乙烯吹塑薄膜  "]
["轻工及机械检测中心",5,"断裂标称应变","纵向","塑料 拉伸性能的测定 第3部分：薄膜和薄片的试验条件  GB/T 1040.3-2006"," ",200," "," 其他——包装用聚乙烯吹塑薄膜  "]
["轻工及机械检测中心",5,"断裂标称应变","横向","塑料 拉伸性能的测定 第3部分：薄膜和薄片的试验条件  GB/T 1040.3-2006"," ",200," "," 其他——包装用聚乙烯吹塑薄膜  "]
["轻工及机械检测中心",6,"落镖冲击"," ","包装用聚乙烯吹塑薄膜 GB/T 4456-2008 "," ",200," "," 其他——包装用聚乙烯吹塑薄膜  "]
["轻工及机械检测中心",1,"外观"," ","通用型双向拉伸聚丙烯膜压敏胶黏带 GB/T　22378-2008 "," ",50," "," 其他——通用型双向拉伸聚丙烯膜压敏胶黏带  "]
["轻工及机械检测中心",2,"初粘力"," ","压敏胶粘带初粘性试验方法(滚球法) GB/T 4852-2002 6.5.5"," ",200," "," 其他——通用型双向拉伸聚丙烯膜压敏胶黏带  "]
["轻工及机械检测中心",3,"持粘力"," ","胶粘带持粘性的试验方法 GB/T 4851-2014 6.5.2"," ",200," "," 其他——通用型双向拉伸聚丙烯膜压敏胶黏带  "]
["轻工及机械检测中心",4,"180°剥离力","常态下","胶粘带剥离强度的试验方法    GB/T 2792-2014   6.5.1"," ",100," "," 其他——通用型双向拉伸聚丙烯膜压敏胶黏带  "]
["轻工及机械检测中心",4,"180°剥离力","湿热老化后","胶粘带剥离强度的试验方法    GB/T 2792-2014   6.5.1"," ",200," "," 其他——通用型双向拉伸聚丙烯膜压敏胶黏带  "]
["轻工及机械检测中心",5,"拉伸强度"," ","通用型双向拉伸聚丙烯膜压敏胶黏带 GB/T　22378-2008 "," ",300," "," 其他——通用型双向拉伸聚丙烯膜压敏胶黏带  "]
["轻工及机械检测中心",6,"断裂伸长率"," ","通用型双向拉伸聚丙烯膜压敏胶黏带 GB/T　22378-2008 "," ",200," "," 其他——通用型双向拉伸聚丙烯膜压敏胶黏带  "]
["轻工及机械检测中心",7,"宽度偏差"," ","通用型双向拉伸聚丙烯膜压敏胶黏带 GB/T　22378-2008 "," ",100," "," 其他——通用型双向拉伸聚丙烯膜压敏胶黏带  "]
["轻工及机械检测中心",1,"外观"," ","GB13735-2017 7.2"," ",50," "," 其他——聚乙烯农用吹塑薄膜"]
["轻工及机械检测中心",2,"厚度极限偏差"," ","GB13735-2017 7.4"," ",100," "," 其他——聚乙烯农用吹塑薄膜"]
["轻工及机械检测中心",3,"厚度平均偏差"," ","GB13735-2017 7.4"," ",100," "," 其他——聚乙烯农用吹塑薄膜"]
["轻工及机械检测中心",4,"拉伸负荷","纵向","GB13735-2017 7.6"," ",200," "," 其他——聚乙烯农用吹塑薄膜"]
["轻工及机械检测中心",4,"拉伸负荷","横向","GB13735-2017 7.6"," ",200," "," 其他——聚乙烯农用吹塑薄膜"]
["轻工及机械检测中心",5,"断裂标称应变","纵向","GB13735-2017 7.6"," ",200," "," 其他——聚乙烯农用吹塑薄膜"]
["轻工及机械检测中心",5,"断裂标称应变","横向","GB13735-2017 7.6"," ",200," "," 其他——聚乙烯农用吹塑薄膜"]
["轻工及机械检测中心",6,"直角撕裂负荷","纵向","GB13735-2017 7.7 "," ",200," "," 其他——聚乙烯农用吹塑薄膜"]
["轻工及机械检测中心",6,"直角撕裂负荷","横向","GB13735-2017 7.7"," ",200," "," 其他——聚乙烯农用吹塑薄膜"]
["轻工及机械检测中心",1,"标识要求","非食品接触用塑料购物袋","GB/T21661-2020 5.2"," ",50," "," 其他——塑料购物袋"]
["轻工及机械检测中心",1,"标识要求","环保声明","GB/T21661-2020 5.2"," ",50," "," 其他——塑料购物袋"]
["轻工及机械检测中心",1,"标识要求","安全性声明","GB/T21661-2020 5.2"," ",50," "," 其他——塑料购物袋"]
["轻工及机械检测中心",2,"尺寸偏差","厚度极限偏差","GB/T21661-2020 6.3"," ",200," "," 其他——塑料购物袋"]
["轻工及机械检测中心",2,"尺寸偏差","厚度平均偏差","GB/T21661-2020 6.3"," ",200," "," 其他——塑料购物袋"]
["轻工及机械检测中心",2,"尺寸偏差","宽度偏差","GB/T21661-2020 6.3"," ",50," "," 其他——塑料购物袋"]
["轻工及机械检测中心",2,"尺寸偏差","长度偏差","GB/T21661-2020 6.3"," ",50," "," 其他——塑料购物袋"]
["轻工及机械检测中心",3,"感官要求","颜色","GB/T21661-2020 6.5.1"," ",50," "," 其他——塑料购物袋"]
["轻工及机械检测中心",3,"感官要求","异嗅","GB/T21661-2020 6.5.2"," ",50," "," 其他——塑料购物袋"]
["轻工及机械检测中心",3,"感官要求","外观","GB/T21661-2020 6.5.1"," ",50," "," 其他——塑料购物袋"]
["轻工及机械检测中心",3,"感官要求","印刷质量","GB/T 21661-2020 6.5.3.1"," ",100," "," 其他——塑料购物袋"]
["轻工及机械检测中心",4,"跌落试验"," ","GB/T 21661-2020 6.3.9"," ",300," "," 其他——塑料购物袋"]
["轻工及机械检测中心",5,"漏水性试验"," ","GB/T 21661-2020 6.3.10"," ",300," "," 其他——塑料购物袋"]
["轻工及机械检测中心",6,"封合强度"," ","QB/T 2358-1998"," ",500," "," 其他——塑料购物袋"]
["轻工及机械检测中心",7,"落镖冲击试验"," ","GB/T 9639.1-2008 8"," ",800," "," 其他——塑料购物袋"]
["轻工及机械检测中心",8,"环保要求"," ","GB/T 21661-2020 5.2"," ",200," "," 其他——塑料购物袋"]
["轻工及机械检测中心",9,"提吊实验"," ","GB/T 21661-2020"," ",500," "," 其他——塑料购物袋"]
["轻工及机械检测中心",1,"外观"," ","CJ/T 409-2012 6.1"," ",50," "," 其他——玻璃钢化粪池"]
["轻工及机械检测中心",2,"尺寸偏差"," ","CJ/T 409-2012 6.2"," ",100," "," 其他——玻璃钢化粪池"]
["轻工及机械检测中心",3,"吸水率"," ","CJ/T 409-2012 6.6"," ",300," "," 其他——玻璃钢化粪池"]
["轻工及机械检测中心",4,"冲击强度"," ","CJ/T 409-2012 6.8"," ",300," "," 其他——玻璃钢化粪池"]
["轻工及机械检测中心",5,"渗漏试验"," ","CJ/T 409-2012 6.9"," ",500," "," 其他——玻璃钢化粪池"]
["轻工及机械检测中心",1,"外观"," ","CJ/T489-2016 6.1"," ",50," "," 其他——塑料化粪池"]
["轻工及机械检测中心",2,"构造"," ","CJ/T489-2016 6.2"," ",100," "," 其他——塑料化粪池"]
["轻工及机械检测中心",3,"尺寸偏差"," ","CJ/T489-2016 6.3"," ",150," "," 其他——塑料化粪池"]
["轻工及机械检测中心",4,"满水试验"," ","CJ/T489-2016 6.5"," ",500," "," 其他——塑料化粪池"]
["轻工及机械检测中心",5,"抗冲击"," ","GB/T14152-2001 "," ",200," "," 其他——塑料化粪池"]
["轻工及机械检测中心",1,"尺寸偏差"," ","GB/T 6672-2001"," ",300," "," 其他——日用塑料袋"]
["轻工及机械检测中心",2,"感官"," ","GB/T 24984-2010"," ",100," "," 其他——日用塑料袋"]
["轻工及机械检测中心",3,"跌落试验"," ","GB/T 24984-2010"," ",300," "," 其他——日用塑料袋"]
["轻工及机械检测中心",4,"抗渗漏性"," ","GB/T 24984-2010"," ",300," "," 其他——日用塑料袋"]
["轻工及机械检测中心",5,"封合强度"," ","QB/T 2358-1998"," ",500," "," 其他——日用塑料袋"]
["轻工及机械检测中心",6,"落镖冲击"," ","GB/T 9639.1-2008"," ",800," "," 其他——日用塑料袋"]
["轻工及机械检测中心",2,"标识"," ","GB/T 38082-2019"," ",200," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",4,"感官"," ","GB/T 38082-2019"," ",100," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",5,"尺寸偏差","厚度极限偏差","GB/T 6672-2001"," ",200," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",5,"尺寸偏差","厚度平均偏差","GB/T 6672-2001"," ",200," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",5,"尺寸偏差","宽度偏差","GB/T 6671-2001"," ",50," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",5,"尺寸偏差","长度偏差","GB/T 6672-2001"," ",50," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",6,"跌落试验"," ","GB/T 38082-2019"," ",300," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",7,"漏水性"," ","GB/T 38082-2019"," ",300," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",8,"封合强度"," ","QB/T 2358-1998"," ",500," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",9,"落镖冲击试验"," ","GB/T 9639.1-2008 "," ",800," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",10,"提吊实验"," ","GB/T 38082-2019"," ",500," "," 其他——生物降解塑料购物袋（淀粉基塑料购物袋）"]
["轻工及机械检测中心",1,"尺寸偏差"," ","GB/T 6672-2001"," ",300," "," 其他——塑料垃圾袋"]
["轻工及机械检测中心",2,"感官"," ","GB/T 24454-2009"," ",100," "," 其他——塑料垃圾袋"]
["轻工及机械检测中心",3,"抗渗漏性能"," ","GB/T 24454-2009"," ",300," "," 其他——塑料垃圾袋"]
["轻工及机械检测中心",4,"跌落性能"," ","GB/T 24454-2009"," ",500," "," 其他——塑料垃圾袋"]
["轻工及机械检测中心",5,"拉紧绳拉伸力"," ","GB/T 1040.3-2006"," ",500," "," 其他——塑料垃圾袋"]
["轻工及机械检测中心",6,"提吊实验"," ","GB/T 24454-2009"," ",500," "," 其他——塑料垃圾袋"]
["轻工及机械检测中心",1,"标识"," ","BB/T 0039-2013"," ",100," "," 其他——商品零售包装袋"]
["轻工及机械检测中心",2,"尺寸偏差"," ","GB/T 6672-2001"," ",300," "," 其他——商品零售包装袋"]
["轻工及机械检测中心",3,"感官与外观质量"," ","BB/T 0039-2013"," ",100," "," 其他——商品零售包装袋"]
["轻工及机械检测中心",4,"漏水性"," ","BB/T 0039-2013"," ",300," "," 其他——商品零售包装袋"]
["轻工及机械检测中心",5,"跌落性能"," ","BB/T 0039-2013"," ",300," "," 其他——商品零售包装袋"]
["轻工及机械检测中心",6,"塑料和纸塑复合包装袋封合强度"," ","QB/T 2358-1998"," ",500," "," 其他——商品零售包装袋"]
["轻工及机械检测中心",7,"提吊实验"," ","BB/T 0039-2013  "," ",500," "," 其他——商品零售包装袋"]
["轻工及机械检测中心",1,"外观"," ","塑料垃圾桶通用技术条件 CJ/T280-2008 6.1"," ",50," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",2,"容积"," ","塑料垃圾桶通用技术条件 CJ/T280-2008 6.2"," ",200," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",3,"尺寸","宽度","塑料垃圾桶通用技术条件 CJ/T280-2008 6.3"," ",25," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",3,"尺寸","高度","塑料垃圾桶通用技术条件 CJ/T280-2008 6.3"," ",25," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",3,"尺寸","滚轮直径","塑料垃圾桶通用技术条件 CJ/T280-2008 6.3"," ",25," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",3,"尺寸","滚轮宽度","塑料垃圾桶通用技术条件 CJ/T280-2008 6.3"," ",25," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",4,"厚度","桶盖厚度","塑料垃圾桶通用技术条件 CJ/T280-2008 6.4"," ",25," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",4,"厚度","桶盖厚度","塑料垃圾桶通用技术条件 CJ/T280-2008 6.4"," ",25," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",4,"厚度","桶盖厚度","塑料垃圾桶通用技术条件 CJ/T280-2008 6.4"," ",25," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",5,"抗冷热性"," ","塑料垃圾桶通用技术条件 CJ/T280-2008 6.5.1"," ",500," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",6,"维卡软化温度"," ","热塑性塑料维卡软化温度(VST)的测定 GB/T?1633-2000 6.5.1"," ",500," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",7,"邵氏硬度"," ","塑料和硬橡胶 使用硬度计测定压痕硬度（邵氏硬度） GB/T?2411-2008 6.5.1"," ",200," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",8,"轮轴"," ","塑料垃圾桶通用技术条件 CJ/T280-2008 6.5.2"," ",50," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",9,"轮毂与辋圈"," ","塑料垃圾桶通用技术条件 CJ/T280-2008 6.5.3"," "," "," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",10,"跌落试验"," ","塑料垃圾桶通用技术条件 CJ/T280-2008 6.6 "," ",200," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",11,"重锤冲击试验"," ","塑料垃圾桶通用技术条件 CJ/T280-2008 6.6"," ",50," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",12,"台阶下落试验"," ","塑料垃圾桶通用技术条件 CJ/T280-2008 6.6"," ",1000," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",13,"滚轮承载能力试验"," ","塑料垃圾桶通用技术条件 CJ/T280-2008 6.6"," ",200," "," 塑料容器——塑料垃圾桶  "]
["轻工及机械检测中心",1,"标志、使用说明书检验"," ","不锈钢压力锅 GB 15066-2004 5.2"," ",200," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",2,"压力锅与手接触部位"," ","不锈钢压力锅 GB 15066-2004 5.3"," ",50," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",3,"抛光"," ","不锈钢压力锅 GB 15066-2004 5.4"," ",50," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",4,"容积测定"," ","不锈钢压力锅 GB 15066-2004 5.5"," ",100," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",5,"组件"," ","不锈钢压力锅 GB 15066-2004 5.6"," ",50," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",6,"手柄个数"," ","不锈钢压力锅 GB 15066-2004 5.7.1"," ",50," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",7,"手柄结构"," ","不锈钢压力锅 GB 15066-2004 5.7.2"," ",50," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",8,"手柄连接牢固性"," ","不锈钢压力锅 GB 15066-2004 5.7.3"," ",100," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",9,"手柄温升"," ","不锈钢压力锅 GB 15066-2004 5.7.4"," ",300," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",10,"合盖安全性"," ","不锈钢压力锅 GB 15066-2004 5.8"," ",500," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",11,"工作压力"," ","不锈钢压力锅 GB 15066-2004 5.9"," ",500," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",12,"密封性能"," ","不锈钢压力锅 GB 15066-2004 5.11"," ",500," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",13,"安全压力"," ","不锈钢压力锅 GB 15066-2004 5.12"," ",500," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",14,"耐热压"," ","不锈钢压力锅 GB 15066-2004 5.13"," ",500," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",15,"开盖安全性"," ","不锈钢压力锅 GB 15066-2004 5.14"," ",300," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",16,"防堵安全性"," ","不锈钢压力锅 GB 15066-2004 5.15"," ",300," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",17,"耐内压力"," ","不锈钢压力锅 GB 15066-2004 5.16"," ",500," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",18,"泄压压力"," ","不锈钢压力锅 GB 15066-2004 5.17"," ",800," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",19,"复合底"," ","不锈钢压力锅 GB 15066-2004 5.18"," ",800," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",20,"破坏压力"," ","不锈钢压力锅 GB 15066-2004 5.19"," ",800," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",21,"钢制件"," ","轻工产品金属镀层和化学处理层的耐腐蚀试验方法 中性盐雾试验(NSS)法 QB/T 3826-1999 5.20"," ",800," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",22,"塑料件耐煮性"," ","不锈钢压力锅 GB 15066-2004 5.21"," ",300," "," 不锈钢食具容器——不锈钢压力锅  "]
["轻工及机械检测中心",1,"标志、说明书检查"," ","铝压力锅安全及性能要求 GB?13623-2003 5.2"," ",200," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",2,"外观"," ","铝压力锅安全及性能要求 GB?13623-2003 5.3"," ",100," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",3,"组件"," ","铝压力锅安全及性能要求 GB?13623-2003 5.4"," ",100," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",4,"手柄结构"," ","铝压力锅安全及性能要求 GB?13623-2003 5.5"," ",100," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",5,"容积测定"," ","铝压力锅安全及性能要求 GB?13623-2003 5.6"," ",100," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",6,"表面处理"," ","铝压力锅安全及性能要求 GB?13623-2003 5.7"," ",300," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",7,"手柄连接牢固性"," ","铝压力锅安全及性能要求 GB?13623-2003 5.8"," ",100," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",8,"手柄温升"," ","铝压力锅安全及性能要求 GB?13623-2003 5.9"," ",300," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",9,"合盖安全性"," ","铝压力锅安全及性能要求 GB?13623-2003 5.10"," ",500," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",10,"工作压力"," ","铝压力锅安全及性能要求 GB?13623-2003 5.11"," ",500," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",11,"限压阀体"," ","铝压力锅安全及性能要求 GB?13623-2003 5.12"," ",100," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",12,"密封性能"," ","铝压力锅安全及性能要求 GB?13623-2003 5.13"," ",500," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",13,"安全压力"," ","铝压力锅安全及性能要求 GB?13623-2003 5.14"," ",500," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",14,"耐热压"," ","铝压力锅安全及性能要求 GB?13623-2003 5.15"," ",500," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",15,"开盖安全性"," ","铝压力锅安全及性能要求 GB?13623-2003 5.16"," ",300," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",16,"防堵安全性"," ","铝压力锅安全及性能要求 GB?13623-2003 5.17"," ",300," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",17,"耐内压力"," ","铝压力锅安全及性能要求 GB?13623-2003 5.18"," ",500," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",18,"泄压压力"," ","铝压力锅安全及性能要求 GB?13623-2003 5.19"," ",800," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",19,"钢制件"," ","铝压力锅安全及性能要求 GB?13623-2003 5.20"," ",800," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",20,"塑料件耐煮性"," ","铝压力锅安全及性能要求 GB?13623-2003 5.21"," ",300," "," 铝制食具容器——铝压力锅  "]
["轻工及机械检测中心",1,"外观"," ","卫生洁具 软管 GB/T?23448-2009 6.1"," ",100," "," 卫生洁具——卫生洁具 软管  "]
["轻工及机械检测中心",2,"长度允许偏差"," ","卫生洁具 软管 GB/T?23448-2009 6.2"," ",100," "," 卫生洁具——卫生洁具 软管  "]
["轻工及机械检测中心",3,"螺纹连接"," ","卫生洁具 软管 GB/T?23448-2009 6.3"," ",300," "," 卫生洁具——卫生洁具 软管  "]
["轻工及机械检测中心",4,"密封性"," ","卫生洁具 软管 GB/T?23448-2009 6.4"," ",200," "," 卫生洁具——卫生洁具 软管  "]
["轻工及机械检测中心",5,"耐压性"," ","卫生洁具 软管 GB/T?23448-2009 6.4"," ",300," "," 卫生洁具——卫生洁具 软管  "]
["轻工及机械检测中心",1,"外观"," ","陶瓷片密封水嘴 GB?18145-2014 7.1"," ",100," "," 卫生洁具——陶瓷片密封水嘴  "]
["轻工及机械检测中心",2,"螺纹","螺纹精度","陶瓷片密封水嘴 GB?18145-2014 7.2"," ",50," "," 卫生洁具——陶瓷片密封水嘴  "]
["轻工及机械检测中心",2,"螺纹","螺纹表面","陶瓷片密封水嘴 GB?18145-2014 7.2"," ",50," "," 卫生洁具——陶瓷片密封水嘴  "]
["轻工及机械检测中心",3,"装配"," ","陶瓷片密封水嘴 GB?18145-2014 7.3"," ",100," "," 卫生洁具——陶瓷片密封水嘴  "]
["轻工及机械检测中心",4,"尺寸"," ","陶瓷片密封水嘴 GB?18145-2014 7.5"," ",100," "," 卫生洁具——陶瓷片密封水嘴  "]
["轻工及机械检测中心",5,"抗水压机械性能","阀芯上游","陶瓷片密封水嘴 GB?18145-2014 7.6.1"," ",200," "," 卫生洁具——陶瓷片密封水嘴  "]
["轻工及机械检测中心",5,"抗水压机械性能","阀芯下游（带流量调节器）","陶瓷片密封水嘴 GB?18145-2014 7.6.1"," ",200," "," 卫生洁具——陶瓷片密封水嘴  "]
["轻工及机械检测中心",6,"密封性能","阀芯及阀芯上游","陶瓷片密封水嘴 GB?18145-2014 7.6.2"," ",200," "," 卫生洁具——陶瓷片密封水嘴  "]
["轻工及机械检测中心",6,"密封性能","阀芯下游（出水口能够被堵住）","陶瓷片密封水嘴 GB?18145-2014 7.6.2"," ",200," "," 卫生洁具——陶瓷片密封水嘴  "]
["轻工及机械检测中心",1,"感官质量","杯体外表面","双层玻璃口杯 QB/T?5035-2017 5.1"," ",15," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",1,"感官质量","杯体内表面","双层玻璃口杯 QB/T?5035-2017 5.1"," ",15," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",1,"感官质量","杯盖","双层玻璃口杯 QB/T?5035-2017 5.1"," ",15," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",1,"感官质量","印刷字迹及图案","双层玻璃口杯 QB/T?5035-2017 5.1"," ",15," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",1,"感官质量","杯体内外壁","双层玻璃口杯 QB/T?5035-2017 5.1"," ",15," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",1,"感官质量","杯体中气泡、杂粒","双层玻璃口杯 QB/T?5035-2017 5.1"," ",15," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",1,"感官质量","异味","双层玻璃口杯 QB/T?5035-2017 5.1"," ",15," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",2,"冲击温差试验"," ","实验室玻璃仪器 热冲击和热冲击强度试验方法 GB/T?6579-2007 5.2"," ",500," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",3,"卫生指标"," ","玻璃容器 铅、镉溶出量的测定方法 GB/T?21170-2007 5.3"," ",1000," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",4,"容量"," ","双层玻璃口杯 QB/T?5035-2017 5.4.1"," ",100," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",5,"稳定性"," ","双层玻璃口杯 QB/T?5035-2017 5.4.2"," ",50," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",6,"外表面温度"," ","双层玻璃口杯 QB/T?5035-2017 5.4.3"," ",100," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",7,"密封性能"," ","双层玻璃口杯 QB/T?5035-2017 5.4.4"," ",100," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",8,"橡胶件耐热水"," ","双层玻璃口杯 QB/T?5035-2017 5.4.5"," ",100," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",9,"盖与杯的配合"," ","双层玻璃口杯 QB/T?5035-2017 5.4.6"," ",50," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",10,"手柄"," ","双层玻璃口杯 QB/T?5035-2017 5.4.7"," ",100," "," 玻璃容器——双层玻璃口杯  "]
["轻工及机械检测中心",1,"最小板材厚度"," ","电缆桥架 QB/T?1453-2003 4.1.2"," ",200," "," 电缆桥架——电缆桥架  "]
["轻工及机械检测中心",2,"承载能力"," ","电缆桥架 QB/T?1453-2003 4.2"," ",800," "," 电缆桥架——电缆桥架  "]
["轻工及机械检测中心",3,"锌层厚度"," ","磁性基体上非磁性覆盖层 覆盖层厚度测量 磁性法 GB/T 4956-2003 4.3.1"," ",300," "," 电缆桥架——电缆桥架  "]
["轻工及机械检测中心",4,"涂层厚度"," ","色漆和清漆 漆膜厚度的测定 GB/T?13452.2-2008 4.3.2"," ",300," "," 电缆桥架——电缆桥架  "]
["轻工及机械检测中心",5,"外观"," ","电缆桥架 QB/T?1453-2003 4.2"," ",100," "," 电缆桥架——电缆桥架  "]
["轻工及机械检测中心",1,"外观","表面","手动密集书架 GB/T?13667.3-2013 5.1"," ",25," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",1,"外观","焊接件","手动密集书架 GB/T?13667.3-2013 5.1"," ",25," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",1,"外观","表面涂层","手动密集书架 GB/T?13667.3-2013 5.1"," ",25," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",1,"外观","电镀件镀层","手动密集书架 GB/T?13667.3-2013 5.1"," ",25," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",2,"表面涂层理化性能","冲击强度","色漆和清漆 漆膜的划格试验 GB/T?9286-1998 5.2"," ",100," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",2,"表面涂层理化性能","附着力","色漆和清漆 漆膜的划格试验 GB/T?9286-1998 5.2"," ",100," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",2,"表面涂层理化性能","耐腐蚀","色漆和清漆 漆膜的划格试验 GB/T?9286-1998 5.2"," ",100," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","外形尺寸偏差","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","外形尺寸偏差","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","外形尺寸偏差","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","导轨偏差","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","导轨偏差","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","导轨偏差","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","导轨偏差","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","导轨偏差","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","立柱与底梁的垂直度","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","架列侧面相邻两平面的位差度 ","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","侧面板和中腰板对缝处的间隙","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","防尘门缝间隙","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","可调性    ","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","互换性","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","传动装置的性能","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","防倾倒","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","限位","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",3,"装配要求","固定","手动密集书架 GB/T?13667.3-2013 5.3"," ",50," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",4,"载重性能"," ","手动密集书架 GB/T?13667.3-2013 5.4"," ",100," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",5,"稳定性"," ","手动密集书架 GB/T?13667.3-2013 5.5"," ",100," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",6,"结构强度"," ","手动密集书架 GB/T?13667.3-2013 5.6"," ",100," "," 办公用品——手动密集书架  "]
["轻工及机械检测中心",1,"外形尺寸偏差"," ","钢制书柜、资料柜通用技术条件 GB/T 13668-2015 4.1"," ",50," "," 办公用品——钢制书柜、资料柜  "]
["轻工及机械检测中心",2,"形状和位置偏差"," ","钢制书柜、资料柜通用技术条件 GB/T 13668-2015 4.2"," ",100," "," 办公用品——钢制书柜、资料柜  "]
["轻工及机械检测中心",3,"外观"," ","钢制书柜、资料柜通用技术条件 GB/T 13668-2015 4.3"," ",100," "," 办公用品——钢制书柜、资料柜  "]
["轻工及机械检测中心",4,"钢板厚度"," ","钢制书柜、资料柜通用技术条件 GB/T 13668-2015 4.4"," ",50," "," 办公用品——钢制书柜、资料柜  "]
["轻工及机械检测中心",5,"表面理化性能"," ","轻工产品金属镀层和化学处理层的耐腐蚀性试验方法 中性盐雾试验 QB/T 3826-1999 4.5"," ",200," "," 办公用品——钢制书柜、资料柜  "]
["轻工及机械检测中心",6,"其它要求"," ","钢制书柜、资料柜通用技术条件 GB/T 13668-2015 4.6"," ",100," "," 办公用品——钢制书柜、资料柜  "]
["轻工及机械检测中心",7,"稳定性"," ","钢制书柜、资料柜通用技术条件 GB/T 13668-2015 4.7"," ",100," "," 办公用品——钢制书柜、资料柜  "]
["轻工及机械检测中心",1,"壳体试验"," ","GB/T13927-2022 6.1"," ",400," "," 工业阀门——阀门  "]
["轻工及机械检测中心",2,"上密封试验"," ","GB/T13927-2022 6.2"," ",400," "," 工业阀门——阀门  "]
["轻工及机械检测中心",3,"密封试验"," ","GB/T13927-2022 6.3"," ",400," "," 工业阀门——阀门  "]
["轻工及机械检测中心",1,"形式尺寸"," ","卫生洁具及暖气管道用直角阀 GB/T26712-2011 4.1"," ",100," "," 卫生洁具——直角阀  "]
["轻工及机械检测中心",2,"加工与装配"," ","卫生洁具及暖气管道用直角阀 GB/T26712-2011 4.3"," ",100," "," 卫生洁具——直角阀  "]
["轻工及机械检测中心",3,"表面镀层"," ","卫生洁具及暖气管道用直角阀 GB/T26712-2011 4.4"," ",100," "," 卫生洁具——直角阀  "]
["轻工及机械检测中心",4,"使用性能","阀体强度","卫生洁具及暖气管道用直角阀 GB/T26712-2011 4.7"," ",300," "," 卫生洁具——直角阀  "]
["轻工及机械检测中心",4,"使用性能","密封性能","卫生洁具及暖气管道用直角阀 GB/T26712-2011 4.7"," ",200," "," 卫生洁具——直角阀  "]
["轻工及机械检测中心",4,"使用性能","上密封","卫生洁具及暖气管道用直角阀 GB/T26712-2011 4.7"," ",200," "," 卫生洁具——直角阀  "]
["轻工及机械检测中心",1,"外观质量","铜铸件外表面","卫生洁具 淋浴用花洒 GB／T 23447-2009 5.1"," ",50," "," 卫生洁具——沐浴用花洒  "]
["轻工及机械检测中心",1,"外观质量","塑料件外表面","卫生洁具 淋浴用花洒 GB／T 23447-2009 5.1"," ",50," "," 卫生洁具——沐浴用花洒  "]
["轻工及机械检测中心",1,"外观质量","所有在使用中人体可触及的表面","卫生洁具 淋浴用花洒 GB／T 23447-2009 5.1"," ",50," "," 卫生洁具——沐浴用花洒  "]
["轻工及机械检测中心",1,"外观质量","产电镀外观表面","卫生洁具 淋浴用花洒 GB／T 23447-2009 5.1"," ",50," "," 卫生洁具——沐浴用花洒  "]
["轻工及机械检测中心",2,"管螺纹精度"," ","卫生洁具 淋浴用花洒 GB／T 23447-2009 5.2"," ",100," "," 卫生洁具——沐浴用花洒  "]
["轻工及机械检测中心",3,"表面涂镀层质量","耐腐蚀性能","人造气氛腐蚀试验盐雾试验 GB/T 10125-2012 5.4"," ",1500," "," 卫生洁具——沐浴用花洒  "]
["轻工及机械检测中心",4,"密封性能使用"," ","卫生洁具 淋浴用花洒 GB／T 23447-2009 5.5"," ",300," "," 卫生洁具——沐浴用花洒  "]
["轻工及机械检测中心",5,"机械强度试验"," ","卫生洁具 淋浴用花洒 GB／T 23447-2009 5.6"," ",200," "," 卫生洁具——沐浴用花洒  "]
["轻工及机械检测中心",6,"整体抗拉性能"," ","卫生洁具 淋浴用花洒 GB／T 23447-2009 5.9"," ",300," "," 卫生洁具——沐浴用花洒  "]
["轻工及机械检测中心",1,"外观"," ","GB/T11981-2024　7.3.1"," ",50," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",2,"尺寸","宽度偏差","GB/T11981-2024　7.3.2"," ",50," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",2,"尺寸","高度偏差","GB/T11981-2024　7.3.2"," ",50," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",2,"尺寸","厚度","GB/T11981-2024　7.3.2"," ",50," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",2,"尺寸","侧面和底面的平直度","GB/T11981-2024　7.3.2"," ",50," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",2,"尺寸","弯曲内角半径","GB/T11981-2024　7.3.2"," ",50," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",3,"彩色涂层钢板性能","涂渡层厚度","GB/T11981-2024 7.3.6.2"," ",500," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",3,"彩色涂层钢板性能","涂层铅笔硬度","GB/T 6739-2022","GB/T 6739-2022",200," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",4,"双面镀锌量"," ","GB/T11981-2024 7.3.6.1"," ",600," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",5,"耐盐雾性能"," ","GB/T 10125-2021","GB/T 10125-2021",960," "," 薄壁型钢——建筑用轻钢龙骨  "]
["轻工及机械检测中心",1,"材料"," ","玩具安全 第二部分:机械与物理性能 GB 6675.2-2014 5.2"," ",200," "," 玩具——玩具  "]
["轻工及机械检测中心",2,"边缘"," ","玩具安全 第二部分:机械与物理性能 GB 6675.2-2014 5.3"," ",300," "," 玩具——玩具  "]
["轻工及机械检测中心",5,"尖端"," ","玩具安全 第二部分:机械与物理性能 GB 6675.2-2014 5.6"," ",300," "," 玩具——玩具  "]
["轻工及机械检测中心",6,"小零件"," ","玩具安全 第二部分:机械与物理性能 GB 6675.2-2014 5.7"," ",300," "," 玩具——玩具  "]
["轻工及机械检测中心",10,"突出物"," ","玩具安全 第二部分:机械与物理性能 GB 6675.2-2014 5.11"," ",300," "," 玩具——玩具  "]
["轻工及机械检测中心",13,"缝纫拼缝牢度"," ","玩具安全 第二部分:机械与物理性能 GB 6675.2-2014 5.24"," ",200," "," 玩具——玩具  "]
["轻工及机械检测中心",14,"声压级的测量"," ","玩具安全 第二部分:机械与物理性能 GB 6675.2-2014 5.25"," ",300," "," 玩具——玩具  "]
["轻工及机械检测中心",1,"尺寸偏差"," ","运输包装用单瓦楞纸箱和双瓦楞纸箱 GB/T 6543-2008 4.1"," ",100," "," 纸品——运输包装用单瓦楞纸箱和双瓦楞纸箱  "]
["轻工及机械检测中心",2,"外观"," ","运输包装用单瓦楞纸箱和双瓦楞纸箱 GB/T 6543-2008 "," ",50," "," 纸品——运输包装用单瓦楞纸箱和双瓦楞纸箱  "]
["轻工及机械检测中心",3,"抗压力"," ","包装?运输包装件基本试验?第4部分:采用压力试验机进行的抗压 GB/T?4857.4-2008 5.38"," ",300," "," 纸品——运输包装用单瓦楞纸箱和双瓦楞纸箱  "]
["轻工及机械检测中心",4,"耐破强度"," ","瓦楞纸板耐破强度的测定法 GB/T?6545-1998 5.11"," ",300," "," 纸品——运输包装用单瓦楞纸箱和双瓦楞纸箱  "]
["轻工及机械检测中心",5,"边压强度"," ","瓦楞纸板边压强度的测定法 GB/T?6546-1998 5.11"," ",300," "," 纸品——运输包装用单瓦楞纸箱和双瓦楞纸箱  "]
["轻工及机械检测中心",6,"粘合强度"," ","瓦楞纸板 GB/T6544-2008       5.11"," ",300," "," 纸品——运输包装用单瓦楞纸箱和双瓦楞纸箱  "]
["轻工及机械检测中心",7,"厚度"," ","瓦楞纸板厚度的测定法 GB/T 6547-1998 5.11"," ",100," "," 纸品——运输包装用单瓦楞纸箱和双瓦楞纸箱  "]
["轻工及机械检测中心",8,"含水率"," ","纸和纸板水分的测定  GB/T462-2008 5.11"," ",150," "," 纸品——运输包装用单瓦楞纸箱和双瓦楞纸箱  "]
["轻工及机械检测中心",1,"尺寸偏差"," ","军用瓦楞纸箱GJB　1109A-1999　"," ",100," "," 纸品——军用瓦楞纸箱  "]
["轻工及机械检测中心",2,"外观"," ","军用瓦楞纸箱GJB　1109A-1999　"," ",50," "," 纸品——军用瓦楞纸箱  "]
["轻工及机械检测中心",3,"抗压力"," ","军用瓦楞纸箱GJB　1109A-1999　"," ",300," "," 纸品——军用瓦楞纸箱  "]
["轻工及机械检测中心",4,"自由跌落性能"," ","军用瓦楞纸箱GJB　1109A-1999　"," ",300," "," 纸品——军用瓦楞纸箱  "]
["轻工及机械检测中心",5,"防潮性能"," ","军用瓦楞纸箱GJB　1109A-1999　"," ",1500," "," 纸品——军用瓦楞纸箱  "]
["轻工及机械检测中心",6,"含水率"," ","军用瓦楞纸箱GJB　1109A-1999　"," ",150," "," 纸品——军用瓦楞纸箱  "]
["轻工及机械检测中心",1,"外观质量"," ","军用瓦楞纸板 GJB 1110A-1999 5.1"," ",50," "," 纸品——军用瓦楞纸板  "]
["轻工及机械检测中心",2,"厚度"," ","瓦楞纸板厚度的测定法 GB 6547-1998 5.2.3"," ",100," "," 纸品——军用瓦楞纸板  "]
["轻工及机械检测中心",3,"含水率"," ","纸、纸板和纸浆分析试样水分的测定 GB/T462-2008 5.2.4"," ",150," "," 纸品——军用瓦楞纸板  "]
["轻工及机械检测中心",4,"边压强度"," ","军用瓦楞纸板 GJB 1110A-1999 5.1"," ",150," "," 纸品——军用瓦楞纸板  "]
["轻工及机械检测中心",5,"耐破强度"," ","瓦楞纸板边压强度的测定 GB/T6546-1998 5.2.5"," ",300," "," 纸品——军用瓦楞纸板  "]
["轻工及机械检测中心",6,"戳穿强度"," ","瓦楞纸板耐破强度的测定法 GB/T6545-1998 5.2.6"," ",300," "," 纸品——军用瓦楞纸板  "]
["轻工及机械检测中心",7,"粘合强度"," ","纸板戳穿强度的测定  GB/T2679.7-2005 5.2.7"," ",300," "," 纸品——军用瓦楞纸板  "]
["轻工及机械检测中心",1,"规格尺寸"," ","簿册 QB/T 1438-2007 6.1"," ",100," "," 纸品——簿册  "]
["轻工及机械检测中心",2,"定量"," ","纸和纸板定量的测定 GB/T451.2-2002 6.2"," ",200," "," 纸品——簿册  "]
["轻工及机械检测中心",3,"套印"," ","簿册 QB/T 1438-2007 6.3"," ",200," "," 纸品——簿册  "]
["轻工及机械检测中心",4,"簿背内芯"," ","簿册 QB/T 1438-2007 6.4"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",5,"压槽簿背"," ","簿册 QB/T 1438-2007 6.5"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",6,"芯页"," ","簿册 QB/T 1438-2007 6.6"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",7,"页数"," ","簿册 QB/T 1438-2007 6.8"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",8,"两面对线"," ","簿册 QB/T 1438-2007 6.7"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",9,"断线"," ","簿册 QB/T 1438-2007 6.6"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",10,"破页"," ","簿册 QB/T 1438-2007 6.4"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",11,"白页"," ","簿册 QB/T 1438-2007 6.4"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",12,"脏迹"," ","簿册 QB/T 1438-2007 6.6"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",13,"圆角"," ","簿册 QB/T 1438-2007 6.4"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",14,"漂口"," ","簿册 QB/T 1438-2007 6.9"," ",20," "," 纸品——簿册  "]
["轻工及机械检测中心",15,"施胶度"," ","纸 施胶度的测定 GB/T 460-2008 6.10"," ",100," "," 纸品——簿册  "]
["轻工及机械检测中心",1,"装订质量"," ","课业簿册 QB/T 1437-2014 6.1"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",2,"纸张定量"," ","课业簿册 QB/T 1437-2014 6.2"," ",200," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",3,"破页"," ","课业簿册 QB/T 1437-2014 6.3"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",4,"脏迹"," ","课业簿册 QB/T 1437-2014 6.4"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",5,"白页"," ","课业簿册 QB/T 1437-2014 6.5"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",6,"印划线"," ","课业簿册 QB/T 1437-2014 6.6"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",7,"张数"," ","课业簿册 QB/T 1437-2014 6.7"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",8,"断线"," ","课业簿册 QB/T 1437-2014 6.8"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",9,"偏斜"," ","课业簿册 QB/T 1437-2014 6.9"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",10,"封面/封底"," ","课业簿册 QB/T 1437-2014 6.10"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",11,"套印偏差"," ","课业簿册 QB/T 1437-2014 6.11"," ",200," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",12,"施胶度"," ","纸 施胶度的测定 GB/T 460-2008 6.12"," ",100," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",13,"成品尺寸偏差"," ","课业簿册 QB/T 1437-2014 6.13"," ",100," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",14,"装订偏差"," ","课业簿册 QB/T 1437-2014 6.14"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",15,"危险锐利尖端"," ","课业簿册 QB/T 1437-2014 6.15"," ",20," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",16,"可迁移元素"," "," 学生用品的安全通用要求  GB 21027-2007 6.16"," ",1600," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",17,"脱色试验 "," ","课业簿册 QB/T 1437-2014 6.17"," ",50," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",18,"亮度 "," ","纸、纸板和纸浆 蓝光漫反射因数D65亮度的测定(漫射/垂直法 GB/T 7974-2013 6.18"," ",100," "," 纸品——课业簿册——旧标准QB/T 1437-2014"]
["轻工及机械检测中心",1,"装订"," "," QB/T 1437-2023"," ",50," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",2,"封面、封底定量"," ","GB/T451.2-2023"," ",200," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",4,"内芯定量"," ","GB/T451.2-2023"," ",200," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",5,"破页张数"," ","QB/T 1437-2023中 6.2.2"," ",50," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",6,"脏迹"," ","QB/T 1437-2023中 6.2.2"," ",50," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",7,"白页"," ","QB/T 1437-2023中 6.2.1"," ",50," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",8,"印划线两面对线偏差"," ","QB/T 1437-2023中 6.2.4"," ",50," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",9,"内芯张数"," ","QB/T 1437-2023中 6.2.3"," ",50," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",10,"断线"," ","QB/T 1437-2023中 6.2.2"," ",50," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",11,"偏斜"," ","QB/T 1437-2023中 6.2.5"," ",100," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",12,"印刷"," ","QB/T 1437-2023中 6.2.1"," ",50," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",13,"套印偏差"," ","QB/T 1437-2023中 6.2.6"," ",200," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",14,"施胶度"," ","GB/T 460-2008"," ",100," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",15,"成品整体规格尺寸偏差"," ","QB/T 1437-2023中 6.2.8"," ",100," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",16,"装订偏差"," ","QB/T 1437-2023中 6.2.7"," ",100," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",18,"安全"," ","QB/T 1437-2023中 6.4"," ",100," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",19,"可迁移元素"," ","GB 21027-2020"," ",1600," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",20,"内芯D65亮度"," ","GB/T 7974-2013"," ",100," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",21,"内芯D65荧光亮度"," ","GB/T 7974-2013"," ",500," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",22,"内芯平滑度"," ","GB/T 456-2002"," ",80," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",23,"内芯格线印刷尺寸"," ","QB/T 1437-2023中 6.2"," ",100," "," 纸品——课业簿册——新标准QB/T 1437-2023"]
["轻工及机械检测中心",1,"定量"," ","纸和纸板定量的测定  GB/T451.2-2002 4.4"," ",200," "," 纸品——图画纸  "]
["轻工及机械检测中心",2,"定量偏差"," ","纸和纸板定量的测定  GB/T451.2-2002 4.4"," ",200," "," 纸品——图画纸  "]
["轻工及机械检测中心",3,"紧度"," ","纸和纸板厚度的测定 GB/T 451.3-2002 4.5"," ",100," "," 纸品——图画纸  "]
["轻工及机械检测中心",4,"裂断长"," ","纸和纸板抗张强度的测定  GB/T 12914-2008 5.1.9"," ",300," "," 纸品——图画纸  "]
["轻工及机械检测中心",5,"耐折度"," ","纸和纸板耐折度的测定 GB/T457-2008  4.7"," ",200," "," 纸品——图画纸  "]
["轻工及机械检测中心",6,"施胶度"," ","纸 施胶度的测定 GB/T 460-2008 4.8"," ",100," "," 纸品——图画纸  "]
["轻工及机械检测中心",7,"亮度"," ","纸、纸板和纸浆 蓝光漫反射因数D65亮度的测定(漫射/垂直法 GB/T 7974-2013 4.9"," ",100," "," 纸品——图画纸  "]
["轻工及机械检测中心",8,"尘埃度"," ","纸和纸板尘埃度的测定 GB/T 1541-2013 4.10"," ",100," "," 纸品——图画纸  "]
["轻工及机械检测中心",9,"水分"," ","纸、纸板和纸浆分析试样水分的测定 GB/T462-2008 4.11"," ",150," "," 纸品——图画纸  "]
["轻工及机械检测中心",10,"耐擦性"," "," "," ",100," "," 纸品——图画纸  "]
["轻工及机械检测中心",11,"尺寸和偏斜度"," ","图画纸 GB/T22833-2008中附录A GB/T22833-2008 4.12"," ",100," "," 纸品——图画纸  "]
["轻工及机械检测中心",12,"外观"," ","纸和纸板尺寸及偏斜度的测定  GB/T451.1-2002 4.3"," ",50," "," 纸品——图画纸  "]
["轻工及机械检测中心",1,"印刷"," ","平装书刊质量分级与检验方法 CY/T 15-1995 6.1.2"," ",200," "," 纸品——平装书刊  "]
["轻工及机械检测中心",2,"印后加工"," ","平装书刊质量分级与检验方法 CY/T 15-1995 6.1.3"," ",50," "," 纸品——平装书刊  "]
["轻工及机械检测中心",3,"外观"," ","平装书刊质量分级与检验方法 CY/T 15-1995 6.1.4"," ",50," "," 纸品——平装书刊  "]
["轻工及机械检测中心",4,"裁切歪斜及误差"," "," 图书和杂志开本及其幅面尺寸  GB/T 788-1999 6.1.4"," ",50," "," 纸品——平装书刊  "]
["轻工及机械检测中心",1,"规格尺寸"," ","胶印印书质量分级与检验方法 CY/T 13-1995 4.2"," ",50," "," 纸品——胶印印书  "]
["轻工及机械检测中心",2,"墨色"," ","胶印印书质量分级与检验方法 CY/T 13-1995 4.3.1"," ",50," "," 纸品——胶印印书  "]
["轻工及机械检测中心",3,"文字印迹"," ","胶印印书质量分级与检验方法 CY/T 13-1995 4.3.2"," ",50," "," 纸品——胶印印书  "]
["轻工及机械检测中心",4,"实地密度"," ","胶印印书质量分级与检验方法 CY/T 13-1995 4.3.3"," ",200," "," 纸品——胶印印书  "]
["轻工及机械检测中心",5,"图象印迹"," ","胶印印书质量分级与检验方法 CY/T 13-1995 4.3.4"," ",50," "," 纸品——胶印印书  "]
["轻工及机械检测中心",6,"表格印迹"," ","胶印印书质量分级与检验方法 CY/T 13-1995 4.3.5"," ",50," "," 纸品——胶印印书  "]
["轻工及机械检测中心",7,"套印"," ","胶印印书质量分级与检验方法 CY/T 13-1995 4.4"," ",200," "," 纸品——胶印印书  "]
["轻工及机械检测中心",8,"外观"," ","胶印印书质量分级与检验方法 CY/T 13-1995 4.5"," ",50," "," 纸品——胶印印书  "]
["轻工及机械检测中心",9,"装订质量"," ","胶印印书质量分级与检验方法 CY/T 13-1995 4.6"," ",50," "," 纸品——胶印印书  "]
["轻工及机械检测中心",1,"纸张定量偏差"," ","纸和纸板定量的测定  GB/T451.2-2002 5.1.3"," ",200," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",2,"纸张厚度偏差"," ","纸和纸板尺寸及偏斜度的测定  GB/T451.1-2002 5.1.2"," ",100," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",3,"纸张白度"," ","纸、纸板和纸浆 、蓝光漫反射因数D65亮度的测定  GB/T7974-2013 5.1.4"," ",100," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",4,"纸张平滑度"," ","纸和纸板平滑度的测定   GB/T456-2002 5.1.6"," ",80," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",5,"纸张抗张指数"," ","纸和纸板抗张强度的测定  GB/T 12914-2008 5.1.9"," ",200," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",6,"纸张吸水性"," ","纸和纸板吸水性的测定 可勃法   GB/T 1540-2002 5.1.10"," ",100," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",7,"纸张耐折度"," ","纸和纸板耐折度的测定 GB/T457-2008 5.1.12"," ",200," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",8,"纸张尘埃度"," ","纸和纸板 尘埃度的测定   GB/T 1541-2013 5.1.13"," ",100," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",9,"纸张PH"," ","纸、纸板和纸浆 水抽提液酸度或碱度的测定   GB/T1545-2008 6.6"," ",150," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",10,"水分"," ","纸、纸板和纸浆分析试样水分的测定 GB/T462-2008 5.1.16"," ",150," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",11,"纸张外观质量"," "," "," ",50," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",12,"单色印刷要求"," ","中小学教科书用纸、印制质量要求和检验方法 G8/T18359-2009 5.1.17     5.1.18"," ",50," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",13,"彩色印刷"," ","中小学教科书用纸、印制质量要求和检验方法                                   平版印刷品质量要求及检验方法                    G8/T18359-2009"," ",300," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",14,"折页配页"," ","中小学教科书用纸、印制质量要求和检验方法 G8/T18359-2009 5.5.1"," ",50," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",15,"覆膜上光质量"," ","中小学教科书用纸、印制质量要求和检验方法 G8/T18359-2009 5.5.2"," ",50," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",16,"书芯订联"," ","中小学教科书用纸、印制质量要求和检验方法 G8/T18359-2009 5.5.3.1"," ",50," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",17,"包封面"," ","中小学教科书用纸、印制质量要求和检验方法 G8/T18359-2009 5.5.3.2"," ",50," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",18,"骑马钉装"," ","中小学教科书用纸、印制质量要求和检验方法 G8/T18359-2009 5.5.4"," ",50," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",19,"成品质量"," ","中小学教科书用纸、印制质量要求和检验方法 G8/T18359-2009 5.6"," ",50," "," 纸品——中小学教科书用纸、印制质量试验方法  "]
["轻工及机械检测中心",1,"成品规格误差"," ","凸版装璜印刷品 GB/T 7706-2008 6.3"," ",50," "," 纸品——凸版装璜印刷品  "]
["轻工及机械检测中心",2,"套印误差"," ","凸版装璜印刷品 GB/T 7706-2008 6.4"," ",200," "," 纸品——凸版装璜印刷品  "]
["轻工及机械检测中心",3,"同色密度偏差"," ","凸版装璜印刷品 GB/T 7706-2008 6.5"," ",200," "," 纸品——凸版装璜印刷品  "]
["轻工及机械检测中心",4,"同批同色色差"," ","凸版装璜印刷品 GB/T 7706-2008 6.6"," ",200," "," 纸品——凸版装璜印刷品  "]
["轻工及机械检测中心",5,"外观"," ","凸版装璜印刷品 GB/T 7706-2008 6.2"," ",50," "," 纸品——凸版装璜印刷品  "]
["轻工及机械检测中心",1,"成品规格误差"," ","平版装璜印刷品 GB/T 7705-2008 6.3"," ",50," "," 纸品——账册  ——平版装璜印刷品"]
["轻工及机械检测中心",2,"套印误差"," ","平版装璜印刷品 GB/T 7705-2008 6.4"," ",200," "," 纸品——账册  ——平版装璜印刷品"]
["轻工及机械检测中心",3,"同色密度偏差"," ","平版装璜印刷品 GB/T 7705-2008 6.5"," ",200," "," 纸品——账册  ——平版装璜印刷品"]
["轻工及机械检测中心",4,"同批同色色差"," ","平版装璜印刷品 GB/T 7705-2008 6.6"," ",200," "," 纸品——账册  ——平版装璜印刷品"]
["轻工及机械检测中心",5,"外观"," ","平版装璜印刷品 GB/T 7705-2008 6.2"," ",50," "," 纸品——账册  ——平版装璜印刷品"]
["轻工及机械检测中心",1,"规格尺寸"," ","帐册 QB/T 1439-2005 5.1"," ",100," "," 纸品——账册  "]
["轻工及机械检测中心",2,"定量"," ","纸和纸板定量的测定 GB/T451.2-2002 5.2"," ",200," "," 纸品——账册  "]
["轻工及机械检测中心",3,"簿背与内芯"," ","帐册 QB/T 1439-2005 5.1"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",4,"压槽与簿背"," ","帐册 QB/T 1439-2005 5.1"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",5,"封面"," ","帐册 QB/T 1439-2005 5.1"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",6,"内芯"," ","帐册 QB/T 1439-2005 5.1"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",7,"霉变"," ","帐册 QB/T 1439-2005 5.6"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",8,"线条套印线"," ","帐册 QB/T 1439-2005 5.6"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",9,"页码"," ","帐册 QB/T 1439-2005 5.6"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",10,"白度"," ","帐册 QB/T 1439-2005 5.3"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",11,"断线"," ","帐册 QB/T 1439-2005 5.6"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",12,"字迹线条"," ","帐册 QB/T 1439-2005 5.6"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",13,"印刷脏迹"," ","帐册 QB/T 1439-2005 5.6"," ",20," "," 纸品——账册  "]
["轻工及机械检测中心",14,"施胶度"," ","纸 施胶度的测定 GB/T 460-2008 5.5"," ",100," "," 纸品——账册  "]
["轻工及机械检测中心",1,"定量"," "," 纸和纸板定量的测定 GB/T 451.2-2002 5.3"," ",200," "," 纸品——箱纸板  "]
["轻工及机械检测中心",2,"横幅定量差"," ","纸和纸板定量的测定_ GB/T 451.2-2002 5.3"," ",200," "," 纸品——箱纸板  "]
["轻工及机械检测中心",3,"紧度"," "," 纸和纸板厚度的测定 GB/T 451.3-2002 5.4"," ",100," "," 纸品——箱纸板  "]
["轻工及机械检测中心",4,"耐破指数"," ","纸耐破度的测定                                                                     纸板耐破度的测定  GB/T454-2002 GB/T1539-2007 5.5"," ",300," "," 纸品——箱纸板  "]
["轻工及机械检测中心",5,"横向环压指数"," "," 纸和纸板环压强度的测定            GB/T 2679.8-2016  5.6"," ",300," "," 纸品——箱纸板  "]
["轻工及机械检测中心",6,"平滑度"," ","纸和纸板平滑度的测定   GB/T456-2002 5.7"," ",100," "," 纸品——箱纸板  "]
["轻工及机械检测中心",7,"耐折度"," ","纸和纸板耐折度的测定 GB/T457-2008  5.8"," ",200," "," 纸品——箱纸板  "]
["轻工及机械检测中心",8,"吸水性"," ","纸和纸板吸水性的测定 可勃法 GB/T 1540-2002 5.9"," ",150," "," 纸品——箱纸板  "]
["轻工及机械检测中心",9,"水分"," ","纸和纸板水分的测定  GB/T462-2008 5.10"," ",150," "," 纸品——箱纸板  "]
["轻工及机械检测中心",10,"尺寸"," "," "," ",50," "," 纸品——箱纸板  "]
["轻工及机械检测中心",1,"外观"," ","箱纸板 GB/T13024-2016 5.11"," ",50," "," 纸品——瓦楞芯原纸  "]
["轻工及机械检测中心",2,"定量"," ","纸和纸板定量的测定 GB/T451.2-2002 6.1"," ",200," "," 纸品——瓦楞芯原纸  "]
["轻工及机械检测中心",3,"紧度"," ","纸和纸板厚度的测定 GB/T 451.3-2002 6.1"," ",100," "," 纸品——瓦楞芯原纸  "]
["轻工及机械检测中心",4,"横向环压指数"," ","纸和纸板环压强度的测定 GB/T 2679.8-2016 6.3"," ",300," "," 纸品——瓦楞芯原纸  "]
["轻工及机械检测中心",5,"纵向裂断长"," ","纸和纸板 抗张强度的测定 GB/T12914-2008 6.5"," ",300," "," 纸品——瓦楞芯原纸  "]
["轻工及机械检测中心",6,"水分"," ","纸、纸板和纸浆 分析试样水分的测定 GB/T 462-2008/ 6.6"," ",150," "," 纸品——瓦楞芯原纸  "]
["轻工及机械检测中心",6,"外观"," ","纸和纸板吸水性的测定 可勃法 GB/T 1540-2002 6.7"," ",50," "," 纸品——瓦楞芯原纸  "]
["轻工及机械检测中心",7,"吸水性"," "," "," ",150," "," 纸品——瓦楞芯原纸  "]
["轻工及机械检测中心",1,"尺寸偏差"," ","纸和纸板尺寸及偏斜度的测定  GB/T 451.1-2002    5.2"," ",50," "," 纸品——复印纸  "]
["轻工及机械检测中心",2,"定量"," ","纸和纸板定量的测定 GB/T451.2-2002 5.3"," ",200," "," 纸品——复印纸  "]
["轻工及机械检测中心",3,"定量偏差"," ","纸和纸板定量的测定 GB/T451.2-2002 5.3"," ",200," "," 纸品——复印纸  "]
["轻工及机械检测中心",4,"厚度"," ","纸和纸板厚度的测定 GB/T 451.3-2002 5.4"," ",100," "," 纸品——复印纸  "]
["轻工及机械检测中心",5,"平滑度"," ","纸和纸板平滑度的测定(别克法) GB/T 456-2002 5.6"," ",100," "," 纸品——复印纸  "]
["轻工及机械检测中心",6,"亮度"," ","纸、纸板和纸浆 蓝光漫反射因数D65亮度的测定(漫射/垂直法 GB/T 7974-2013 5.8"," ",100," "," 纸品——复印纸  "]
["轻工及机械检测中心",7,"施胶度"," ","纸 施胶度的测定 GB/T 460-2008 5.9"," ",100," "," 纸品——复印纸  "]
["轻工及机械检测中心",8,"尘埃度"," ","纸和纸板尘埃度的测定 GB/T 1541-2013 5.10"," ",50," "," 纸品——复印纸  "]
["轻工及机械检测中心",9,"水分"," ","纸、纸板和纸浆 分析试样水分的测定 GB/T 462-2008/ 5.11"," ",150," "," 纸品——复印纸  "]
["轻工及机械检测中心",10,"内装量偏差"," "," "," ",100," "," 纸品——复印纸  "]
["轻工及机械检测中心",11,"外观质量"," ","复印纸 GB/T 24988-2010 5.12"," ",50," "," 纸品——复印纸  "]
["轻工及机械检测中心",1,"长度偏差"," ","湿巾 GB/T 27728-2011 6.2"," ",50," "," 纸品——湿巾  "]
["轻工及机械检测中心",2,"宽度偏差"," ","湿巾 GB/T 27728-2011 6.2"," ",50," "," 纸品——湿巾  "]
["轻工及机械检测中心",3,"含液量"," ","湿巾 GB/T 27728-2011 6.3"," ",150," "," 纸品——湿巾  "]
["轻工及机械检测中心",4,"横向抗张强度"," ","纸和纸板 抗张强度的测定 GB/T12914-2008 6.4"," ",200," "," 纸品——湿巾  "]
["轻工及机械检测中心",5,"包装密封性能"," ","湿巾 GB/T 27728-2011 6.5"," ",100," "," 纸品——湿巾  "]
["轻工及机械检测中心",6,"PH"," ","纸、纸板和纸浆 水抽提液酸度或碱度的测定   GB/T1545-2008 6.6"," ",150," "," 纸品——湿巾  "]
["轻工及机械检测中心",7,"去污力"," ","湿巾 GB/T 27728-2011 6.7"," ",100," "," 纸品——湿巾  "]
["轻工及机械检测中心",8,"腐蚀性"," ","湿巾 GB/T 27728-2011 6.8"," ",100," "," 纸品——湿巾  "]
["轻工及机械检测中心",9,"可迁移性荧光增白剂"," ","湿巾 GB/T 27728-2011 6.9"," ",100," "," 纸品——湿巾  "]
["轻工及机械检测中心",10,"尘埃度"," ","湿巾 GB/T 27728-2011 6.10"," ",100," "," 纸品——湿巾  "]
["轻工及机械检测中心",11,"内装量"," ","湿巾 GB/T 27728-2011 6.11"," ",50," "," 纸品——湿巾  "]
["轻工及机械检测中心",12,"外观质量"," ","湿巾 GB/T 27728-2011 6.12"," ",50," "," 纸品——湿巾  "]
["轻工及机械检测中心",13,"细菌菌落总数"," ","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",100," "," 纸品——湿巾  "]
["轻工及机械检测中心",14,"致病性球菌","金黄色葡萄球菌","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",150," "," 纸品——湿巾  "]
["轻工及机械检测中心",14,"致病性球菌","化脓菌指绿浓杆菌","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",150," "," 纸品——湿巾  "]
["轻工及机械检测中心",14,"致病性球菌","溶血性链球菌","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",150," "," 纸品——湿巾  "]
["轻工及机械检测中心",15,"大肠菌群"," ","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",100," "," 纸品——湿巾  "]
["轻工及机械检测中心",16,"真菌菌落总数"," ","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",100," "," 纸品——湿巾  "]
["轻工及机械检测中心",1,"定量"," ","纸和纸板定量的测定 GB/T451.2-2002  6.2"," ",200," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",2,"亮度"," ","纸、纸板和纸浆 蓝光漫反射因数D65亮度的测定(漫射/垂直法 GB/T 7974-2013 6.3"," ",300," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",3,"横向吸液高度"," ","纸和纸板毛细吸液高度的(克列姆法） GB/T 461.1-2002 6.4"," ",200," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",4,"抗张指数（纵横平均）"," ","纸和纸板 抗张强度的测定 GB/T 12914-2008 6.5"," ",300," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",5,"柔软度"," ","纸柔软度的测定 GB/T 8942-2016 6.6"," ",200," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",6,"洞眼"," ","卫生纸（含卫生纸原纸） GB/T 20810-2006 6.7"," ",50," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",7,"尘埃度"," "," 纸和纸板 尘埃度的测定 GB/T 1541-2013 6.8"," ",50," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",8,"水分"," ","纸、纸板和纸浆 分析试样水分的测定 GB/T 462-2008 6.9"," ",150," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",9,"微生物指标","细菌总数","卫生纸（含卫生纸原纸） GB/T 20810-2006 6.7"," ",100," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",9,"微生物指标","大肠菌群","卫生纸（含卫生纸原纸） GB/T 20810-2006 6.7"," ",100," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",9,"微生物指标","金黄色葡萄球菌","卫生纸（含卫生纸原纸） GB/T 20810-2006 6.7"," ",150," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",9,"微生物指标","溶血链球菌","卫生纸（含卫生纸原纸） GB/T 20810-2006 6.7"," ",150," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",10,"尺寸偏差"," ","GB/T 20810-2006 GB/T 20810-2006 6.12"," ",50," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",11,"偏斜度"," ","纸和纸板尺寸及偏斜度的测定  GB/T 451.1-2002 6.11"," ",50," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",12,"外观"," ","卫生纸（含卫生纸原纸） GB/T20810-2006  4.6"," ",50," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",13,"掉粉率"," ","GB/T 20810-2018附录B","GB/T 20810-2018",300," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",14,"球形耐破度"," ","GB/T 24328.7-2020"," ",300," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",15,"允许短缺量"," ","GB/T 20810-2018","GB/T 20810-2018",100," "," 纸品——卫生纸（含卫生纸原纸）  "]
["轻工及机械检测中心",1,"尺寸偏差"," ","卫生巾(含卫生护垫) GB/T8939-2008 5.2"," ",100," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",2,"条质量"," ","卫生巾(含卫生护垫) GB/T8939-2008 5.2"," ",150," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",3,"吸水倍率"," ","卫生巾(含卫生护垫) GB/T8939-2008 5.3"," ",100," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",4,"吸收速度"," ","GB/T8939-2018 附录A"," ",800," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",5,"PH"," ","卫生巾(含卫生护垫) GB/T8939-2008 5.5"," ",150," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",6,"水分"," ","纸、纸板和纸浆 分析试样水分的测定 GB/T 462-2008 5.6"," ",150," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",7,"原材料"," ","一次性使用卫生用品卫生标准 GB 15979-2002 4.3"," ",50," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",8,"包装"," ","卫生巾(含卫生护垫) GB/T8939-2008 4.4"," ",20," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",9,"封口"," ","卫生巾(含卫生护垫) GB/T8939-2008 4.5"," ",20," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",10,"防粘纸"," ","卫生巾(含卫生护垫) GB/T8939-2008 4.6"," ",20," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",11,"细菌菌落总数"," ","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",100," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",12,"致病性球菌","金黄色葡萄球菌","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",150," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",12,"致病性球菌","化脓菌指绿浓杆菌","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",150," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",12,"致病性球菌","溶血性链球菌","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",150," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",13,"大肠菌群"," ","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",100," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",14,"真菌菌落总数"," ","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",100," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",15,"背胶剥离强度"," ","GB/T 8939-2018附录E","GB/T 8939-2018",500," "," 纸品——卫生巾(含卫生护垫)  "]
["轻工及机械检测中心",1,"纸品预处理"," "," 纸、纸板和纸浆试样处理和试验的标准大气条件GB/T 10739-2002 "," "," "," "," 纸品——纸品预处理  "]
["轻工及机械检测中心",1,"条质量偏差"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",150," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",2,"吸收速度"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",600," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",3,"回渗量"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",600," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",4,"渗漏量"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",600," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",5,"面层附着物"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",100," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",6,"PH"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",150," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",7,"杂质"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",200," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",8,"防侧漏性能"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",200," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",9,"交货水分"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",150," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",10,"可迁移荧光物质"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",200," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",11,"纸尿裤适用腰围最大值"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",100," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",12,"外观"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",50," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",13,"细菌菌落总数"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",100," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",14,"大肠菌群"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",150," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",15,"金黄色葡萄球菌"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",150," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",16,"溶血性链球菌"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",150," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",17,"绿脓杆菌"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",100," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",18,"真菌菌落总数"," ","GB/T 28004.1-2021《纸尿裤 第1部分：婴儿纸尿裤》"," ",100," "," 纸品——婴儿纸尿裤(新标准)"]
["轻工及机械检测中心",1,"条质量偏差"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",150," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",2,"吸收速度"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",600," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",3,"回渗量"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",600," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",4,"渗漏量"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",600," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",5,"面层附着物"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",100," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",6,"PH"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",150," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",7,"杂质"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",200," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",8,"饱和吸收量"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",200," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",9,"交货水分"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",150," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",10,"可迁移荧光物质"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",200," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",11,"纸尿裤适用腰围最大值"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",100," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",12,"外观"," ","GB/T 28004.2-2021《纸尿裤 第2部分：成人纸尿裤》"," ",50," "," 纸品——成人纸尿裤(新标准)"]
["轻工及机械检测中心",1,"定量"," ","GB/T 24328.5-2009"," ",200," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",2,"亮度"," ","GB/T 7974-2013"," ",300," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",3,"可迁移性荧光增白剂"," ","GB/T 20808-2022"," ",200," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",4,"横向吸收液高度"," ","GB/T 461.1-2002"," ",200," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",5,"横向抗张强度"," ","GB/T 24328.3-2020"," ",300," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",6,"纵向湿抗张强度"," ","GB/T465.2-2008"," ",350," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",7,"柔软度"," ","GB/T 8942-2016"," ",200," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",8,"可分散性"," ","GB/T 20808-2022"," ",500," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",9,"掉粉率"," ","GB/T 20808-2022"," ",300," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",10,"洞眼"," ","GB/T 20808-2022"," ",50," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",11,"水分"," ","GB/T 462-2023"," ",150," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",12,"内装量偏差"," ","GB/T 20808-2022"," ",100," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",13,"尺寸偏差"," ","GB/T 20808-2022"," ",50," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",14,"外观质量"," ","GB/T 20808-2022"," ",50," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",15,"细菌菌落总数"," ","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",100," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",16,"致病性球菌","金黄色葡萄球菌","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",150," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",16,"致病性球菌","化脓菌指绿浓杆菌","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",150," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",16,"致病性球菌","溶血性链球菌","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",150," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",17,"大肠菌群"," ","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",100," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",18,"真菌菌落总数"," ","一次性使用卫生用品卫生标准  GB 15979-2002 6.13"," ",100," "," 纸品——纸巾——监督抽查项目"]
["轻工及机械检测中心",1,"整车标志","铭牌","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",1,"整车标志","整车编码","GB 17761-2018《电动自行车安全技术规范》"," ",200," "," 电动自行车  "]
["轻工及机械检测中心",1,"整车标志","电动机编码","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",1,"整车标志","号牌安装位置","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",1,"整车标志","产品合格证","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","车速限值","GB 17761-2018《电动自行车安全技术规范》"," ",1000," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","车速限值","GB 17761-2018《电动自行车安全技术规范》"," ",500," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","制动性能","GB 17761-2018《电动自行车安全技术规范》"," ",1500," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","整车质量","GB 17761-2018《电动自行车安全技术规范》"," ",150," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","脚踏骑行能力","GB 17761-2018《电动自行车安全技术规范》"," ",1000," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","脚踏骑行能力","GB 17761-2018《电动自行车安全技术规范》"," ",200," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","脚踏骑行能力","GB 17761-2018《电动自行车安全技术规范》"," ",200," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","尺寸限值","GB 17761-2018《电动自行车安全技术规范》"," ",500," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","结构","GB 17761-2018《电动自行车安全技术规范》"," ",200," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","结构","GB 17761-2018《电动自行车安全技术规范》"," ",200," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","结构","GB 17761-2018《电动自行车安全技术规范》"," ",200," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","车速提示音","GB 17761-2018《电动自行车安全技术规范》"," ",450," "," 电动自行车  "]
["轻工及机械检测中心",2,"整车安全","涉水淋水性能","GB 17761-2018《电动自行车安全技术规范》"," ",3500," "," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","车架/前叉组合件","GB 17761-2018《电动自行车安全技术规范》"," ",1600," "," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","车架/前叉组合件","GB 17761-2018《电动自行车安全技术规范》"," ",1650," "," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","把立管和鞍管","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","把立管和鞍管","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","把立管和鞍管","GB 17761-2018《电动自行车安全技术规范》"," ",600," "," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","反射器、照明和鸣号装置","GB 17761-2018《电动自行车安全技术规范》"," ",500,"每个500"," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","反射器、照明和鸣号装置","GB 17761-2018《电动自行车安全技术规范》"," ",500,"每个500"," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","反射器、照明和鸣号装置","GB 17761-2018《电动自行车安全技术规范》"," ",500,"每个500"," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","反射器、照明和鸣号装置","GB 17761-2018《电动自行车安全技术规范》"," ",500,"每个500"," 电动自行车  "]
["轻工及机械检测中心",3,"机械安全","反射器、照明和鸣号装置","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","电气装置","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","电气装置","GB 17761-2018《电动自行车安全技术规范》"," ",30," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","电气装置","GB 17761-2018《电动自行车安全技术规范》"," ",600," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","控制系统","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","控制系统","GB 17761-2018《电动自行车安全技术规范》"," ",200," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","控制系统","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","电动机连续额定输出功率","GB 17761-2018《电动自行车安全技术规范》"," ",860," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","充电器与蓄电池","GB 17761-2018《电动自行车安全技术规范》"," ",2000," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","充电器与蓄电池","GB 17761-2018《电动自行车安全技术规范》"," ",480," "," 电动自行车  "]
["轻工及机械检测中心",4,"电气安全","充电器与蓄电池","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",5,"防火性能","550℃灼热丝试验","GB 17761-2018《电动自行车安全技术规范》"," ",300,"每个300"," 电动自行车  "]
["轻工及机械检测中心",5,"防火性能","750℃灼热丝试验","GB 17761-2018《电动自行车安全技术规范》"," ",300,"每个300"," 电动自行车  "]
["轻工及机械检测中心",6,"阻燃性能","固体非金属材料","GB 17761-2018《电动自行车安全技术规范》"," ",800,"每个800"," 电动自行车  "]
["轻工及机械检测中心",6,"阻燃性能","装饰性固体非金属材料","GB 17761-2018《电动自行车安全技术规范》"," ",720,"每个720"," 电动自行车  "]
["轻工及机械检测中心",7,"无线电骚扰特性"," ","GB 17761-2018《电动自行车安全技术规范》"," ",10000," "," 电动自行车  "]
["轻工及机械检测中心",8,"使用说明书"," ","GB 17761-2018《电动自行车安全技术规范》"," ",100," "," 电动自行车  "]
["轻工及机械检测中心",1,"外观质量"," ","GB 6264-2011"," ",110," "," 消防器材——消防水带"]
["轻工及机械检测中心",2,"内径"," ","GB 6264-2011"," ",110," "," 消防器材——消防水带"]
["轻工及机械检测中心",3,"长度"," ","GB 6264-2011"," ",110," "," 消防器材——消防水带"]
["轻工及机械检测中心",4,"设计工作压力、试验压力及最小爆破压力"," ","GB 6264-2011"," ",660," "," 消防器材——消防水带"]
["轻工及机械检测中心",5,"单位长度质量"," ","GB 6264-2011"," ",275," "," 消防器材——消防水带"]
["轻工及机械检测中心",6,"延伸率和膨胀率及扭转方向"," ","GB 6264-2011"," ",440," "," 消防器材——消防水带"]
["轻工及机械检测中心",7,"黏附性"," ","GB 6264-2011"," ",275," "," 消防器材——消防水带"]
["轻工及机械检测中心",8,"耐低温性能"," ","GB 6264-2011"," ",440," "," 消防器材——消防水带"]
["轻工及机械检测中心",9,"耐磨性能"," ","GB 6264-2011"," ",440," "," 消防器材——消防水带"]
["轻工及机械检测中心",1,"质量"," ","GB 4351.1-2005"," ",110," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",2,"最小有效喷射时间"," ","GB 4351.1-2005"," ",275," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",3,"最小有效喷射距离"," ","GB 4351.1-2005"," ",275," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",4,"使用温度范围"," ","GB 4351.1-2005"," ",275," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",5,"干粉灭火器振撞后的喷射性能"," ","GB 4351.1-2005"," ",275," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",6,"振动试验"," ","GB 4351.1-2005"," ",275," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",7,"冲击试验"," ","GB 4351.1-2005"," ",330," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",8,"水压试验"," ","GB 4351.1-2005"," ",440," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",9,"爆破试验"," ","GB 4351.1-2005"," ",440," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",10,"压力交变试验"," ","GB 4351.1-2005"," ",440," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",11,"灭火器的开启结构"," ","GB 4351.1-2005"," ",275," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",12,"灭火器喷射软管"," ","GB 4351.1-2005"," ",110," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",13,"灭火器提把"," ","GB 4351.1-2005"," ",110," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",14,"其他要求"," ","GB 4351.1-2005"," ",110," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",15,"灭火器压力指示器示值误差"," ","GB 4351.1-2005"," ",275," "," 消防器材——手提式灭火器"]
["轻工及机械检测中心",1,"外观质量"," ","GB 3445-2018"," ",110," "," 消防器材——室内消火栓"]
["轻工及机械检测中心",2,"密封性能"," ","GB 3445-2018"," ",550," "," 消防器材——室内消火栓"]
["轻工及机械检测中心",3,"水压强度"," ","GB 3445-2018"," ",550," "," 消防器材——室内消火栓"]
["轻工及机械检测中心",4,"手轮"," ","GB 3445-2018"," ",275," "," 消防器材——室内消火栓"]
["轻工及机械检测中心",5,"开启高度"," ","GB 3445-2018"," ",275," "," 消防器材——室内消火栓"]
["轻工及机械检测中心",1,"表面质量"," ","GB 8181-2005"," ",110," "," 消防器材——消防水枪"]
["轻工及机械检测中心",2,"密封性能"," ","GB 8181-2005"," ",440," "," 消防器材——消防水枪"]
["轻工及机械检测中心",3,"耐水压强度"," ","GB 8181-2005"," ",440," "," 消防器材——消防水枪"]
["轻工及机械检测中心",4,"抗跌落性能"," ","GB 8181-2005"," ",440," "," 消防器材——消防水枪"]
["轻工及机械检测中心",5,"耐腐蚀性能"," ","GB 8181-2005"," ",440," "," 消防器材——消防水枪"]
["轻工及机械检测中心",1,"箱内消防器材配置"," ","GB/T 14561-2019",null,110," "," 消防器材——消火栓箱"]
["轻工及机械检测中心",2,"外观质量、外形尺寸和极限偏差"," ","GB/T 14561-2019",null,300," "," 消防器材——消火栓箱"]
["轻工及机械检测中心",3,"标志"," ","GB/T 14561-2019",null,100," "," 消防器材——消火栓箱"]
["轻工及机械检测中心",4,"箱体刚度"," ","GB/T 14561-2019",null,440," "," 消防器材——消火栓箱"]
["轻工及机械检测中心",5,"箱门"," ","GB/T 14561-2019",null,440," "," 消防器材——消火栓箱"]
["轻工及机械检测中心",6,"消防水带安置"," ","GB/T 14561-2019",null,110," "," 消防器材——消火栓箱"]
["轻工及机械检测中心",1,"外观",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,50]
["轻工及机械检测中心",2,"尺寸与偏差",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,100]
["轻工及机械检测中心",3,"方正度",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,50]
["轻工及机械检测中心",4,"箱角漏洞",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,50]
["轻工及机械检测中心",5,"钉接/粘结",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,50]
["轻工及机械检测中心",6,"摇盖耐折",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,50]
["轻工及机械检测中心",7,"耐破强度",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,300]
["轻工及机械检测中心",8,"边压强度",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,300]
["轻工及机械检测中心",9,"粘合强度",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,300]
["轻工及机械检测中心",10,"厚度",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,100]
["轻工及机械检测中心",11,"印刷质量",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,100]
["轻工及机械检测中心",12,"印刷质量",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,50]
["轻工及机械检测中心",13,"空箱抗压强度",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,300]
["轻工及机械检测中心",14,"含水率",null,"GB/T 6543-2025 运输包装用单瓦楞纸箱和双瓦楞纸箱",null,150]